### Information to Gather: Frame Relay Configuration

For frame relay configurations, gather and record the following information from your network service provider or your system administrator:

- LMI protocol and maximum frame size used by the network
- DLCI and CIR for each virtual circuit
- Higher-layer protocols to run over each virtual circuit
- Higher-layer addresses associated with each virtual circuit
- Encapsulation method (as defined in RFC 1490) that should be used to communicate with remote devices
- Line speed and clock source