### Configuring a Device for a Terminal with scoadmin

Use this procedure to configure a RealPort device for a terminal in SCO UnixWare. See your operating system documentation for more information on configuring a serial device for a terminal.

The Digi device and RealPort should be properly installed, configured and functioning before proceeding.

#### Procedure

1. Connect a proper cable between the port and terminal.
2. Enable and configure the port using one of the these three methods:

   Method | Description
   Using pmadm | This method can be used in any SVR4-based Unix system. Though effective, it is often tedious to use because the command used is complicated. See Configuring a Device with pmadm.
   Using the Serial Manager in SCO UnixWare | This method works only in SCO UnixWare. See General SCO UnixWare Device Configuration.
   Using sysadm | This procedure works only in SVR4 systems that have access to a utility called sysadm. See General SVR4 Device Configuration.