### Managing a Digi Device with Digi RealPort Manager

#### Introduction

Digi RealPort Manager can be used to perform these tasks. Select a link to navigate to the corresponding procedure.

Task | Procedure
Add a Digi Device | See Adding a Digi Device.
Delete a Digi Device | See Deleting a Digi Device.
Configure an existing Digi One RealPort or PortServer | See Configuring an Existing Digi One RealPort or PortServer.
Start a RealPort daemon | See Starting a RealPort Driver.
Stop a RealPort daemon | See Stopping a RealPort Driver.
Monitor port status | See Monitoring Port Status.

#### The Main Screen

The main screen of the Digi RealPort Manager is used to manage the Digi devices registered with the RealPort driver. It lists all of the currently configured Digi devices in the central window, and provides buttons and menu options to manipulate these Digi Devices.

Menu Field | Description
RealPort ID | The RealPort ID must be one or two alphanumeric characters used to designate your TTY devices for RealPort. This id must be unique to your system. An underscore character may also be used for an ID character. An example for a RealPort device name where the letters rp are used would be: TTYrp01
address | The address may be specified as an IP number, or IP name. No attempt is made to validate this address, nor to connect to the specified address during the installation.
ports | This field is an integer indicating the number of device files which should be created for this Digi Device. This does not have to match the physical number of ports, but physical ports beyond the number specified will not be available. The maximum port count allowed is 64.
IP Port | This is the Digi Device IP port number. Normally this should be left at the default.
Access Mode | Access Mode sets the file protection mode for any device files created.
Owner | This field sets the user ID of the file owner for any device files created. The value must be an integer.
Group | This field sets the group ID of the file owner for any device files created. The value must be an integer.
Link Speed | Link Speed sets the link speed string. The default is auto, and can be used under most circumstances. See the drpd(8) man page for information on the custom speed parameters.