### Setup Examples for Transparent Printing

Use the ditty program to set up your terminal for transparent printing.

Note: The device /dev/dty/a001s is used an example in the following ditty commands. Substitute your Digi product's specific device path and device name when using ditty.

#### Example 1:

The following command configures the transparent print options for a DEC VT100 terminal connected to /dev/cua/a001 (note that the printer will be called /dev/dpr/a001s). maxcps, maxchar and bufsize are left to defaults. Enter:

`ditty term vt100 /dev/dty/a001s`

#### Example 2:

The following example uses onstr and offstr arguments (this sets the terminal to use ANSI Standard). Again maxcps, maxchar, and bufsize are defaults. Enter (on a single command line):

`ditty onstr \033[5i offstr \033[4i /dev/dty/a001s`

#### Example 3:

This example command sets the transparent print option for a WYSE30 terminal, with maxcps of 75, a maxchar of 100, and a printer buffer size, bufsize, of 1000. Enter (on a single command line):

`ditty term wyse30 maxcps 75 maxchar 100 bufsize 1000 /dev/dty/a001s`