### Channelized T1, Short Haul (PBX or other Internal Network) Configuration Worksheet

Use the worksheet below to collect information that may be required to configure your DataFire PTE adapter in your operating system environment. Note that not all operating systems support all parameters.

The parameters on this page are for channelized T1 connected to a PBX or similar in-house network (Short Haul). If your adapter is connected directly to an external T1 telephone line, use the Channelized T1, Long Haul (External T1) worksheet.

Parameter | Value
--- | ---
Coding | [ ] B8ZS [ ] AMI
Framing | [ ] ESF [ ] D4
Short Haul Length (in feet) | [ ] 0-133 [ ] 133-266 [ ] 266-399 [ ] 399-533 [ ] 533-655
Signaling | [ ] Ground Start [ ] Loop Start [ ] Immediate Start [ ] Wink Start -- Wink Digits (1-20): ________
Modem Nationality | Enter the country in which the PTE adapter will be installed: