### Installing the Driver: Downloaded

Use this topic to install the downloaded Digi ClassicBoard Linux driver.

#### Procedure

Note: Enter the commands in this procedure at a root prompt.

1. Change directories to the same directory as the downloaded driver file.

2. Enter this command:

   `rpm --rebuild driver.src.rpm`

3. Change your working directory to `/usr/src/redhat/RPMS/i386`:

   `cd /usr/src/redhat/RPMS/i386`

4. Enter this command:

   `rpm -ivv cpci-driver.i386.rpm`

5. Change your working directory to `/etc/digicpci`:

   `cd /etc/digicpci`

6. Enter this command:

   `./rc.cpci load`