### Master Setup Process: IP over Frame Relay

Use this process to configure a SYNC 2000 line for IP traffic over a frame relay link.

#### Procedure

1. Gather information for configuration. See Information to Gather: Frame Relay Configuration.

2. Ensure that the SCO patches have been installed. See Required SCO Patches.

3. Understand key concepts. These include the following:

   - PVCs and IP Addresses. See About PVCs and IP Addresses.

   - RFC 1490 Encapsulation. See About RFC 1490 Encapsulation.

4. Install the Digi adapter. See the hardware installation card.

5. Install the Digi driver. See Installing the Driver: CD.

6. Add a WAN device. See Adding a WAN Device

7. Configure general frame relay parameters. See Configuring a Line: General Frame Relay.

8. Configure IP-specific parameters. See Configuring a Frame Relay Connection: IP.