### Master Setup Process

These are the steps necessary for the installation and configuration of an EtherLite module.

1. Attach the EtherLite module to the network using only a 10Base-T cable. Do not plug in the power cable at this time.
2. Assign the EtherLite module an IP address. See Assigning an IP Address: Store IP, Assigning a Temporary IP Address: Boot Console, and Assigning a Permanent IP Address: Boot Console.
3. Install the driver. See Installing the Driver: Downloaded.
4. Follow the prompts to configure the driver.