### Master Setup Process

Here are the steps required to setup the SYNC/570 on Novell NetWare systems.

1. Prepare for your installation by gathering configuration information:

   - Information to Gather: Frame Relay

   - Information to Gather: X.25

2. Install the adapter. See the hardware installation card.

3. Install the driver. See Installing the Driver.

4. Configure the adapter. See Configuring the Adapter.

5. Configure the line. See one of the following:

   - Configuring a Line: Frame Relay

   - Configuring a Line: X.25

   - Configuring a Line: PPP WAN Calls

6. Configure virtual circuits. See one of the following:

   - Configuring Frame Relay PVCs

   - Configuring X.25 Virtual Circuits

7. Configure protocols and bindings. See the Novell NetWare documentation for more information.