### Installing the Driver: Server Console

Use this procedure to install driver files from the server console.

#### Prerequisites

Install the driver files for your Digi adapter directly from the CD. You need to know whether you have a DOS-mounted or a Novell NetWare-mounted CD-ROM drive. If it is DOS-mounted, the CD-ROM drive is accessible to DOS applications and Novell NetWare applications without mounting.

If your CD-ROM drive is Novell NetWare-mounted, you must be sure that all of the Novell NetWare CD-ROM device drivers are loaded, insert the CD, and enter the following command to mount it before you begin your installation:

cd mount digi_cd

#### Procedure

1. At the system command prompt, type the following:

   load install

   A Novell NetWare menu will be displayed.

2. Choose Product Options, and then choose Install a Product Not Listed from the next menu that displays.
3. Choose a source directory from which the drivers will be copied.

   Press ENTER if you are installing from a diskette.

   If installing from CD, press F3, then specify the path to the CD-ROM drive, as shown below:

   Dos Mounted | Novell NetWare-Mounted
   Drive:\Novell\directory | digi_cd:\drivers\netware\directory

   where Drive is the drive letter of the CD device under DOS, and directory is the directory containing the driver files for your Digi adapter (see table):

   Directory | Product Family
   RAS | DataFire Product Family
   RAS | AccelePort RAS Family
   Xr | AccelePort Xr Family
   Xe | AccelePort Xe Family
   Xem | AccelePort Xem System
   CXP | AccelePort PCI C/X System
   CX | AccelePort ISA C/X System
   EPC | AccelePort EPC/X System

4. Choose Install Product from the menu.
5. At the prompt, choose the server on which you want driver files installed.
6. At the Start installation? prompt, choose Yes.
7. When the installation is complete, exit the installation and then bring down and restart the server.