### Configuring a Line for X.25

Use this procedure to configure a line for X.25.

#### Prerequisites

This topic assumes that the driver has been installed and the configuration Wizard displayed.

Note: For information on configuration fields, access the online help by choosing Help.

#### Procedure

1. To access the Digi Configuration Wizard, do the following:
   1. Choose Control Panel > Network > Adapters.
   2. Select the adapter from the Network Adapters list and then choose Properties. The Digi configuration utility appears.
2. Use the Wizard to guide you through the setup process, which will produce a configuration that works for most sites.
3. If you specified switched virtual circuits, specify how you want SYNC 2000 to route outbound calls.
   1. Select the X.25 Routing label and choose Properties.
   2. See the online help for information on configuring outbound routes.