### Device Names

Use the information on this page to determine the names of the devices created for each Digi adapter supported by the Solaris driver.

#### Device Name Format

The devices for the DataFire RAS PTE, AccelePort RAS and AccelePort Xp products are located in /dev/DIGIras after the driver installation. They are named according to the following conventions:

`/dev/bMMpNNm and /dev/bMMpNNs`

where:

b | Is constant
MM | Is a number designating the adapter board. It is a two-digit base-10 number assigned by the operating system when the driver is installed.
p | Is constant
NN | Is a number designating the port number. It is a two-digit base-10 number assigned by the operating system when the driver is installed.
m,s | m specifies a modem-control (dial-out) device. s specifies a non-modem-control (dial-in) device.

#### Example:

The modem-control device for the fourth port of an adapter with a designation number of 00 would be b00p04m.