### Configuring a Device for a Terminal

Use this procedure to configure a Digi device for a terminal. Consult your Solaris documentation for more information on configuring a serial device for a terminal.

#### Procedure

1. Connect a proper cable between the port and terminal. See the Cable Guide.
2. Invoke admintool either through the window interface, or by entering this command at a root prompt:

   `admintool`

   Note: An alternative to admintool is the pmadm command. See Configuring Ports with pmadm.

3. Choose Browse > Serial Ports.
4. Choose a device.
5. Choose Edit > Modify.
6. Configure the device parameters. Typically a terminal device is set to Terminal-Hardwired and Service Enabled.
7. Set the Baud Rate.

   Note that the default admintool baud rates cycle, meaning the speed at the end of the corresponding /etc/ttydefs entry, is different than the speed at the beginning of the entry. It preferable to configure a device to a fixed rate.

   As an example, this line can be added to /etc/ttydefs and used as a fixed rate for devices:

   `38400N:38400 hupcl:38400 hupcl::38400N`

   If a custom /etc/ttydefs entry is created and used, set Baud Rate to Other and enter the /etc/ttydefs identifier (e.g. 38400N).

#### Troubleshooting Tips

- If a login does not appear on the terminal, try disabling and reenabling the device in admintool.
- If a cycling baud rate is used and scrambled characters appear on the terminal screen, hitting the Enter key several times at the terminal may cause the port to change baud rates and display a login.
- If a cycling baud rate is used and scrambled characters appear on the terminal screen, change the baud rate to a fixed /etc/ttydef entry matching the terminal's settings.