### C/CON-16 Rack Concentrator Specifications

Power Requirements
Voltage | 100 - 250 Volts AC
Frequency | 60 - 50 Hz
Current | 0.5 - 1.0 Amps
Environmental
Ambient temperature | 0 to 50 degrees C
Relative humidity | 20% to 80%
Serial Interface Surge Suppression
Threshold voltage: |
(EIA-232) | 13 volts
(EIA-422) | 13 volts (input signals)
5 volts (output signals)
Response time | < 10 nS
Mechanical
Length | 17.5 inches
Width | 11.5 inches
Height | 1.75 inches
Weight | 7 pounds