### Master Setup Process

Use this process to set up and install the Novell NetWare AIO driver for the AccelePort Xp family.

#### Overview of Setup Steps

1. Install the driver. See one of the following: Installing Driver Files: Server Console or Installing Driver Files: Windows Client.
2. Create a driver load command line for AUTOEXEC.NCF. See Configuring and Loading Drivers.
3. Create a Communication Agent load command line for AUTOEXEC.NCF. See Loading the Communication Agent. This enables PortAssist Manager to interact with the adapter.