### Loading the Driver

Use this procedure to load the configured AIO driver.

#### Procedure

At the server console, enter the following command:

load aiopsdrv

When the driver is successfully loaded, a message similar to the following will appear:

`NetWare AIO Digi PortServer
Version 1.02 June 19, 1997
Waiting for Connection to Complete
Connected to chris: Digi PortServer2 HREV 0.f SREV 3.0 Ports = 16
Digi AIO driver initialized successfully`

The driver is now ready for use.