### Running PortServer TS 8/16 Hardware Diagnostics

Use this topic to run hardware diagnostic procedures on the PortServer TS 8/16.

#### Procedure

1. Connect a terminal to port 1.
2. If the port is still using the default configuration, configure the terminal to use the following settings (Otherwise, configure the terminal to match the port configuration):

- VT-100 emulation
- 9600 baud
- 8-bit characters
- 1 stop bit
- No parity

3. Boot the PortServer TS 8/16.
4. When the LEDs begin to blink, press x

The Diagnostic Menu appears.

5. Choose a test and press Enter.