### DataFire SYNC 2000 cPCI Specifications

Power Requirements: | + 5 Volts ± 5%, .2 amps maximum
+ 3 Volts ± 5%, 1.9 amps maximum
+ 12 Volts ± 5%, .02 amps maximum
Temperature: | 10º to 55º C (50º to 131ºF)
Relative Humidity: | 5% to 90%, non-condensing
Air Movement: | 30 CFM Forced
Altitude: | 0 to 3658 meters (12000 ft.)
Length: | 160 mm (6.3 in.)
Width: | 13 mm (.5 in.)
Height: | 6U form factor: 233 mm (9.2 in.)
Weight: | 284 gm. (10 oz.)