### Enabling Devices for Dial-in

This topic describes how to enable ports for dial-in access.

#### Procedure

1. Enter `scoadmin modem`.
2. Select Modem > Add > Manual Configuration.
3. Select Digi from the left-hand column and Digi RAS modem 56000 from the right-hand column.
4. Select a port from the Modem port field and then press Configure port....
5. Specify the type of call the modem will handle (inbound, outbound, or both) and specify a speed of 9600.
6. Select OK > OK.

   The Digi RAS modem 56000 appears in the list.

7. Exit the Modem Manager by selecting Host > Exit.
8. If you want to use this port for PPP traffic, this procedure is complete.
9. If you want to enable the port for non-PPP traffic, do the following:
   1. Enter the following

      `/usr/local/bin/fixmon`

   2. Look in the Flags field for a capital P, which indicates the port is expecting PPP traffic.
   3. If the port is set for PPP traffic, enter the port number at the prompt.