### Xe Error Messages and Solutions

#### Load Command Errors

The following error messages may occur while the driver is parsing the parameters.

`*Usage Error: AIODGXI port=XXXX mem=XXXXX [name=bname].`

> This error will appear if you load the driver with no parameters on ISA bus computers.

`*Usage Error: First parameter not 'port='.`

> The driver expects the first parameter to be port=xxx, but this is not the case.

`*Error: Invalid Port Address 0x310.`

> This message indicates that an invalid port address was specified.

`*Error: Port Address 0x320 is already supported.`

> This message indicates that the driver is already supporting an adapter at this port address.

`*Usage Error: Second parameter not 'mem='`

> The driver expects the second parameter to be mem=xxxxx, but this is not the case.

`*Error: Invalid Memory Address 0xF0000.`

> This message indicates that an invalid memory address was specified.

#### Adapter Errors

The following error messages may occur while the driver is performing some initial tests on the adapter.

`Adapter 4: Port 220 Mem D0000 Port 220 not found.`

> This message indicates that the driver could not find an adapter with port 220h. Check to insure that you have specified the correct I/O port or that you have properly configured the adapter's port address.

`Adapter 4: Port 220 Mem D0000 Hardware Reset Fails.`

> This message indicates that the driver could not place the adapter into a reset state. This is most likely the result of an I/O port ad-dress conflict or a faulty adapter. Be sure that there are no other I/O ports in your system at the indicated I/O port address.

`Adapter 4: Port 220 Mem D0000 Memory not found error x.`

> This message indicates that the driver could not find the adapter's memory. x indicates the number of memory errors found in a 256 byte block.

`Adapter 4: Port 220 Mem D0000 Memory error x.`

> This message indicates that the driver has found the adapter's memory, but it appears to be faulty. x indicates the number of errors found in a 256 byte block.

#### Initialization Errors

The following messages may occur during the driver's attempt to initialize the adapter.

`Adapter 4: Port 220 Mem D0000 BIOS fails initialization.`

> This message indicates that the adapter's on-board BIOS did not initialize properly.

`Adapter 4: Port 220 Mem D0000 BIOS passes init but reports 0 ports.`

> This message indicates that the BIOS initialized successfully, but could not find any of the asynchronous channels.

`Adapter 4: Port 220 Mem D0000 NMI Fails during FEPOS code move.`

> This message indicates a failure during transfer of the on-board operating system code.

`Adapter 4: Port 220 Mem D0000 NMI Fails during FEPOS execution.`

> This message indicates a failure during startup of the on-board operating system.

`Adapter 4: Port 220 Mem D0000 FEPOS Fails Initialization.`

> This message indicates that the on-board operating system did not initialize successfully.

`Adapter 4: Port 220 Mem D0000 Command failure during Initialization.`

> This message indicates that the on-board operating system encountered a failure during initialization of the asynchronous channels.