### Specifications: DataFire DSP PTE Series

Power Requirements, One-Port Models | + 5 Volts ± 5%, 2.33 - 2.44 A typical
Power Requirements, Two-Port Models | + 5 Volts ± 5%, 3.87 - 4.87 A typical
Temperature | 10º to 50º C (50º to 122ºF)
Relative Humidity | 5% to 90%, non-condensing
Air Movement | 30 CFM Forced
Altitude | 0 to 3658 meters (12000 ft.)
Length | 6.30 inches
Width | 9.19 inches
Height | .57 inches (component side) .60 inches (back side)
Weight | .7 pounds (one-port models) 1.0 pound (two-port models)