### Configuring Frame Relay PVCs

Use this procedure to configure PVCs on a SYNC/570 line.

#### Procedure

1. From the Internetworking Configuration menu, choose WAN Call Directory.

   The Configured WAN Call Destination screen appears.

2. Press the INSERT key.

3. Configure the PVC by doing the following:

   1. Supply a name for the destination

   2. Choose frame relay as the Supported Wide Area Medium

   3. Choose an interface

   4. Specify the DLCI provided by your network supplier for this destination.