### Configuring a Device with pmadm

Use this procedure to configure a RealPort device with pmadm. This procedure can be used from a command line prompt in the absence of a window interface to the operating system. For additional information and help on pmadm, consult your SCO UnixWare or SVR4 documentation.

The Digi device and RealPort should be properly installed, configured and functioning before proceeding.

#### Procedure

1. Enter a pmadm command at a root prompt. Here is an example of a command that will enable a port for 9600 8,1,N. Modify the command as necessary for your terminal.

   `pmadm -a -p digimon -s a001s -fu -i root -v `ttyadm -V`
   -m "`ttyadm -d /dev/term/a01s -l 9600 -s /usr/bin/login`"`

   where:

   digimon | is the port monitor tag. Use a different one if appropriate.
   a01s | is the name of the device.
   -l 9600 | sets the port for a baud rate of 9600.

2. Verify that the port is enabled with this command:

   `pmadm -l`