### AccelePort 2p PCI Adapter Specifications

Power Requirements
+5 volts +/- 5% | 430 mA typical
+12 volts +/- 5% | 100 mA typical
-12 volts +/- 5% | 100 mA typical
Environmental
Ambient temperature | 10 to 55 degrees C (50 to 131 degrees F)
Relative humidity | 5% to 90%
Air Movement | 30 CFM forced
Altitude | 0 to 2438 meters (0 to 8,000 feet)
Serial Interface Surge Suppression
Threshold voltage: | Inputs= +/- 30 volts
Outputs= +/- 15 volts
Response time | < 10 nS
Mechanical
Length | 11.239 centimeters (4.425 inches)
Width | 1.625 centimeters (.64 inches)
Height | 8.801 centimeters (3.465 inches)
Weight | 0.18660 kilograms (6.0 ounces)