### Tips for Configuring SNA over Frame Relay PVCs

Here are some tips for configuring SNA over Frame Relay PVCs:

- Ensure that the Network Address on this side of a virtual circuit is not the same as the Network Address on the other side.

- Configure Bridged or Bridged with fcs as the encapsulation method. The encapsulation method used on this side of the PVC must be identical to one used on the other side.