### Installing a Driver

Use these procedures to install a RealPort driver on a Microsoft Windows 2000 system.

1. From the Start menu, choose Settings > Control Panel > Add/Remove Hardware > Next.
2. Choose Add/Troubleshoot a device > Next.
   The system searches for the device. When it determines that it cannot find the device, it displays a list of devices.
3. Choose Add a new device > Next.
4. Choose No, I want to select the hardware from a list > Next.
5. Choose Multi-port serial adapters > Next.
6. Select Have Disk.
7. Select Browse, point the system to the appropriate driver location and follow the installation and configuration procedure.
8. Select the RealPort driver and Next > Next.
9. If the Digital Signatures Not Found screen appears, choose Yes.
10. f you are using an Etherlite unit that has not been assigned an IP address, do the following to assign an address:

1. Press the DgIPServ button.
2. Use the wizard and the associated help text to assign an IP address to the Etherlite unit.
3. When you finish, return to the Add Digi RealPort wizard.

11. Use the Add Digi RealPort wizard and the associated help text to configure the RealPort driver with the IP address and TCP port number used by the Digi One RealPort, PortServer, or Etherlite.
12. Follow the prompts to complete configuration of the RealPort driver.