### Configuring the Driver

Use the the following procedure to access the ClassicBoard Setup window if it is not already displayed.

#### Procedure

1. From the Control Panel, choose Network > Adapters.
2. Choose the ClassicBoard Adapter.
3. Choose Properties.

#### Configuration Options

Three configuration options are available on the ClassicBoard Setup window. They are:

- FIFO
- Baud Mapping
- Ports

The FIFO and Baud Mapping options are advanced features that you usually do not need to change. Choose Help for each option for more information.