### Configuring the EtherLite for RealPort

Use this process to install and configure the EtherLite Terminal Server on the RealPort.

1. Attach the EtherLite module to the network using an appropriate cable. Do not plug in the power cable at this time.
2. Assign an IP address to the EtherLite module. Use one of the following methods:

> - Assigning an IP Address: dgipserv
> - Assigning an IP Address (Temporary): Boot Console
> - Assigning an IP Address (Permanent): Boot Console.