### Uninstalling the Driver

Use this procedure to remove the AccelePort RAS driver.

#### Procedure

1. Enter this command at a root prompt:

   `swremove`

   The SD - Remove Software Selection window appears.

2. Choose DGDXB.

3. Choose Actions > Mark for Remove

4. Choose Actions > Remove (Analysis)...

5. Choose OK to continue at the Remove Analysis window.

6. Choose Yes at the Confirmation windows that appear.

7. Choose Done at the Remove window.

8. Confirm the prompt to reboot the system when it appears. If it does not appear, the system should be rebooted manually.