### Basic Rate ISDN (BRI) Configuration Worksheet

Use the form below to gather information that may be required to configure your DataFire RAS B4STU adapter in your operating system environment. Note that not all operating systems support all parameters.

With the exception of Modem Nationality, all parameters should be obtained from your network service provider.

Parameter | Value
--- | ---
Switch Type | [ ] 5ESS [ ] DMS100 [ ] INS-64 (Japan) [ ] NI1 [ ] Euro ISDN DSS1
Telephone Number | List the telephone number of each logical terminal:
SPID or Subaddress | For switch types 5ESS, DMS100, NI1 and None, list the SPID (Service Profile Identifier) for each logical terminal. For switch types ETSI (Euro ISDN) and INS-64, list the Subaddress of each logical terminal:
Modem Nationality | Enter the country in which the RAS B4STU adapter will be installed:
MSN (Multiple Subscriber Numbers) | Available only for ETSI (Euro ISDN) switch type, in Linux installations. [ ] Disabled [ ] 1-8 (specify):