### SCSI Terminal Server Specifications

WARNING: To prevent electric shock, do not remove the cover of a SCSI Terminal Server module. There are no user-serviceable parts inside. Refer servicing to qualified personnel.

AC Power Requirements (maximum)
Models 1002, 1008, 1400, 1800, 1610, 1616 | Two external power supplies available: 120 VAC, 60 Hz, 15VA (U.S., Canada) 100-240 VAC, 50-60 Hz, 15VA (universal)
Model 1032 | 100-240 VAC, 50-60 Hz, 25VA internal power supply
The recommended power cord for North American units is: UL Listed, CN, detachable type SJT or SVT, 3 conductor, 18 AWG, rated 125 V, 10 A.
Environmental
Ambient temperature: Models 1002, 1008, 1400, 1800, 1610, 1616 | 50°F (10°C) to 122°F (50°C)
Ambient temperature: Model 1032 | 50°F (10°C) to 95°F (35°C)
Relative humidity | 5% to 90% non-condensing
Altitude | 0 to 12,000 feet (0 to 3650 meters)
Serial Interface Surge Suppression
15 kilovolts per IEC 1000-4-2, Level 4
Mechanical
Models 1002, 1008 | Height: 1.2 inches (3.1 cm) Width: 8.1 inches (20.6 cm) Depth: 5.9 inches (14.8 cm) Weight: 1.2 lbs. (0.6 kg)
Models 1400, 1800 | Height: 1.1 inches (2.8 cm) Width: 8.1 inches (20.6 cm) Depth: 5.5 inches (14.1 cm) Weight: 1.0 lbs. (0.5 kg)
Model 1610 | Height: 1.2 inches (3.1 cm) Width: 11.5 inches (29.3 cm) Depth: 5.4 inches (13.8 cm) Weight: ?.? lbs. (?.? kg)
Model 1616 | Height: 1.2 inches (3.1 cm) Width: 8.1 inches (20.6 cm) Depth: 5.5 inches (14.1 cm) Weight: 2.1 lbs. (1.0 kg)
Model 1032 | Height: 1.8 inches (4.5 cm) Width: 15.1 inches (38.4 cm) Depth: 7.6 inches (19.2 cm) Weight: 3.3 lbs. (1.5 kg)