### Device Names

Use the information on this page to determine which device to use for a particular Digi port.

During the driver installation, Digi devices are created in the /dev directory. The table below shows the device naming conventions.

Format | Device Information
ttyNyyz | ttyN is constant. yy is the unit number, starting with zero. z is the port number. Use 0-9 for ports 1-10; use a-v for ports 11-32. Example: ttyN003 is the fourth port on the first EtherLite unit.