# AP-2000 Help Contents |
[ Home ] [Proxim website]

## ASCII Character Chart You can configure WEP Encryption Keys in either Hexadecimal or ASCII format. Hexadecimal digits are 0-9 and A-F (not case sensitive). ASCII characters are 0-9, A-F, a-f (case sensitive), and punctuation marks. Each ASCII character corresponds to two hexadecimal digits. The table below lists the ASCII characters that you can use to configure WEP Encryption Keys. It also lists the Hexadecimal equivalent for each ASCII character.
ASCII Character | Hex Equivalent |  | ASCII Character | Hex Equivalent |  | ASCII Character | Hex Equivalent |  | ASCII Character | Hex Equivalent
--- | --- | --- | --- | --- | --- | --- | --- | --- | --- | ---
! | 21 |  | 9 | 39 |  | Q | 51 |  | i | 69
" | 22 |  | : | 3A |  | R | 52 |  | j | 6A
# | 23 |  | ; | 3B |  | S | 53 |  | k | 6B
$ | 24 |  | < | 3C |  | T | 54 |  | l | 6C
% | 25 |  | = | 3D |  | U | 55 |  | m | 6D
& | 26 |  | > | 3E |  | V | 56 |  | n | 6E
' | 27 |  | ? | 3F |  | W | 57 |  | o | 6F
( | 28 |  | @ | 40 |  | X | 58 |  | p | 70
) | 29 |  | A | 41 |  | Y | 59 |  | q | 71
* | 2A |  | B | 42 |  | Z | 5A |  | r | 72
+ | 2B |  | C | 43 |  | [ | 5B |  | s | 73
, | 2C |  | D | 44 |  | \ | 5C |  | t | 74
- | 2D |  | E | 45 |  | ] | 5D |  | u | 75
. | 2E |  | F | 46 |  | ^ | 5E |  | v | 76
/ | 2F |  | G | 47 |  | _ | 5F |  | w | 77
0 | 30 |  | H | 48 |  | ` | 60 |  | x | 78
1 | 31 |  | I | 49 |  | a | 61 |  | y | 79
2 | 32 |  | J | 4A |  | b | 62 |  | z | 7A
3 | 33 |  | K | 4B |  | c | 63 |  | { | 7B
4 | 34 |  | L | 4C |  | d | 64 |  | | | 7C
5 | 35 |  | M | 4D |  | e | 65 |  | } | 7D
6 | 36 |  | N | 4E |  | f | 66 |  | ~ | 7E
7 | 37 |  | O | 4F |  | g | 67 |  |  |
8 | 38 |  | P | 50 |  | h | 68 |  |  |