PowerStorm 3D30/PowerStorm 4D20 V4.8 Readme.1st
===========================================================

This kit contains a driver which supports the PowerStorm 3D30 and
PowerStorm 4D20 graphics cards. The driver is for Windows NT V4.0 and Service 
Pak 3.

This driver does not support multiheaded systems and will not work on
Windows NT V3.51 or earlier versions.

NOTE: The jumper labeled ALIAS on the PowerStorm 3D30 and PowerStorm 4D20
cards must be jumpered when running Windows NT V4.0. 

See the release notes in the file relnotes.doc for for additional
information concerning this driver. This document can be read with the WordPad 
application. This can be invoked by selecting Start the the icon bar, then Programs, 
Accessories and then WordPad.


The driver can be installed either directly from the product CD or from the files
copied down from the website(see relnotes.doc) and unzipped and placed on a hard
disk:

To install the new driver, please follow these steps:

1)  Start the Control Panel Display applet.

2)  Click on the "Settings" tab.

3)  Click on the "Display Type..." button.

6)  In the Display Type dialog box, click on the "Change..." 
    button.

7)  In the Change Display dialog box, click on the "Have Disk..." 
    button and either insert the CD-ROM containing the drivers and
    specify the drive and path for the CD-ROM or specify the
    hard disk path if the drivers have been copied to your system.
    
    For the PowerStorm 3D30/4D20 drivers from CD-ROM the
    path is:

	dev:\alpha\tga\nt40_533a2

    After the path has been specified, choose OK.

8)  In the Change Display dialog box, the driver whose path you just defined
    is displayed. Confirm this choice by choosing OK.

    The driver name displayed is:

    COMPAQ PowerStorm 3D30/PowerStorm 4D20

11) You will see an informational message in the Third-party Drivers dialog.
    Click on the "Yes" button.

12) The files are now copied onto the system.

13) You will see an informational message in the Installing Drivers dialog.
    Click on the "OK" button.

13) Click on the "Close" button in the Display Type dialog.

14) Click on the "Close" button in the Display Properties dialog.

15) You must restart the computer before the new driver will take effect. Check
    the PowerStorm 3D30 and PowerStorm 4D20 jumper as noted above when the 
    computer is shut down.
