\input texinfo @c -*-texinfo-*-
@c %**start of header
@setfilename mtools.info
@settitle Mtools
@c UPDATE THIS DATE WHENEVER YOU MAKE CHANGES!
@c For double-sided printing, uncomment:
@c @setchapternewpage odd
@setchapternewpage off
@c %**end of header

@ignore
@unnumbered Name
mtools - utilities to access DOS disks in Unix.
@end ignore

@c MANskip

@set EDITION 3.9
@set VERSION 3.9
@set UPDATED March 1998

@iftex
@finalout
@end iftex

@ifinfo
@format
START-INFO-DIR-ENTRY
* Mtools: (mtools).        Mtools: utilities to access DOS disks in Unix.
END-INFO-DIR-ENTRY
@end format
@end ifinfo


@ifinfo
Mtools
Copyright (C) 1992-1998 Free Software Foundation, Inc.

Permission is granted to make and distribute verbatim copies of
this manual provided the copyright notice and this permission notice
are preserved on all copies.

@ignore
Permission is granted to process this file through TeX and print the
results, provided the printed document carries copying permission
notice identical to this one except for the removal of this paragraph
(this paragraph not being relevant to the printed manual).
@end ignore

Permission is granted to copy and distribute modified versions of this
manual under the conditions for verbatim copying, provided that the
entire resulting derived work is distributed under the terms of a
permission notice identical to this one, and provided that the privacy
of any reader of the resulting derived work is respected. In particular
is it strictly forbidden to make this documentation available on a World
Wide Web server which deals cookies. However, keeping access statistics
is allowed.

Permission is granted to copy and distribute translations of this manual
into another language, under the above conditions for modified versions,
except that this permission notice may be stated in a translation approved
by the Free Software Foundation.
@end ifinfo

@titlepage
@title Mtools
@subtitle Accessing MS-DOS disks
@subtitle Edition @value{EDITION}, for Mtools version @value{VERSION}
@subtitle @value{UPDATED}
@author by Alain Knaff
@page

@vskip 0pt plus 1filll
Copyright @copyright{} 1992, 1993, 1994, 1995, 1996 Free Software Foundation, Inc.

Permission is granted to make and distribute verbatim copies of
this manual provided the copyright notice and this permission notice
are preserved on all copies.

Permission is granted to copy and distribute modified versions of this
manual under the conditions for verbatim copying, provided that the
entire resulting derived work is distributed under the terms of a
permission notice identical to this one and provided that the privacy of
any reader of the resulting derived work is respected. In particular is
it strictly forbidden to make this documentation available on a World
Wide Web server which deals cookies. However, keeping access statistics
is allowed.

Permission is granted to copy and distribute translations of this manual
into another language, under the above conditions for modified versions,
except that this permission notice may be stated in a translation approved
by the Free Software Foundation.

@end titlepage

@ifinfo
@node Top, Location, (dir), (dir)

@end ifinfo

@c MANend-skip

@unnumbered Introduction
Mtools is a public domain collection of tools to allow Unix systems to
manipulate MS-DOS files: read, write, and move around files on an MS-DOS
filesystem (typically a floppy disk).  Where reasonable, each program
attempts to emulate the MS-DOS equivalent command. However, unnecessary
restrictions and oddities of DOS are not emulated. For instance, it is
possible to move subdirectories from one subdirectory to another.

Mtools is sufficient to give access to MS-DOS filesystems.  For
instance, commands such as @code{mdir a:} work on the @code{a:} floppy
without any preliminary mounting or initialization (assuming the default
@file{/etc/mtools.conf} works on your machine).  With mtools, one can
change floppies too without unmounting and mounting.


@menu
* Location::          Where to find mtools and early bug fixes
* Common features::   Common features of all mtools commands
* Configuration::     How to configure mtools for your environment
* Commands::          The available mtools commands
* Compiling mtools::  Architecture specific compilation flags
* Porting mtools::    Porting mtools to architectures which are not
                      yet supported

* Command Index::     Command Index
* Variable Index::    Variable Index
* Concept Index::     Concept Index
@end menu

@c MANskip

@unnumbered Warning, beware of the cookie monster!

If you are reading this documentation on the World Wide Web, this
section might interest you.  If you are reading it using info, or as a
printed document, or on one of our own sites (www.tux.org and
www.poboxes.com/Alain.Knaff) you do not need to worry.

It has come to my attention that some of the Web sites which display
this documentation deal so called "cookies".  These "cookies" are tags
sent from the server to the browser, which enable the server to keep
track of the sites that the user visits, and thus compromise his
privacy.  If you use netscape, you can enable confirmation messages for
any cookies sent to your browser by going into
Options->Network_Preferences->Protocols and checking the box for "Show
an Alert before Accepting a cookie". Then, when the alert box pops up,
click "Cancel" to refuse the cookie and protect your privacy.

@c MANend-skip

@node Location, Common features, Top, Top
@chapter Where to get mtools
@cindex bugs
@cindex ALPHA patches
@cindex patches
@cindex diffs
@cindex mailing list

Mtools can be found at the following places (and their mirrors):
@example
ftp://www.tux.org/pub/knaff/mtools/mtools-3.9.tar.gz
ftp://sunsite.unc.edu/pub/Linux/utils/disk-management/mtools-3.9.tar.gz
@end example

Before reporting a bug, make sure that it has not yet been fixed in the
Alpha patches which can be found at:
@example
http://www.poboxes.com/Alain.Knaff/mtools
ftp://www.tux.org/pub/knaff/mtools
@end example

Note: It is highly probable that the innet address will cease to exist after
November 1997.  The wauug address is permanent.

These patches are named
@code{mtools-}@var{version}@code{-}@var{ddmm}@code{.taz}, where version
stands for the base version, @var{dd} for the day and @var{mm} for the
month. Due to a lack of space, I usually leave only the most recent
patch.

There is an mtools mailing list at mtools @@ tux.org .  Please
send all bug reports to this list.  You may subscribe to the list by
sending a message with 'subscribe mtools @@ tux.org' in its
body to majordomo @@ tux.org . (N.B. Please remove the spaces
around the "@@" both times. I left them there in order to fool
spambots.)  Announcements of new mtools versions will also be sent to
the list, in addition to the linux announce newsgroups.  The mailing
list is archived at http://www.tux.org/hypermail/mtools/latest


@node Common features, Configuration, Location, Top
@chapter Common features of all mtools commands

@menu
* arguments::              What the command line parameters of mtools
                           mean
* drive letters::          Which drives are defined by default
* directory::              Current working directory
* long names::             VFAT-style long filenames
* name clashes::           Name clash handling, and associated command
                           line options
* case sensitivity::       Case sensitivity
* high capacity formats::  How to fit more data on your floppies
* exit codes::             Exit codes
* bugs::                   Happens to everybody
@end menu

@node arguments, drive letters, Common features, Common features
@section Options and filenames
@cindex Filenames
@cindex Options
MS-DOS filenames are composed of a drive letter followed by a colon, a
subdirectory, and a filename. Only the filename part is mandatory, the
drive letter and the subdirectory are optional. Filenames without a
drive letter refer to Unix files. Subdirectory names can use either the
'@code{/}' or '@code{\}' separator.  The use of the '@code{\}' separator
or wildcards requires the names to be enclosed in quotes to protect them
from the shell. However, wildcards in Unix filenames should not be
enclosed in quotes, because here we @strong{want} the shell to expand
them.

The regular expression "pattern matching" routines follow the Unix-style
rules.  For example, `@code{*}' matches all MS-DOS files in lieu of
`@code{*.*}'.  The archive, hidden, read-only and system attribute bits
are ignored during pattern matching.

All options use the @code{-} (minus) as their first character, not
@code{/} as you'd expect in MS-DOS.

Most mtools commands allow multiple filename parameters, which
doesn't follow MS-DOS conventions, but which is more user-friendly.

Most mtools commands allow options that instruct them how to handle file
name clashes. @xref{name clashes}, for more details on these. All
commands accept the @code{-V} flags which prints the version, and most
accept the @code{-v} flag, which switches on verbose mode. In verbose
mode, these commands print out the name of the MS-DOS files upon which
they act, unless stated otherwise. @xref{Commands}, for a description of
the options which are specific to each command.


@node drive letters, directory, arguments, Common features
@section Drive letters

The meaning of the drive letters depends on the target architectures.
However, on most target architectures, drive A is the first floppy
drive, drive B is the second floppy drive (if available), drive J is a
Jaz drive (if available), and drive Z is a Zip drive (if available).  On
those systems where the device name is derived from the SCSI id, the Jaz
drive is assumed to be at Scsi target 4, and the Zip at Scsi target 5
(factory default settings).  On Linux, both drives are assumed to be the
second drive on the Scsi bus (/dev/sdb). The default settings can be
changes using a configuration file (@xref{Configuration}).


@node directory, long names, drive letters, Common features
@section Current working directory
@pindex mcd (introduction)
@cindex Directory
@cindex Working directory
@cindex Current working directory
@cindex Default directory

The @code{mcd} command (@ref{mcd}) is used to establish the device and
the current working directory (relative to the MS-DOS filesystem),
otherwise the default is assumed to be @code{A:/}. However, unlike
MS-DOS, there is only one working directory for all drives, and not one
per drive.

@node long names, name clashes, directory, Common features
@section VFAT-style long file names
@cindex Long file name
@cindex Windows 95-style file names
@cindex VFAT-style file names
@cindex Primary file name (long names)
@cindex Secondary file name (long names)

This version of mtools supports VFAT style long filenames. If a Unix
filename is too long to fit in a short DOS name, it is stored as a
VFAT long name, and a companion short name is generated. This short
name is what you see when you examine the disk with a pre-7.0 version
of DOS.
 The following table shows some examples of short names:

@example
Long name       MS-DOS name      Reason for the change
---------       ----------      ---------------------
thisisatest     THISIS~1        filename too long
alain.knaff     ALAIN~1.KNA     extension too long
prn.txt         PRN~1.TXT       PRN is a device name
.abc            ABC~1           null filename
hot+cold        HOT_CO~1        illegal character
@end example

 As you see, the following transformations happen to derive a short
name:
@itemize @bullet
@item
Illegal characters are replaced by underscores. The illegal characters
are @code{;+=[]',\"*\\<>/?:|}.
@item
Extra dots, which cannot be interpreted as a main name/extension
separator are removed
@item
A @code{~}@var{n} number is generated,
@item
The name is shortened so as to fit in the 8+3 limitation
@end itemize

 The initial Unix-style file name (whether long or short) is also called
the @dfn{primary} name, and the derived short name is also called the
@dfn{secondary} name.

 Example:
@example
 mcopy /etc/motd a:Reallylongname
@end example
 Mtools creates a VFAT entry for Reallylongname, and uses REALLYLO as
a short name. Reallylongname is the primary name, and REALLYLO is the
secondary name.
@example
 mcopy /etc/motd a:motd
@end example
 Motd fits into the DOS filename limits. Mtools doesn't need to
derivate another name. Motd is the primary name, and there is no
secondary name.

 In a nutshell: The primary name is the long name, if one exists, or
the short name if there is no long name.

 Although VFAT is much more flexible than FAT, there are still names
that are not acceptable, even in VFAT. There are still some illegal
characters left (@code{\"*\\<>/?:|}), and device names are still
reserved.

@example
Unix name       Long name      Reason for the change
---------       ----------      ---------------------
prn             prn-1           PRN is a device name
ab:c            ab_c-1          illegal character
@end example

 As you see, the following transformations happen if a long name is
illegal:
@itemize @bullet
@item
Illegal characters are replaces by underscores,
@item
A @code{-}@var{n} number is generated,
@end itemize

@node name clashes, case sensitivity, long names, Common features
@section Name clashes
@cindex Name clashes
@cindex Duplicate file names
@cindex Overwriting files
@cindex Primary file name (name clashes)
@cindex Secondary file name (name clashes)

When writing a file to disk, its long name or short name may collide
with an already existing file or directory. This may happen for all
commands which create new directory entries, such as @code{mcopy},
@code{mmd}, @code{mren}, @code{mmove}, @code{mwrite} and
@code{mread}. When a name clash happens, mtools asks you what it should
do. It offers several choices:

@table @code
@item overwrite
Overwrites the existing file. It is not possible to overwrite a
directory with a file.
@item rename
Renames the newly created file. Mtools prompts for the new filename
@item autorename
Renames the newly created file. Mtools chooses a name by itself, without
prompting
@item skip
Gives up on this file, and moves on to the next (if any)
@end table

To chose one of these actions, type its first letter at the prompt. If
you use a lower case letter, the action only applies for this file only,
if you use an upper case letter, the action applies to all files, and
you won't be prompted again.

You may also chose actions (for all files) on the command line, when
invoking mtools:

@table @code
@item -o
Overwrites primary names by default.
@item -O
Overwrites secondary names by default.
@item -r
Renames primary name by default.
@item -R
Renames secondary name by default.
@item -a
Autorenames primary name by default.
@item -A
Autorenames secondary name by default.
@item -s
Skip primary name by default.
@item -S
Skip secondary name by default.
@item -m
Ask user what to do with primary name.
@item -M
Ask user what to do with secondary name.
@end table

Note that for command line switches lower/upper differentiates between
primary/secondary name whereas for interactive choices, lower/upper
differentiates between just-this-time/always.

The primary name is the name as displayed in Windows 95 or Windows NT:
i.e. the long name if it exists, and the short name otherwise.  The
secondary name is the "hidden" name, i.e. the short name if a long name
exists.

By default, the user is prompted if the primary name clashes, and the
secondary name is autorenamed.

If a name clash occurs in a Unix directory, mtools only asks whether
to overwrite the file, or to skip it.

@node case sensitivity, high capacity formats, name clashes, Common features
@section Case sensitivity of the VFAT filesystem
@cindex Case sensitivity

The VFAT filesystem is able to remember the case of the
filenames. However, filenames which differ only in case are not allowed
to coexist in the same directory. For example if you store a file called
LongFileName on a VFAT filesystem, mdir shows this file as LongFileName,
and not as Longfilename. However, if you then try to add LongFilename to
the same directory, it is refused, because case is ignored for clash
checks.

The VFAT filesystem allows to store the case of a filename in the
attribute byte, if all letters of the filename are the same case, and if
all letters of the extension are the same case too. Mtools uses this
information when displaying the files, and also to generate the Unix
filename when mcopying to a Unix directory. This may have unexpected
results when applied to files written using an pre-7.0 version of DOS:
Indeed, the old style filenames map to all upper case. This is different
from the behavior of the old version of mtools which used to generate
lower case Unix filenames.

@node high capacity formats, exit codes, case sensitivity, Common features
@section high capacity formats
@cindex Special formats
@cindex High capacity formats
@cindex Odd formats
@cindex Weird formats
@cindex Formats, high capacity
@cindex Linux enhancements (High Capacity Formats)

Mtools supports a number of formats which allow to store more data on
disk as usual. Due to different operating system abilities, these
formats are not supported on all OS'es. Mtools recognizes these formats
transparently where supported.

In order to format these disks, you need to use an operating system
specific tool. For Linux, suitable floppy tools can be found in the
@code{fdutils} package at the following locations~:
@example
@code{ftp://www.tux.org/pub/knaff/fdutils/}.
@code{ftp://sunsite.unc.edu/pub/Linux/utils/disk-management/fdutils-*}
@end example

See the manpages included in that package for further detail: Use
@code{superformat} to format all formats except XDF, and use
@code{xdfcopy} to format XDF.

@menu
* more sectors::      Putting more sectors per track on the disk
* bigger sectors::    Use bigger sectors to save header space
* 2m::                Use a standard first track
* XDF::               OS/2's eXtended density format
@end menu

@node more sectors, bigger sectors, high capacity formats, high capacity formats
@subsection More sectors
@cindex fdformat
@cindex vgacopy
@cindex DMF disks
@cindex Windows 95 (DMF disks)

The oldest method of fitting more data on a disk is to use more sectors
and more cylinders. Although the standard format uses 80 cylinders and
18 sectors (on a 3 1/2 high density disk), it is possible to use up to
83 cylinders (on most drives) and up to 21 sectors. This method allows
to store up to 1743K on a 3 1/2 HD disk. However, 21 sector disks are
twice as slow as the standard 18 sector disks because the sectors are
packed so close together that we need to interleave them. This problem
doesn't exist for 20 sector formats.

These formats are supported by numerous DOS shareware utilities such as
@code{fdformat} and @code{vgacopy}. In his infinite hybris, Bill Gate$
believed that he invented this, and called it @samp{DMF disks}, or
@samp{Windows formatted disks}. But in reality, it has already existed
years before! Mtools supports these formats on Linux, on SunOs and on
the DELL Unix PC.

@node bigger sectors, 2m, more sectors, high capacity formats
@subsection Bigger sectors
@cindex 2m
By using bigger sectors it is possible to go beyond the capacity which
can be obtained by the standard 512-byte sectors. This is because of the
sector header. The sector header has the same size, regardless of how
many data bytes are in the sector. Thus, we save some space by using
@emph{fewer}, but bigger sectors. For example, 1 sector of 4K only takes
up header space once, whereas 8 sectors of 512 bytes have also 8
headers, for the same amount of useful data.

This method allows to store up to 1992K on a 3 1/2 HD disk.

Mtools supports these formats only on Linux.

@node 2m, XDF, bigger sectors, high capacity formats
@subsection 2m
@cindex 2m

The 2m format was originally invented by Ciriaco Garcia de Celis. It
also uses bigger sectors than usual in order to fit more data on the
disk.  However, it uses the standard format (18 sectors of 512 bytes
each) on the first cylinder, in order to make these disks easyer to
handle by DOS. Indeed this method allows to have a standard sized
bootsector, which contains a description of how the rest of the disk
should be read.

However, the drawback of this is that the first cylinder can hold less
data than the others. Unfortunately, DOS can only handle disks where
each track contains the same amount of data. Thus 2m hides the fact that
the first track contains less data by using a @dfn{shadow
FAT}. (Usually, DOS stores the FAT in two identical copies, for
additional safety.  XDF stores only one copy, and it tells DOS that it
stores two. Thus the same that would be taken up by the second FAT copy
is saved.) This also means that your should @strong{never use a 2m disk
to store anything else than a DOS fs}.

Mtools supports these format only on Linux.

@node XDF, , 2m, high capacity formats
@subsection XDF
@cindex XDF disks
@cindex OS/2 (XDF disks)

XDF is a high capacity format used by OS/2. It can hold 1840 K per
disk. That's lower than the best 2m formats, but its main advantage is
that it is fast: 600 milliseconds per track. That's faster than the 21
sector format, and almost as fast as the standard 18 sector format. In
order to access these disks, make sure mtools has been compiled with XDF
support, and set the @code{use_xdf} variable for the drive in the
configuration file. @xref{Compiling mtools} and @ref{misc variables},
for details on how to do this. Fast XDF access is only available for
Linux kernels which are more recent than 1.1.34.

Mtools supports this format only on Linux.

@strong{Caution / Attention distributors}: If mtools is compiled on a
Linux kernel more recent than 1.3.34, it won't run on an older
kernel. However, if it has been compiled on an older kernel, it still
runs on a newer kernel, except that XDF access is slower. It is
recommended that distribution authors only include mtools binaries
compiled on kernels older than 1.3.34 until 2.0 comes out. When 2.0 will
be out, mtools binaries compiled on newer kernels may (and should) be
distributed. Mtools binaries compiled on kernels older than 1.3.34 won't
run on any 2.1 kernel or later.

@node exit codes, bugs, high capacity formats, Common features
@section Exit codes
All the Mtools commands return 0 on success, 1 on utter failure, or 2
on partial failure.  All the Mtools commands perform a few sanity
checks before going ahead, to make sure that the disk is indeed an
MS-DOS disk (as opposed to, say an ext2 or minix disk). These checks
may reject partially corrupted disks, which might otherwise still be
readable. To avoid these checks, set the MTOOLS_SKIP_CHECK
environmental variable or the corresponding configuration file variable
(@pxref{global variables})
@node bugs, , exit codes, Common features
@section Bugs
An unfortunate side effect of not guessing the proper device (when
multiple disk capacities are supported) is an occasional error message
from the device driver.  These can be safely ignored.  

The fat checking code chokes on 1.72 Mb disks mformatted with pre-2.0.7
mtools. Set the environmental variable MTOOLS_FAT_COMPATIBILITY (or the
corresponding configuration file variable, @ref{global variables}) to
bypass the fat checking.

@node Configuration, Commands, Common features, Top
@chapter How to configure mtools for your environment
@section Description
@cindex Configuration files
@vindex MTOOLSRC

 This sections explains the syntax of the configurations files for
mtools. The configuration files are called
@file{/usr/local/etc/mtools.conf} and @file{~/.mtoolsrc}. If the
environmental variable @code{MTOOLSRC} is set, its contents is used as
the filename for a third configuration file. These configuration files
describe the following items:

@itemize @bullet
@item Global configuration flags and variables
@item Per drive flags and variables
@item Character translation tables
@end itemize


@menu
* config file location::  Where mtools looks for its configuration files
* general syntax::        The layout of the configuration files
* default values::        Why you don't need a config file in most cases
* global variables::      Variables that are independent of the drive
* per drive variables::   Variables that are specific to a given drive
* character sets::        Character set translation tables
* parsing order::         Location of configuration files and parsing order
* old style config::      Backwards compatibility
@end menu

@node config file location, general syntax, Configuration, Configuration
@section Location of the configuration files

@cindex Configuration file name
@cindex Name of configuration files
@cindex Location of configuration files

@file{/usr/local/etc/mtools.conf} is the system-wide configuration file,
and @file{~/.mtoolsrc} is the user's private configuration file.

On some systems, the system-wide configuration file is called
@file{/etc/defaults/mtools.conf} instead.


@node general syntax, default values, config file location, Configuration
@subsection General configuration file syntax
@cindex Syntax of the configuration file
@cindex Configuration file syntax

The configuration files is made up of sections. Each section starts
with a keyword identifying the section followed by a colon.
Then follow variable assignments and flags. Variable assignments take
the following form:
@display
name=value
@end display
Flags are lone keywords without an equal sign and value following
them.  A section either ends at the end of the file or where the next
section begins.

Lines starting with a hash (@code{#}) are comments. Newline characters
are equivalent to whitespace (except where ending a comment). The
configuration file is case insensitive, except for item enclosed in
quotes (such as filenames).

@node default values, global variables, general syntax, Configuration
@section Default values
@cindex Default values
@cindex Default configuration
@cindex Configuration file
For most platforms, mtools contains reasonable compiled-in defaults for
physical floppy drives.  Thus, you usually don't need to bother with the
configuration file, if all you want to do with mtools is to access your
floppy drives. On the other hand, the configuration file is needed if
you also want to use mtools to access your hard disk partitions and
dosemu image files.

@node global variables, per drive variables, default values, Configuration
@section Global variables
@cindex Global configuration variables
@cindex Drive independent configuration variables
@cindex Environmental variables
@vindex MTOOLS_SKIP_CHECK
@vindex MTOOLS_FAT_COMPATIBILITY
@vindex MTOOLS_LOWER_CASE
@vindex MTOOLS_NO_VFAT
@cindex FreeDos

Global flags may be set to 1 or to 0.

The following global flags are recognized:

@table @code
@item MTOOLS_SKIP_CHECK
If this is set to 1, mtools skips most of its sanity checks. This is
needed to read some Atari disks which have been made with the earlier
ROMs, and which would not be recognized otherwise.
@item MTOOLS_FAT_COMPATIBILITY
If this is set to 1, mtools skips the fat size checks. Some disks have
a bigger FAT than they really need to. These are rejected if this
option is not set.
@item MTOOLS_LOWER_CASE
If this is set to 1, mtools displays all-upper-case short filenames as
lowercase. This has been done to allow a behavior which is consistent
with older versions of mtools which didn't know about the case bits.
@item MTOOLS_NO_VFAT
If this is set to 1, mtools won't generate VFAT entries for filenames
which are mixed-case, but otherwise legal dos filenames.  This is useful
when working with DOS versions which can't grok VFAT longnames, such as
FreeDos.
@item MTOOLS_DOTTED_DIR
In a wide directory, prints the short name with a dot instead of spaces
separating the basename and the extension.
@item MTOOLS_NAME_NUMERIC_TAIL
If this is set to one (default), generate numeric tails for all long
names (~1).  If set to zero, only generate numeric tails if otherwise a
clash would have happened.
@item MTOOLS_TWENTY_FOUR_HOUR_CLOCK
If 1, uses the European notation for times (twenty four hour clock),
else uses the UK/US notation (am/pm)
@end table

Example:
Inserting the following line into your configuration file instructs
mtools to skip the sanity checks:
@example
  MTOOLS_SKIP_CHECK=1
@end example

Global variables may also be set via the environment:
@example
  export MTOOLS_SKIP_CHECK=1
@end example

Global string variables may be set to any value:
@table @code
@item MTOOLS_DATE_STRING
The format used for printing dates of files.  By default, is dd-mm-yyyy.
@end table

@node per drive variables, character sets, global variables, Configuration
@section Per drive flags and variables
@cindex Drive description
@cindex Drive configuration

@menu
* general information::   What a drive description looks like
* geometry description::  Describes the physical characteristics of
                          the media
* open flags::            Flags passed to the open system call when the
                          device is opened
* misc variables::        Variables which don't fit in either category
* misc flags::		  Switch variables, which can be enabled or disabled
* multiple descriptions:: How to supply several descriptions for a
                          drive, to be tried one after the other.
@end menu

@node general information, geometry description, per drive variables, per drive variables
@subsection General information
@cindex Drive description, example
@cindex Drive configuration, example
@vindex drive

Per drive flags and values may be described in a drive section. A
drive section starts with
@code{drive} "@var{driveletter}" :

Then follow variable-value pairs and flags.

This is a sample drive description:
@example
  drive a:
    file="/dev/fd0" use_xdf=1
@end example

@node geometry description, open flags, general information, per drive variables
@subsection Disk Geometry Configuration
@cindex Disk Geometry
@cindex Configuration of disk geometry
@cindex Description of disk geometry
@cindex Format of disk
@cindex High density disk
@cindex Low density disk
@pindex mformat (geometry used for)

Geometry information describes the physical characteristics about the
disk. Its has three purposes:

@table @asis
@item formatting
The geometry information is written into the boot sector of the newly
made disk. However, you may also describe the geometry information on
the command line. @xref{mformat} for details.
@item filtering
On some Unices there are device nodes which only support one physical
geometry. For instance, you might need a different node to access a disk
as high density or as low density. The geometry is compared to the
actual geometry stored on the boot sector to make sure that this device
node is able to correctly read the disk. If the geometry doesn't match,
this drive entry fails, and the next drive entry bearing the same drive
letter is tried. @xref{multiple descriptions} for more details on
supplying several descriptions for one drive letter.

If no geometry information is supplied in the configuration file, all
disks are accepted. On Linux (and on Sparc) there exist device nodes
with configurable geometry (@file{/dev/fd0}, @file{/dev/fd1} etc),
and thus filtering is not needed (and ignored) for disk drives.  (Mtools
still does do filtering on plain files (disk images) in Linux: this is
mainly intended for test purposes, as I don't have access to a Unix
which would actually need filtering).

If you do not need filtering, but want still a default geometry for
mformatting, you may switch off filtering using the @code{mformat_only}
flag.

@item initial geometry
On devices that support it (usually floppy devices), the geometry
information is also used to set the initial geometry. This initial
geometry is applied while reading the boot sector, which contains the
real geometry.  If no geometry information is supplied in the
configuration file, or if the @code{mformat_only} flag is supplied, no
initial configuration is done.

On Linux, initial geometry is not really needed, as the configurable
devices are able to auto-detect the disk type accurately enough (for
most common formats) to read the boot sector.
@end table

Wrong geometry information may lead to very bizarre errors. That's why I
strongly recommend that you add the @code{mformat_only} flag to your
drive description, unless you really need filtering or initial geometry.

The following geometry related variables are available:

@table @code
@item cylinders
@itemx tracks
@vindex cylinders
@vindex tracks
The number of cylinders. (@code{cylinders} is the preferred form,
@code{tracks} is considered obsolete)
@item heads
@vindex heads
The number of heads (sides).
@item sectors
@vindex sectors
The number of sectors per track.
@end table

Example: the following drive section describes a 1.44M drive:

@example
  drive a:
      file="/dev/fd0H1440"
      fat_bits=12
      cylinders=80 heads=2 sectors=18
@end example

The following shorthand geometry descriptions are available:

@table @code
@item 1.44m
high density 3 1/2 disk. Equivalent to:
@code{fat_bits=12 cylinders=80 heads=2 sectors=18}
@item 1.2m
high density 5 1/4 disk. Equivalent to:
@code{fat_bits=12 cylinders=80 heads=2 sectors=15}
@item 720k
double density 3 1/2 disk. Equivalent to:
@code{fat_bits=12 cylinders=80 heads=2 sectors=9}
@item 360k
double density 5 1/4 disk. Equivalent to:
@code{fat_bits=12 cylinders=40 heads=2 sectors=9}
@end table

The shorthand format descriptions may be amended. For example,
@code{360k sectors=8}
describes a 320k disk and is equivalent to:
@code{fat_bits=12 cylinders=40 heads=2 sectors=8}

@node open flags, misc variables, geometry description, per drive variables
@subsection Open Flags
@vindex sync
@vindex nodelay
@vindex exclusive
@cindex open flags
@cindex synchronous writing
@cindex exclusive access to a drive

Moreover, the following flags are available:

@table @code
@item sync
All i/o operations are done synchronously
@item nodelay
The device or file is opened with the O_NDELAY flag. This is needed on
some non-Linux architectures.
@item exclusive
The device or file is opened with the O_EXCL flag. On Linux, this
ensures exclusive access to the floppy drive. On most other
architectures, and for plain files it has no effect at all.
@end table


@node misc variables, misc flags, open flags, per drive variables
@section General Purpose Drive Variables
@cindex Hdimage

The following general purpose drive variables are available.  Depending
to their type, these variables can be set to a string (file, precmd) or
an integer (all others)

@table @code
@item file
@cindex Image file
@cindex Name of device node
@cindex File name of device node
@vindex file
The name of the file or device holding the disk image. This is
mandatory. The file name should be enclosed in quotes.

@item partition
@cindex Dosemu hard disk image
@cindex Zip disks (partitions)
@cindex Jaz disks (partitions)
@cindex Syquest disks
@cindex Magneto-optical disks
@cindex OS/2 (layout of removable media)
@cindex Windows NT (layout of removable media)
@cindex Removable media
@cindex Partitioned image file
Tells mtools to treat the drive as a partitioned device, and to use the
given partition. Only primary partitions are accessible using this
method, and they are numbered from 1 to 4. For logical partitions, use
the more general @code{offset} variable. The @code{partition} variable
is intended for removable media such as Syquests, ZIP drives, and
magneto-optical disks. Although traditional DOS sees Syquests and
magneto-optical disks as @samp{giant floppy disks} which are
unpartitioned, OS/2 and Windows NT treat them like hard disks,
i.e. partioned devices. The @code{partition} flag is also useful DOSEMU
hdimages. It is not recommended for hard disks for which direct access
to partitions is available through mounting.

@item offset
@cindex Ram disk
@cindex Atari Ram disk
Describes where in the file the MS-DOS filesystem starts. This is useful
for logical partitions in DOSEMU hdimages, and for ATARI ram disks. By
default, this is zero, meaning that the filesystem starts right at the
beginning of the device or file.
@item fat_bits
@vindex fat_bits
The number of FAT bits. This may be 12 or 16. This is very rarely
needed, as it can almost always be deduced from information in the
boot sector. On the contrary, describing the number of fat bits may
actually be harmful if you get it wrong. You should only use it if
mtools gets the autodetected number of fat bits wrong, or if you want
to mformat a disk with a weird number of fat bits.
@item precmd
@cindex Solaris (volcheck)
@cindex Executing commands before opening the device

On some variants of Solaris, it is necessary to call 'volcheck -v'
before opening a floppy device, in order for the system to notice that
there is indeed a disk in the drive. @code{precmd="volcheck -v"} in the
drive clause establishes the desired behavior.

@item blocksize
@cindex raw device
@cindex character devices
@cindex blocksize

This parameter represents a default block size to be always used on this
device.  All I/O is done with multiples of this block size,
independantly of the sector size registered in the filesystem's boot
sector.  This is useful for character devices whose sector size is not
512, such as for example CD Rom drives on Solaris.

@end table

Only the @code{file} variable is mandatory. The other parameters may
be left out. In that case a default value or an autodetected value is
used.



@node misc flags, multiple descriptions, misc variables, per drive variables
@section General Purpose Drive Flags

A flag can either be set to 1 (enabled) or 0 (disabled). If the value is
ommitted, it is enabled.  For example, @code{scsi} is equivalent to
@code{scsi=1}

@table @code
@item nolock
@cindex disable locking
@cindex locking (disabling it)
@cindex plain floppy: device xxx busy
Instruct mtools to not use locking on this drive.  This is needed on
systems with buggy locking semantics.  However, enabling this makes
operation less safe in cases where several users may access the same
drive at the same time.

@item scsi
@cindex setuid installation (needed for raw SCSI I/O)
@cindex Solaris (Raw access to SCSI devices such as Zip & Jaz)
@cindex SunOS (Raw access to SCSI devices such as Zip & Jaz)
@cindex Zip disks (raw Scsi access)
@cindex Jaz disks (raw Scsi access)
@cindex Syquests (raw Scsi access)
@cindex SCSI devices
When set to 1, this option tells mtools to use raw SCSI I/O instead of
the standard read/write calls to access the device. Currently, this is
supported on HP/UX, Solaris and SunOs.  This is needed because on some
architectures, such as SunOs or Solaris, PC media can't be accessed
using the @code{read} and @code{write} syscalls, because the OS expects
them to contain a Sun specific "disk label".

As raw Scsi access always uses the whole device, you need to specify the
"partition" flag in addition

On some architectures, such as Solaris, mtools needs root privileges to
be able to use the @code{scsi} option.  Thus mtools should be installed
set uid root on Solaris if you want to access Zip/Jaz drives.  Thus, if
the @code{scsi} flag is given, @code{privileged} is automatically
implied, unless explicitly disabled by @code{privileged=0}

Mtools uses its root privileges to open the device, and to issue the
actual SCSI I/O calls.  Moreover, root privileges are only used for
drives described in a system-wide configuration file such as
@file{/usr/local/etc/mtools.conf}, and not for those described in
@file{~/.mtoolsrc} or @file{$MTOOLSRC}.  

@item privileged
@cindex setuid installation
@cindex setgid installation
When set to 1, this instructs mtools to use its set-uid and set-gid
privileges for opening the given drive.  This option is only valid for
drives described in the system-wide configuration files (such as
@file{/usr/local/etc/mtools.conf}, not @file{~/.mtoolsrc} or
@file{$MTOOLSRC}).  Obviously, this option is also a no op if mtools is
not installed setuid or setgid.  This option is implied by 'scsi=1', but
again only for drives defined in system-wide configuration files.
Privileged may also be set explicitely to 0, in order to tell mtools not
to use its privileges for a given drive even if @code{scsi=1} is set.

Mtools only needs to be installed setuid if you use the
@code{privileged} or @code{scsi} drive variables.  If you do not use
these options, mtools works perfectly well even when not installed
setuid root.

@item vold
@cindex Solaris (vold)
@cindex Vold (mediamgr)

Instructs mtools to interpret the device name as a vold identifier
rather than as a filename.  The vold identifier is translated into a
real filename using the @code{media_findname()} and
@code{media_oldaliases()} functions of the @code{volmgt} library.  This
flag is only available if you configured mtools with the
@code{--enable-new-vold} option before compilation.

@item use_xdf
@cindex XDF disks (how to configure)
@vindex use_xdf
If this is set to a non-zero value, mtools also tries to access this
disk as an XDF disk. XDF is a high capacity format used by OS/2. This
is off by default. @xref{XDF} for more details.
@item mformat_only
@vindex mformat_only
Tells mtools to use the geometry for this drive only for mformatting and 
not for filtering.

@end table


@node multiple descriptions, , misc flags, per drive variables
@subsection Supplying multiple descriptions for a drive

It is possible to supply multiple descriptions for a drive. In that
case, the descriptions are tried in order until one is found that
fits. Descriptions may fail for several reasons:

@enumerate
@item
because the geometry is not appropriate,
@item
because there is no disk in the drive,
@item
or because of other problems.
@end enumerate

Multiple definitions are useful when using physical devices which are
only able to support one single disk geometry.
Example:
@example
  drive a: file="/dev/fd0H1440" 1.44m
  drive a: file="/dev/fd0H720" 720k
@end example

This instructs mtools to use /dev/fd0H1440 for 1.44m (high density)
disks and /dev/fd0H720 for 720k (double density) disks. On Linux, this
feature is not really needed, as the /dev/fd0 device is able to handle
any geometry.

You may also use multiple drive descriptions to access both of your
physical drives through one drive letter:

@example
  drive z: file="/dev/fd0"
  drive z: file="/dev/fd1"
@end example

With this description, @code{mdir z:} accesses your first physical
drive if it contains a disk. If the first drive doesn't contain a disk,
mtools checks the second drive.

When using multiple configuration files, drive descriptions in the files
parsed last override descriptions for the same drive in earlier
files. In order to avoid this, use the @code{drive+} or @code{+drive}
keywords instead of @code{drive}. The first adds a description to the
end of the list (i.e. it will be tried last), and the first adds it to
the start of the list.

@node character sets, parsing order, per drive variables, Configuration
@section Character set translation tables
@cindex Internationalization
@cindex Accented characters
@cindex National character set

If you live in the USA, in Western Europe or in Australia, you may
skip this section.

@menu
* why::              Why character set tables are needed
* country::          Using the COUNTRY variable to select tables
* explicit tables::  Supplying a new table for an unknown country
@end menu

@node why, country, character sets, character sets
@subsection Why character set translation tables are needed

DOS uses a different character code mapping than Unix. 7-bit
characters still have the same meaning, only characters with the eight
bit set are affected. To make matters worse, there are several
translation tables available depending on the country where you
are. The appearance of the characters is defined using
code pages. These code pages aren't the same for all countries. For
instance, some code pages don't contain upper case accented
characters. On the other hand, some code pages contain characters which
don't exist in Unix, such as certain line-drawing characters or
accented consonants used by some Eastern European countries. This
affects two things, relating to filenames:

@table @asis
@item upper case characters
In short names, only upper case characters are allowed. This also
holds for accented characters. For instance, in a code page which
doesn't contain accented uppercase characters, the accented lowercase
characters get transformed into their unaccented counterparts.
@item long file names
Micro$oft has finally come to their senses and uses a more standard
mapping for the long file names. They use Unicode, which is basically
a 32 bit version of ASCII. Its first 256 characters are identical to
Unix ASCII. Thus, the code page also affects the correspondence
between the codes used in long names and those used in short names
@end table


Mtools considers the filenames entered on the command line as having the
Unix mapping, and translates the characters to get short names.  By
default, code page 850 is used with the Swiss uppercase/lowercase
mapping. I chose this code page, because its set of existing characters
most closely matches Unix's. Moreover, this code page covers most
characters in use in the USA, Australia and Western Europe. However, it
is still possible to chose a different mapping. There are two methods:
the @code{country} variable and explicit tables.

@node country, explicit tables, why, character sets
@subsection Configuration using Country

The @code{COUNTRY} variable is recommended for people which also have
access to MS-DOS system files and documentation. If you don't have access
to these, I'd suggest you'd rather use explicit tables instead.

Syntax:

@code{COUNTRY="}@var{country}@code{[,[}@var{codepage}@code{],}
@var{country-file}@code{]"}

This tells mtools to use a Unix-to-DOS translation table which matches
@var{codepage} and an lowercase-to-uppercase table for @var{country} and
to use the @var{country-file} file to get the lowercase-to-uppercase
table. The country code is most often the telephone prefix of the
country. Refer to the DOS help page on "country" for more details. The
@var{codepage} and the @var{country-file} parameters are
optional. Please don't type in the square brackets, they are only there
to say which parameters are optional. The @var{country-file} file is
supplied with MS-DOS, and is usually called @file{COUNTRY.SYS}, and
stored in the @file{C:\DOS} directory. In most cases you don't need it,
as the most common translation tables are compiled into mtools. So,
don't worry if you run a Unix-only box which lacks this file.

If @var{codepage} is not given, a per country default code page is
used. If the @var{country-file} parameter isn't given, compiled-in
defaults are used for the lowercase-to-uppercase table. This is useful
for other Unices than Linux, which may have no @file{COUNTRY.SYS} file
available online.

The Unix-to-DOS are not contained in the @file{COUNTRY.SYS} file, and
thus mtools always uses compiled-in defaults for those. Thus, only a
limited amount of code pages are supported. If your preferred code page
is missing, or if you know the name of the Windows 95 file which
contains this mapping, could you please drop me a line at
@code{Alain.Knaff@@poboxes.com}.

The @code{COUNTRY} variable can also be set using the environment.

@node explicit tables, , country, character sets
@subsection Configuration using explicit translation tables

Translation tables may be described in line in the configuration
file. Two tables are needed: first the DOS-to-Unix table, and then the
Lowercase-to-Uppercase table. A DOS-to-Unix table starts with the
@code{tounix}
keyword, followed by a colon, and 128 hexadecimal numbers.
A lower-to-upper table starts with the
@code{fucase}
keyword, followed by a colon, and 128 hexadecimal numbers.

The tables only show the translations for characters whose codes is
greater than 128, because translation for lower codes is trivial.

Example:
@vindex tounix
@vindex fucase

@example
 tounix:
   0xc7 0xfc 0xe9 0xe2 0xe4 0xe0 0xe5 0xe7 
   0xea 0xeb 0xe8 0xef 0xee 0xec 0xc4 0xc5 
   0xc9 0xe6 0xc6 0xf4 0xf6 0xf2 0xfb 0xf9 
   0xff 0xd6 0xdc 0xf8 0xa3 0xd8 0xd7 0x5f 
   0xe1 0xed 0xf3 0xfa 0xf1 0xd1 0xaa 0xba 
   0xbf 0xae 0xac 0xbd 0xbc 0xa1 0xab 0xbb 
   0x5f 0x5f 0x5f 0x5f 0x5f 0xc1 0xc2 0xc0 
   0xa9 0x5f 0x5f 0x5f 0x5f 0xa2 0xa5 0xac 
   0x5f 0x5f 0x5f 0x5f 0x5f 0x5f 0xe3 0xc3 
   0x5f 0x5f 0x5f 0x5f 0x5f 0x5f 0x5f 0xa4 
   0xf0 0xd0 0xc9 0xcb 0xc8 0x69 0xcd 0xce 
   0xcf 0x5f 0x5f 0x5f 0x5f 0x7c 0x49 0x5f 
   0xd3 0xdf 0xd4 0xd2 0xf5 0xd5 0xb5 0xfe 
   0xde 0xda 0xd9 0xfd 0xdd 0xde 0xaf 0xb4 
   0xad 0xb1 0x5f 0xbe 0xb6 0xa7 0xf7 0xb8 
   0xb0 0xa8 0xb7 0xb9 0xb3 0xb2 0x5f 0x5f 

 fucase:
   0x80 0x9a 0x90 0xb6 0x8e 0xb7 0x8f 0x80 
   0xd2 0xd3 0xd4 0xd8 0xd7 0xde 0x8e 0x8f 
   0x90 0x92 0x92 0xe2 0x99 0xe3 0xea 0xeb 
   0x59 0x99 0x9a 0x9d 0x9c 0x9d 0x9e 0x9f 
   0xb5 0xd6 0xe0 0xe9 0xa5 0xa5 0xa6 0xa7 
   0xa8 0xa9 0xaa 0xab 0xac 0xad 0xae 0xaf 
   0xb0 0xb1 0xb2 0xb3 0xb4 0xb5 0xb6 0xb7 
   0xb8 0xb9 0xba 0xbb 0xbc 0xbd 0xbe 0xbf 
   0xc0 0xc1 0xc2 0xc3 0xc4 0xc5 0xc7 0xc7 
   0xc8 0xc9 0xca 0xcb 0xcc 0xcd 0xce 0xcf 
   0xd1 0xd1 0xd2 0xd3 0xd4 0x49 0xd6 0xd7 
   0xd8 0xd9 0xda 0xdb 0xdc 0xdd 0xde 0xdf 
   0xe0 0xe1 0xe2 0xe3 0xe5 0xe5 0xe6 0xe8 
   0xe8 0xe9 0xea 0xeb 0xed 0xed 0xee 0xef 
   0xf0 0xf1 0xf2 0xf3 0xf4 0xf5 0xf6 0xf7 
   0xf8 0xf9 0xfa 0xfb 0xfc 0xfd 0xfe 0xff 
@end example

The first table maps DOS character codes to Unix character codes. For
example, the DOS character number 129. This is a u with to dots on top
of it. To translate it into Unix, we look at the character number 1 in
the first table (1 = 129 - 128). This is 0xfc. (Beware, numbering
starts at 0).
The second table maps lower case DOS characters to upper case DOS
characters. The same lower case u with dots maps to character 0x9a,
which is an uppercase U with dots in DOS.

@subsection Unicode characters greater than 256
If an existing MS-DOS name contains Unicode character greater than 256,
these are translated to underscores or to characters which are close
in visual appearance. For example, accented consonants are translated
into their unaccented counterparts. This translation is used for mdir
and for the Unix filenames generated by mcopy. Linux does support
Unicode too, but unfortunately too few applications support it yet to bother
with it in mtools. Most importantly, xterm can't display Unicode
yet. If there is sufficient demand, I might include support for
Unicode in the Unix filenames as well.

@strong{Caution:}
When deleting files with mtools, the underscore matches all characters
which can't be represented in Unix. Be careful with mdel!

@node parsing order, old style config, character sets, Configuration
@section Location of configuration files and parsing order
@cindex Parsing order
@cindex Configuration file parsing order
@cindex Configuration file name (parsing order)
@cindex Name of configuration files (parsing order)
@cindex Location of configuration files (parsing order)

The configuration files are parsed in the following order:
@enumerate
@item
compiled-in defaults
@item
@file{/usr/local/etc/mtools.conf}
@item
@file{/etc/mtools}
This is for backwards compatibility only, and is only parsed if
@file{mtools.conf}
doesn't exist.
@item
@file{~/.mtoolsrc}.
@item
@file{$MTOOLSRC} (file pointed by the @code{MTOOLSRC} environmental
variable)
@end enumerate

Options described in the later files override those described in the
earlier files. Drives defined in earlier files persist if they are not
overridden in the later files. For instance, drives A and B may be
defined in @file{/usr/local/etc/mtools.conf} and drives C and D may be
defined in @file{~/.mtoolsrc} However, if @file{~/.mtoolsrc} also
defines drive A, this new description would override the description of
drive A in @file{/usr/local/etc/mtools.conf} instead of adding to it. If
you want to add a new description to a drive already described in an
earlier file, you need to use either the @code{+drive} or @code{drive+}
keyword.

@node old style config, , parsing order, Configuration
@section Backwards compatibility with old configuration file syntax
@cindex Backwards compatibility
@cindex Old configuration file syntax
@cindex Configuration file, old syntax

The syntax described herein is new for version @code{mtools-3.0}. The
old line-oriented syntax is still supported. Each line beginning with a
single letter is considered to be a drive description using the old
syntax. Old style and new style drive sections may be mixed within the
same configuration file, in order to make upgrading easier. Support for
the old syntax will be phased out eventually, and in order to discourage
its use, I purposefully omit its description here.


@node Commands, Compiling mtools, Configuration, Top
@chapter Command list
@cindex Command list
@cindex List of available commands

 This section describes the available mtools commands, and the command
line parameters that each of them accepts. Options which are common to
all mtools commands are not described here, @ref{arguments} for a
description of those.

@menu
* mattrib::           change MS-DOS file attribute flags
* mbadblocks::        tests a floppy disk, and marks the bad blocks in the FAT
* mcd::               change MS-DOS directory
* mcopy::             copy MS-DOS files to/from Unix
* mdel::              delete an MS-DOS file
* mdeltree::          recursively delete an MS-DOS directory
* mdir::              display an MS-DOS directory
* mdu::               list space occupied by directory and its contents
* mformat::           add an MS-DOS filesystem to a low-level formatted floppy disk
* minfo::             get information about an MS-DOS filesystem.
* mlabel::            make an MS-DOS volume label
* mkmanifest::        makes a list of short name equivalents
* mmd::               make an MS-DOS subdirectory
* mmount::            mount an MS-DOS disk
* mpartition::        create an MS-DOS as a partition
* mrd::               remove an MS-DOS subdirectory
* mmove::             move or rename an MS-DOS file or subdirectory
* mren::              rename an existing MS-DOS file
* mshowfat::          shows the FAT map of a file
* mtoolstest::        tests and displays the configuration
* mtype::             display contents of an MS-DOS file
* mzip::              zip disk specific commands
* xcopy::             recursively copy a dos directory into another
@end menu

@node mattrib, mbadblocks, Commands, Commands
@section Mattrib
@pindex mattrib
@cindex Changing file attributes
@cindex Hidden files
@cindex Read-only files (changing the attribute)
@cindex System files
@cindex Archive bit

@code{Mattrib} is used to change MS-DOS file attribute flags. It has the
following syntax:

@code{mattrib} [@code{-a|+a}] [@code{-h|+h}] [@code{-r|+r}]
[@code{-s|+s}] [@code{-/}]  [@code{-X}] @var{msdosfile} [ @var{msdosfiles} @dots{} ]

@code{Mattrib} adds attribute flags to an MS-DOS file (with the
`@code{+}' operator) or remove attribute flags (with the `@code{-}'
operator).

@code{Mattrib} supports the following attribute bits:

@table @code
@item a
Archive bit.  Used by some backup programs to indicate a new file.
@item r
Read-only bit.  Used to indicate a read-only file.  Files with this bit
set cannot be erased by @code{DEL} nor modified.
@item s
System bit.  Used by MS-DOS to indicate a operating system file.
@item h
Hidden bit.  Used to make files hidden from @code{DIR}.
@end table

@code{Mattrib} supports the following command line flags:
@table @code
@item /
Recursive.  Recursively list the attributes of the files in the subdirectories.
@item X
Concise. Prints the attributes whithout any whitespace padding.  This is 
convenient for script.  If neither the "/" option is given, nor the
@var{msdosfile} contains a wildcard, and there is only one Msdos file
parameter on the command line, only the attribute is printed, and not
the filename.
This option is convenient for scripts
@end table

@node mbadblocks, mcd, mattrib, Commands
@section Mbadblocks

The @code{mbadblocks} command is used to scan an MS-DOS floppy and mark
its unused bad blocks as bad. It uses the following syntax:

@code{mbadblocks} @var{drive}@code{:}
@pindex mbadblocks
@cindex Marking blocks as bad
@cindex Bad blocks
@cindex Read errors

@code{Mbadblocks} scans an MS-DOS floppy for bad blocks. All unused bad
blocks are marked as such in the FAT. This is intended to be used right
after @code{mformat}.  It is not intended to salvage bad disks.
@subsection Bugs
@code{Mbadblocks} should (but doesn't yet :-( ) also try to salvage bad
blocks which are in use by reading them repeatedly, and then mark them
bad.

@node mcd, mcopy, mbadblocks, Commands
@section Mcd
@pindex mcd
@cindex Directory (changing)
@cindex Working directory
@cindex Current working directory (changing the)
@cindex Default directory (changing the)
@cindex Mcwd file

The @code{mcd} command is used to change the mtools working directory
on the MS-DOS disk. It uses the following syntax:

@example
@code{mcd} [@var{msdosdirectory}]
@end example

Without arguments, @code{mcd} reports the current device and working
directory.  Otherwise, @code{mcd} changes the current device and current
working directory relative to an MS-DOS filesystem.

The environmental variable @code{MCWD} may be used to locate the file
where the device and current working directory information is stored.
The default is @file{$HOME/.mcwd}.  Information in this file is ignored
if the file is more than 6 hours old.

@code{Mcd} returns 0 on success or 1 on failure.

Unlike MS-DOS versions of @code{CD}, @code{mcd} can be used to change to
another device. It may be wise to remove old @file{.mcwd} files at logout.

@node mcopy, mdel, mcd, Commands
@section Mcopy
@pindex mcopy
@cindex Reading MS-DOS files
@cindex Writing MS-DOS files
@cindex Copying MS-DOS files
@cindex Concatenating MS-DOS files
@cindex Text files
@cindex CR/LF conversions

The @code{mcopy} command is used to copy MS-DOS files to and from
Unix. It uses the following syntax:

@example
@code{mcopy} [@code{-b/ptnvmoQOsSrRA}] @var{sourcefile} @var{targetfile}
@code{mcopy} [@code{-b/ptnvmoQOsSrRA}] @var{sourcefile} [ @var{sourcefiles}@dots{} ] @var{targetdirectory}
@code{mcopy} [@code{-tnvm}] @var{MSDOSsourcefile}
@end example



@code{Mcopy} copies the specified file to the named file, or copies
multiple files to the named directory.  The source and target can be
either MS-DOS or Unix files.

The use of a drive letter designation on the MS-DOS files, 'a:' for
example, determines the direction of the transfer.  A missing drive
designation implies a Unix file whose path starts in the current
directory.  If a source drive letter is specified with no attached file
name (e.g. @code{mcopy a: .}), all files are copied from that drive.

If only a single, MS-DOS source parameter is provided (e.g. "mcopy
a:foo.exe"), an implied destination of the current directory
(`@code{.}') is assumed.

A filename of `@code{-}' means standard input or standard output, depending
on its position on the command line.

@code{Mcopy} accepts the following command line options:

@table @code
@item b
Batch mode. Optimized for huge recursive copies, but less secure if a
crash happens during the copy.
@item /
Recursive copy.  Also copies directories and their contents
@item p
Preserves the attributes of the copied files
@item Q
When mcopying multiple files, quits as soon as one copy fails (for
example due to lacking storage space on the target disk)
@item t
Text file transfer.  @code{Mcopy} translates incoming carriage
return/line feeds to line feeds.
@item n
No confirmation when overwriting Unix files.  @code{Mcopy} doesn't warn
the user when overwriting an existing Unix file.  In order to switch off
confirmation for DOS files, use @code{-o}.
@item m
Preserve the file modification time. If the target file already exists,
and the @code{-n} option is not in effect, @code{mcopy} asks whether to
overwrite the file or to rename the new file (@ref{name clashes}) for
details).
@end table

@subsection Bugs
Unlike MS-DOS, the '+' operator (append) from MS-DOS is not
supported. However, you may use @code{mtype} to produce the same effect:
@example
mtype a:file1 a:file2 a:file3 >unixfile
mtype a:file1 a:file2 a:file3 | mcopy - a:msdosfile
@end example

@node mdel, mdeltree, mcopy, Commands
@section Mdel
@pindex mdel
@cindex removing MS-DOS files
@cindex erasing MS-DOS files
@cindex deleting MS-DOS files

The @code{mdel} command is used to delete an MS-DOS file. Its syntax
is:

@display
@code{mdel} [@code{-v}] @var{msdosfile} [ @var{msdosfiles} @dots{}  ]
@end display

@code{Mdel} deletes files on an MS-DOS filesystem.

@code{Mdel} asks for verification prior to removing a read-only file.

@node mdeltree, mdir, mdel, Commands
@section Mdeltree
@pindex mdeltree
@cindex removing an MS-DOS directory recursively
@cindex erasing an MS-DOS directory recursively
@cindex deleting an MS-DOS directory recursively
@cindex recursively removing an MS-DOS directory

The @code{mdeltree} command is used to delete an MS-DOS file. Its syntax
is:

@display
@code{mdeltree} [@code{-v}] @var{msdosdirectory} [@var{msdosdirectories}@dots{}]
@end display

@code{Mdeltree} removes a directory and all the files and subdirectories
it contains from an MS-DOS filesystem. An error occurs if the directory
to be removed does not exist.

@node mdir, mdu, mdeltree, Commands
@section Mdir
@pindex mdir
@cindex Read-only files (listing them)
@cindex Listing a directory
@cindex Directory listing

The @code{mdir} command is used to display an MS-DOS directory. Its
syntax is:

@code{mdir} [@code{-/}] [@code{-f}] [@code{-w}] [@code{-a}] [@code{-X}] @var{msdosfile} [ @var{msdosfiles}@dots{}] 

@code{Mdir}
displays the contents of MS-DOS directories, or the entries for some
MS-DOS files.

@code{Mdir} supports the following command line options:

@table @code
@item /
Recursive output, just like Dos' @code{-s} option
@item w
Wide output.  With this option, @code{mdir} prints the filenames across
the page without displaying the file size or creation date.
@item a
Also list hidden files.
@item f
Fast.  Do not try to find out free space.  On larger disks, finding out
the amount of free space takes up some non trivial amount of time, as
the whole FAT must be read in and scanned.  The @code{-f} flag bypasses
this step.  This flag is not needed on FAT32 filesystems, which store
the size explicitely.
@item X
Concise listing.  List only a newline separated list of pathnames
without any decoration nor additional information
@end table

An error occurs if a component of the path is not a directory.

@node mdu, mformat, mdir, Commands, Commands
@section Mdu
@pindex mdu
@cindex Space occupied by directories and files
@cindex du
@cindex Listing space occupied by directories and files
@cindex Occupation of space by directories and files

@code{Mdu} is used to list the space occupied by a directory, its
subdirectories and its files. It is similar to the @code{du} command on
Unix.  The unit used are clusters.  Use the minfo command to find out
the cluster size.

@code{mdu} [@code{-a}] [ @var{msdosfiles} @dots{} ]


@table @code
@item a
All files.  List also the space occupied for individual files.
@item s
Only list the total space, don't give details for each subdirectory.
@end table



@node mformat, mkmanifest, mdu, Commands
@section Mformat
@pindex mformat
@cindex Initializing disks
@cindex Formatting disks
@cindex Filesystem creation

The @code{mformat} command is used to add an MS-DOS filesystem to a
low-level formatted diskette. Its syntax is:

@display
@code{mformat} [@code{-t} @var{cylinders}] [@code{-h} @var{heads}]
[@code{-s} @var{sectors}] [@code{-l} @var{volume_label}] [@code{-F}]
[@code{-I} @var{fsVersion}] [@code{-S} @var{sizecode}] [@code{-2}
@var{sectors_on_track_0}] [@code{-M} @var{software_sector_size}]
[@code{-a}] [@code{-X}] [@code{-C}] [@code{-H} @var{hidden_sectors}]
[@code{-r} @var{root_sectors}] [@code{-B} @var{boot_sector}]
[@code{-k}] @var{drive:}
@end display

@code{Mformat} adds a minimal MS-DOS filesystem (boot sector, FAT, and
root directory) to a diskette that has already been formatted by a Unix
low-level format.


The following options are supported: (The S, 2, 1 and M options may not
exist if this copy of mtools has been compiled without the USE_2M
option)

@c xMANoptions

@table @code
@item t
The number of cylinders.
@item h
The number of heads (sides).
@item s
The number of sectors per track. If the 2m option is given, number of
512-byte sector equivalents on generic tracks (i.e. not head 0 track 0).
If the 2m option is not given, number of physical sectors per track
(which may be bigger than 512 bytes).
@item l
An optional volume label.
@item S
The sizecode. The size of the sector is 2 ^ (sizecode + 7).
@item 2
2m format. The parameter to this option describes the number of
sectors on track 0, head 0. This option is recommended for sectors
bigger than normal.
@item 1
don't use a 2m format, even if the current geometry of the disk is a 2m 
geometry.
@item M
software sector size. This parameter describes the sector size in bytes used
by the MS-DOS filesystem. By default it is the physical sector size.
@item a
If this option is given, an Atari style serial number is generated.
Ataris store their serial number in the OEM label.
@item X
formats the disk as an XDF disk. @xref{XDF} for more details. The
disk has first to be low-level formatted using the xdfcopy utility
included in the fdutils package.
@item C
creates the disk image file to install the MS-DOS filesystem on
it. Obviously, this is useless on physical devices such as floppies
and hard disk partitions.
@item H
number of hidden sectors. This parameter is useful for formatting hard
disk partition, which are not aligned on track boundaries (i.e. first
head of first track doesn't belong to the partition, but contains a
partition table). In that case the number of hidden sectors is in
general the number of sectors per cylinder. This is untested.
@item n
serial number
@item F
Format the partition as FAT32 (experimental).
@item I
Sets the fsVersion id when formatting a FAT32 drive.  In order to find
this out, run minfo on an existing FAT32 drive, and mail me about it, so
I can include the correct value in future versions of mtools.
@item c
Sets the size of a cluster (in sectors).  If this cluster size would
generate a FAT that too big for its number of bits, mtools automatically
increases the cluster size, until the FAT is small enough.
@item r
Sets the size of the root directory (in sectors).  Only applicable to 12
and 16 bit FATs.
@item B
Use the bootsector stored in the given file or device, instead of using
its own.  Only the geometry fields are updated to match the target disks
parameters.
@item k
Keep the existing boot sector as much as possible.  Only the geometry
fields are updated to match the target disks parameters.
@end table

To format a diskette at a density other than the default, you must supply
(at least) those command line parameters that are different from the
default.

@code{Mformat} returns 0 on success or 1 on failure.

It doesn't record bad block information to the Fat, use
@code{mkmanifest} for that.

@node mkmanifest, minfo, mformat, Commands
@section Mkmanifest
@pindex mkmanifest
@cindex packing list

The @code{mkmanifest} command is used to create a shell script (packing
list) to restore Unix filenames. Its syntax is:

@code{mkmanifest} [ @var{files} ]

@code{Mkmanifest} creates a shell script that aids in the restoration of
Unix filenames that got clobbered by the MS-DOS filename restrictions.
MS-DOS filenames are restricted to 8 character names, 3 character
extensions, upper case only, no device names, and no illegal characters.


The mkmanifest program is compatible with the methods used in
@code{pcomm, arc,} and @code{mtools} to change perfectly good Unix
filenames to fit the MS-DOS restrictions. This command is only useful if
the target system which will read the diskette cannot handle vfat long
names.

@subsection Example
You want to copy the following Unix files to a MS-DOS diskette (using the
@code{mcopy} command).

@example
  very_long_name
  2.many.dots
  illegal:
  good.c
  prn.dev
  Capital
@end example

@code{Mcopy}
converts the names to:

@example
  very_lon
  2xmany.dot
  illegalx
  good.c
  xprn.dev
  capital
@end example

The command:
@example
mkmanifest very_long_name 2.many.dots illegal: good.c prn.dev Capital >manifest
@end example
would produce the following:
@example
  mv very_lon very_long_name
  mv 2xmany.dot 2.many.dots
  mv illegalx illegal:
  mv xprn.dev prn.dev
  mv capital Capital
@end example

Notice that "good.c" did not require any conversion, so it did not
appear in the output.

Suppose I've copied these files from the diskette to another Unix
system, and I now want the files back to their original names.  If the
file "manifest" (the output captured above) was sent along with those
files, it could be used to convert the filenames.

@subsection Bugs

The short names generated by @code{mkmanifest} follow the old convention
(from mtools-2.0.7) and not the one from Windows 95 and mtools-3.0.


@node minfo, mlabel, mkmanifest, Commands
@section Minfo
@pindex mlabel
@cindex mformat parameters
@cindex getting parameters of a Dos fs

The @code{minfo} command prints the parameters of a Dos filesystem, such
as number of sectors, heads and cylinders.  It also prints an mformat
command line which can be used to create a similar Dos filesystem on
another media.  However, this doesn't work with 2m or Xdf media, and
with Dos 1.0 filesystems
@display
@code{minfo} @var{drive}:
@end display

Mlabel supports the following option:
@table @code
@item v
Prints a hexdump of the bootsector, in addition to the other information
@end table


@node mlabel, mmd, minfo, Commands
@section Mlabel
@pindex mlabel
@cindex Labeling a disk
@cindex Disk label

The @code{mlabel} command adds a volume label to a disk. Its syntax is:
@display
@code{mlabel} [@code{-vcs}] @var{drive}:[@var{new_label}]
@end display

@code{Mlabel} displays the current volume label, if present. If
@var{new_label} is not given, and if neither the @code{c} nor the
@code{s} options are set, it prompts the user for a new volume label.
To delete an existing volume label, press return at the prompt.

Reasonable care is taken to create a valid MS-DOS volume label.  If an
invalid label is specified, @code{mlabel} changes the label (and
displays the new label if the verbose mode is set). @code{Mlabel}
returns 0 on success or 1 on failure.

Mlabel supports the following options:
@table @code
@item c
Clears an existing label, without prompting the user
@item s
Shows the existing label, without prompting the user.
@end table


@node mmd, mmount, mlabel, Commands
@section Mmd
@pindex mmd
@cindex Making a directory
@cindex Creating a directory
@cindex Directory creation
@cindex Subdirectory creation

The @code{mmd} command is used to make an MS-DOS subdirectory. Its
syntax is:

@code{mmd} [@code{-voOsSrRA}] @var{msdosdirectory} [
@var{msdosdirectories}@dots{} ]

@code{Mmd} makes a new directory on an MS-DOS filesystem. An error occurs
if the directory already exists.


@node mmount, mmove, mmd, Commands
@section Mmount
@pindex mmount
@cindex Linux enhancements (mmount)
@cindex Mounting a disk
@cindex High capacity formats, mounting

The @code{mmount} command is used to mount an MS-DOS disk. It is only
available on Linux, as it is only useful if the OS kernel allows to
configure the disk geometry. Its syntax is:

@code{mmount} @var{msdosdrive} [@var{mountargs}]

@code{Mmount}
reads the boot sector of an MS-DOS disk, configures the drive geometry,
and finally mounts it passing
@code{mountargs} to @code{mount. }
If no mount arguments are specified, the name of the device is
used. If the disk is write protected, it is automatically mounted read
only.


@node mmove, mpartition, mmount, Commands
@section Mmove
@pindex mmove
@cindex Moving files (mmove)
@cindex Renaming files (mmove)

The @code{mmove} command is used to moves or renames an existing MS-DOS
file or subdirectory.
@display
@code{mmove} [@code{-voOsSrRA}] @var{sourcefile} @var{targetfile}
@code{mmove} [@code{-voOsSrRA}] @var{sourcefile} [ @var{sourcefiles}@dots{} ] @var{targetdirectory}
@end display
@code{Mmove} moves or renames an existing MS-DOS file or
subdirectory. Unlike the MS-DOS version of @code{MOVE}, @code{mmove} is
able to move subdirectories.


@node mpartition, mrd, mmove, Commands
@section Mpartition
@pindex mpartition
@cindex partitions (creating)
@cindex Zip disks (partitioning them)
@cindex Jaz disks (partitioning them)

The @code{mpartition} command is used to create MS-DOS filesystems as
partitions.  This is intended to be used on non-Linux systems,
i.e. systems where fdisk and easy access to Scsi devices are not
available.  This command only works on drives whose partition variable
is set.

@display
@code{mpartition} @code{-p} @var{drive}
@code{mpartition} @code{-r} @var{drive}
@code{mpartition} @code{-I} @var{drive}
@code{mpartition} @code{-a} @var{drive}
@code{mpartition} @code{-d} @var{drive}
@code{mpartition} @code{-c} [@code{-s} @var{sectors}] [@code{-h} @var{heads}]
[@code{-t} @var{cylinders}] [@code{-v} [@code{-T} @var{type}] [@code{-b}
@var{begin}] [@code{-l} length] [@code{-f}]

@end display

Mpartition supports the following operations:

@table @code
@item p
Prints a command line to recreate the partition for the drive.  Nothing
is printed if the partition for the drive is not defined, or an
inconsistency has been detected.  If verbose (@code{-v}) is also set,
prints the current partition table.
@item r
Removes the partition described by @var{drive}.
@item I
Initializes the partition table, and removes all partitions.
@item c
Creates the partition described by @var{drive}.
@item a
"Activates" the partition, i.e. makes it bootable.  Only one partition
can be bootable at a time.
@item d
"Desactivates" the partition, i.e. makes it unbootable.
@end table

If no operation is given, the current settings are printed.

For partition creations, the following options are available:
@table @code
@item s @var{sectors}
The number of sectors per track of the partition (which is also the
number of sectors per track for the whole drive).
@item h @var{heads}
The number of heads of the partition (which is also the number of heads
for the whole drive).  By default, the geometry information (number of
sectors and heads) is figured out from neighbouring partition table
entries, or guessed from the size.
@item t @var{cylinders}
The number of cylinders of the partition (not the number of cylinders of
the whole drive.
@item b @var{begin}
The starting offset of the partition, expressed in sectors. If begin is
not given, mpartition lets the partition begin at the start of the disk
(partition number 1), or immediately after the end of the previous
partition.
@item l @var{length}
The size (length) of the partition, expressed in sectors.  If end is not
given, mpartition figures out the size from the number of sectors, heads
and cylinders.  If these are not given either, it gives the partition
the biggest possible size, considering disk size and start of the next
partition.
@end table

The following option is available for all operation which modify the
partition table:
@table @code
@item f
Usually, before writing back any changes to the partition, mpartition
performs certain consistenct checks, such as checking for overlaps and
proper alignment of the partitions.  If any of these checks fails, the
partition table is not changes.  The @code{-f} allows you to override
these safeguards.
@end table

The following option is available for all operations:
@table @code
@item v
Together with @code{-p} prints the partition table as it is now (no
change operation), or as it is after it is modified.
@item vv
If the verbosity flag is given twice, mpartition will print out a
hexdump of the partition table when reading it from and writing it to
the device.
@end table

@node mrd, mren, mpartition, Commands
@section Mrd
@pindex mrd
@cindex Removing a directory
@cindex Erasing a directory
@cindex Deleting a directory
@cindex Directory removing
@cindex Subdirectory removing

The @code{mrd} command is used to remove an MS-DOS subdirectory. Its
syntax is:

@display
@code{mrd} [@code{-v}] @var{msdosdirectory} [ @var{msdosdirectories}@dots{} ]
@end display

@code{Mrd} removes a directory from an MS-DOS filesystem. An error occurs
if the directory does not exist or is not empty.

@node mren, mshowfat, mrd, Commands
@section Mren
@pindex mren
@cindex Renaming files (mren)
@cindex Moving files (mren)

The @code{mren} command is used to rename or move an existing MS-DOS
file or subdirectory. Its syntax is:

@display
@code{mren} [@code{-voOsSrRA}] @var{sourcefile} @var{targetfile}
@end display

@code{Mren}
renames an existing file on an MS-DOS filesystem.

In verbose mode, @code{Mren} displays the new filename if the name
supplied is invalid.

If the first syntax is used (only one sourcefile), and if the target
name doesn't contain any slashes or colons, the file (or subdirectory)
is renamed in the same directory, instead of being moved to the current
@code{mcd} directory as would be the case with @code{mmove}. Unlike the
MS-DOS version of @code{REN}, @code{mren} can be used to rename
directories.

@node mshowfat, mtoolstest, mren, Commands
@section Mshowfat
@pindex mshowfat
@cindex Clusters of a file
@cindex Fat

The @code{mshowfat} command is used to display the FAT entries for a
file.  Syntax:

@display
@code{$ mshowfat files}
@end display

@node mtoolstest, mtype, mshowfat, Commands
@section Mtoolstest
@pindex mtoolstest
@cindex Testing configuration file for correctness
@cindex Checking configuration file
@cindex Verifying configuration file

The @code{mtoolstest} command is used to tests the mtools configuration
files. To invoke it, just type @code{mtoolstest} without any arguments.
@code{Mtoolstest} reads the mtools configuration files, and prints the
cumulative configuration to @code{stdout}. The output can be used as a
configuration file itself (although you might want to remove redundant
clauses).  You may use this program to convert old-style configuration
files into new style configuration files.

@node mtype, mzip, mtoolstest, Commands
@section Mtype

The @code{mtype} command is used to display contents of an MS-DOS
file. Its syntax is:

@display
@code{mtype} [@code{-ts}] @var{msdosfile} [ @var{msdosfiles}@dots{} ]
@end display

@code{Mtype} displays the specified MS-DOS file on the screen.

In addition to the standard options, @code{Mtype} allows the following
command line options:

@table @code
@item t
Text file viewing.  @code{Mtype} translates incoming carriage
return/line feeds to line feeds.
@item s
@code{Mtype} strips the high bit from the data.
@end table

The @code{mcd} command may be used to establish the device and the
current working directory (relative to MS-DOS), otherwise the default is
@code{A:/}.

@code{Mtype} returns 0 on success, 1 on utter failure, or 2 on partial
failure.

Unlike the MS-DOS version of @code{TYPE}, @code{mtype} allows multiple
arguments.


@node mzip, xcopy, mtype, Commands
@section Mzip
@cindex Zip disk (utilities)
@cindex Jaz disk (utilities)
@cindex Ejecting a Zip/Jaz disk
@cindex Write protecting a Zip/Jaz disk
@pindex mzip
@cindex ZipTools disk
@cindex Tools disk (Zip and Jaz drives)
@cindex APlaceForYourStuff
@cindex password protected Zip disks

The @code{mzip} command is used to issue ZIP disk specific commands on
Solaris or HPUX. Its syntax is:

@display
@code{mzip} [@code{-epqrwx}]
@end display

@code{Mzip} allows the following
command line options:

@table @code
@item e
Ejects the disk.
@item f
Force eject even if the disk is mounted (must be given in addition to
@code{-e}).
@item r
Write protect the disk.
@item w
Remove write protection.
@item p
Password write protect.
@item x
Password protect
@item u
Temporarily unprotect the disk until it is ejected.  The disk becomes
writable, and reverts back to its old state when ejected.
@item q
Queries the status
@end table

To remove the password, set it to one of the passwordless modes
@code{-r} or @code{-w}: mzip will then ask you for the password, and
unlock the disk.  If you have forgotten the password, you can get rid of
it by low-level formatting the disk (using your SCSI adaptor's BIOS
setup).

The ZipTools disk shipped with the drive is also password protected.  On
Dos or on a Mac, this password is automatically removed once the
ZipTools have been installed.  From various articles posted to Usenet, I
learned that the password for the tools disk is
@code{APlaceForYourStuff}@footnote{To see the articles, search for
@code{APlaceForYourStuff} using Dejanews}.  Mzip knows about this
password, and tries it first, before prompting you for a password.  Thus
@code{mzip -w z:} unlocks the tools disk@footnote{I didn't know about
this yet when I bought my own Zip drive.  Thus I ended up reformatting
my tools disk, and hence I haven't had the opportunity to test the
password yet.  If anybody still has their tools disk with the original
password, could you try it out? Thanks in advance}.  The tools disk is
formatted in a special way so as to be usable both in a PC and in a Mac.
On a PC, the Mac filesystem appears as a hidden file named
@file{partishn.mac}.  You may erase it to reclaim the 50 Megs of space
taken up by the Mac filesystem.

@node xcopy, , mzip, Commands
@section Xcopy
@cindex recursive copy
@cindex xcopy
@pindex xcopy


The @code{xcopy} script is used to recursively copy one directory to
another. Its syntax is:

@display
@code{xcopy} @var{sourcedirectory} @var{targetdirectory}
@end display


If targetdirectory does not exist, it is created.  If it does exist, the
files of sourcedirectory are directly copied into it, and no
subdirectory called @var{sourcedirectory} is created, unlike with
@code{cp -rf}.

@subsection Bugs

This command is a big kludge.  A proper implementation would take a
rework of significant parts of mtools, but unfortunately I don't have
the time for this right now. The main downside of this implementation is
that it is inefficient on some architectures (several successive calls
to mtools, which defeats mtools' caching).

@node Compiling mtools, Porting mtools, Commands, Top
@chapter Architecture specific compilation flags
@cindex XDF disks (compile time configuration)
@cindex Solaris (compile time configuration of vold)
@cindex Vold (compile time configuration)
@cindex Compile time configuration

To compile mtools, first invoke @code{./configure} before
@code{make}. In addition to the standard @code{autoconfigure} flags,
there are two architecture specific flags available.

@table @code
@item ./configure --enable-xdf
@itemx ./configure --disable-xdf
Enables support for XDF disks. This is on by default. @xref{XDF},
for details.
@item ./configure --enable-vold
@itemx ./configure --disable-vold
Enables support for vold on Solaris. When used in conjunction with vold,
mtools should uses different device nodes as for direct access.

@item ./configure --enable-new-vold
@itemx ./configure --disable-new-vold
Enables new support for vold on Solaris.  This is supposed to work more
smoothly than the old support.
@end table

@node Porting mtools, Command Index, Compiling mtools, Top
@chapter Porting mtools to architectures which are not supported yet
@cindex Porting
@cindex Compiled-in defaults

 This chapter is only interesting for those who want to port mtools to
an architecture which is not yet supported. For most common systems,
default drives are already defined. If you want to add default drives
for a still unsupported system, run config.guess, to see which
identification autoconf uses for that system. This identification is
of the form cpu-vendor-os (for example sparc-sun-sunos). The cpu and
the os parts are passed to the compiler as preprocessor flags.
 The OS part is passed to the compiler in three forms.
@enumerate
@item
The complete os name, with dots replaced by underscores.  sco3.2v2 would
yield sco3_2v2
@item
The base os name. Sco3.2v2 would yield Sco
@item
The base os name plus its major version. Sco3.2v2 would yield Sco3
@end enumerate

 All three versions are passed, if they are different.

 To define the devices, use the entries for the systems that are already
present as templates. In general, they have the following form:

@example
#if (defined (my_cpu) && defined(my_os))
#define predefined_devices
struct device devices[] = @{
        @{ "/dev/first_drive", 'drive_letter', drive_description@},
        @dots{} 
        @{ "/dev/last_drive", 'drive_letter', drive_description@}
@}
#define INIT_NOOP
#endif
@end example

 "/dev/first_drive" is the name of the device or image file
representing the drive. Drive_letter is a letter ranging from a to z
giving access to the drive. Drive_description describes the type of the
drive:
@table @code
@item ED312
extra density (2.88M) 3 1/2 disk
@item HD312
high density 3 1/2 disk
@item DD312
double density 3 1/2 disk
@item HD514
high density 5 1/4 disk
@item DD514
double density 5 1/4 disk
@item DDsmall
8 sector double density 5 1/4 disk
@item SS514
single sided double density 5 1/4 disk
@item SSsmall
single sided 8 sector double density 5 1/4 disk
@item GENFD
generic floppy drive (12 bit FAT)
@item GENHD
generic hard disk (16 bit FAT)
@item GEN
generic device (all parameters match)
@item ZIPJAZ(flags)
generic ZIP drive using normal access. This uses partition 4.
@code{Flags} are any special flags to be passed to open.
@item RZIPJAZ(flags)
generic ZIP drive using raw SCSI access. This uses partition 4.
@code{Flags} are any special flags to be passed to open.
@end table

 Entries may be described in more detail:
@example
 fat_bits,open_flags,cylinders,heads,sectors,DEF_ARG
@end example
 or, if you need to describe an offset (filesystem doesn't start at
beginning of filesystem)
@example
 fat_bits, open_flags, cylinders, heads, sectors, offset, DEF_ARG0
@end example

@table @code
@item fat_bits
is either 12, 16 or 0. 0 means that the device accepts both types of
FAT.
@item open_flags
may include flags such as O_NDELAY, or O_RDONLY, which might be
necessary to open the device. 0 means no special flags are needed.
@item cylinders,heads,sectors
describe the geometry of the disk. If cylinders is 0, the heads and sectors
parameters are ignored, and the drive accepts any geometry.
@item offset 
is used if the DOS filesystem doesn't begin at the start of the device
or image file. This is mostly useful for Atari Ram disks (which contain
their device driver at the beginning of the file) or for DOS emulator
images (which may represent a partitioned device.
@end table

 Definition of defaults in the devices file should only be done if these
same devices are found on a large number of hosts of this type. In that
case, could you also let me know about your new definitions, so that I
can include them into the next release.  For purely local file, I
recommend that you use the @code{/usr/local/etc/mtools.conf} and
@code{~/.mtoolsrc} configuration files.

 However, the devices files also allows to supply geometry setting
routines. These are necessary if you want to access high capacity
disks.

 Two routines should be supplied:

@enumerate
@item
Reading the current parameters
@example
static inline int get_parameters(int fd, struct generic_floppy_struct *floppy)
@end example

 This probes the current configured geometry, and return it in
the structure generic_floppy_struct (which must also be declared).
 Fd is an open file descriptor for the device, and buf is an already
filled in stat structure, which may be useful.
 This routine should return 1 if the probing fails, and 0 otherwise.

@item
Setting new parameters
@example
static inline int set_parameters(int fd, struct generic_floppy_struct *floppy)
                                 struct stat *buf)
@end example
 This configures the geometry contained in floppy on the file descriptor
fd. Buf is the result of a stat call (already filled in).  This should
return 1 if the new geometry cannot be configured, and 0 otherwise.
@end enumerate

 A certain number of preprocessor macros should also be supplied:

@table @code
@item TRACKS(floppy)
refers to the track field in the floppy structure
@item HEADS(floppy)
refers to the heads field in the floppy structure
@item SECTORS(floppy)
refers to the sectors per track field in the floppy structure
@item SECTORS_PER_DISK(floppy)
refers to the sectors per disk field in the floppy structure (if
applicable, otherwise leave undefined)

@item BLOCK_MAJOR
major number of the floppy device, when viewed as a block device

@item CHAR_MAJOR
major number of the floppy device, when viewed as a character device
(a.k.a. "raw" device, used for fsck) (leave this undefined, if your OS
doesn't have raw devices)
@end table

 For the truly high capacity formats (XDF, 2m, etc), there is no clean
and documented interface yet.

@c MANskip

@node Command Index, Variable Index,  Porting mtools, Top
@unnumbered Command Index
@printindex pg

@node Variable Index, Concept Index, Command Index, Top
@unnumbered Variable index
@printindex vr

@node Concept Index, , Variable Index, Top
@unnumbered Concept index
@printindex cp

@contents

@c MANend-skip
@bye
