DATA BACKUP SOLUTIONS	1

Winter, 1996

Adaptec, Inc.

	ADAPTEC® EZ-SCSI®

	If you have, or are planning to add, SCSI peripherals like tape or disk drives, CD-ROM drives, recordable CD-R drives, magneto-optical 
	drives, or scanners, Adaptec EZ-SCSI® software provides everything you need to manage and take full advantage of each device.  
	  
	Adaptec EZ-SCSI software is a suite of 32-bit practical applications and power tools that are remarkably easy to install and use.  
	Simple desktop controls give you immediate access to any fuction.  A unique online tutorial explains everything you need to know about 
	SCSI in easy-to-understand terms.  
	  
	Key benefits:  
	* Easiest way to manage SCSI peripherals  
	* For Windows operating systems  
	* Includes these practical applications:  Adaptec Easy-CD Backup™, QuickScan™, Audio CD player, Photo CD Viewer, CD Writer, and CD 
	Copier  
	* Includes these powerful tools:  SCSI Explorer™ (Power Management, SCSI Interrogator™, Read/Write Disk Cashe tool), SCSI Tutor™, SCSI 
	Bench™ and Drive Light™.

Host Adapters Tested
APA™-348  
APA™-358  
APA™-1460  
AVA™-1505  
AHA®-1510  
AVA™-1515  
AHA®-1520/2  
AHA®-1530/2P  
AHA®-1540/2/F/P  
AHA®-1640  
AHA®-1740/2/4  
AHA®-2740/2/4/T/W  
AHA®-2840/2VL  
AHA®-2920  
AHA®-2940/4/W  
AHA®-2940AU  
AHA®-3940/W  
AHA®-3940U/UW

Adaptec, Inc.
691 S Milpitas Blvd
Milpitas, CA
USA
Phone	1-800-934-2766
Fax	408-262-2533
Toll free	1-800-934-2766
E-mail	sales@adaptec.com
URL	http://www.adaptec.com

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

DATA BACKUP SOLUTIONS	2

Winter, 1996

Adaptec, Inc.

	EASY-CD BACKUP™

	Easy-CD BackUp allows you to backup and archive data to recordable CD.  Drag and drop files from the Windows® File Manager to a "backup
	 List."  Easy CD BackUp supports incremental backup, and always keep previous backups.

Host Adapters Tested
AHA®-1510  
AVA™-1515  
AHA®-1520/2  
AHA®-1530/2P  
AHA®-1540/2/F/P  
AHA®-2740/2/4/T/W  
AHA®-2825VL  
AHA®-2840/2VL  
AHA®-2940/4/W  
AHA®-2940AU

Adaptec, Inc.
691 S Milpitas Blvd
Milpitas, CA
USA
Phone	1-800-934-2766
Fax	408-262-2533
Toll free	1-800-934-2766
E-mail	sales@adaptec.com
URL	http://www.adaptec.com

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

DATA BACKUP SOLUTIONS	3

Winter, 1996

Cactus International, Inc.

	DOS-TAR®

	DOS-TAR® is a fast, UNIX tar compatible, backup and file transfer system.  It is ideal for transferring files from DOS to UNIX, or vice
	 versa.  DOS-TAR® features include master and incremental backups, bit-level verification, support for Fast SCSI Seek devices, error 
	recovery, and speed.  On Fast Seek devices, Dostar can restore a file from the end of a 5 Gig tape in under 25 seconds.  DOS-TAR® can 
	also convert UNIX filenames, pathnames, and ASCII data to DOS, on the fly.  DOS-TAR® as a standalone backup system for MS-DOS is 10 
	times faster than the DOS backup utility.  There are optional Tape Drivers for SCSI and QIC-02 devices.

Host Adapters Tested
AHA®-1510  
AHA®-1520/2  
AHA®-1540/2/F/P  
AHA®-1640  
AHA®-1740/2/4  
AHA®-2740/2/4/T/W

Cactus International, Inc.
13987 West Annapolis Court
Mt. Airy, MD 21771
USA
Phone	(301) 829-1622
Fax	(301) 829-1623
Toll free	(800) 525-UNIX
E-mail	cowboy@cactus.com

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

DATA BACKUP SOLUTIONS	4

Winter, 1996

Cactus International, Inc.

	AIR-BAG

	AIR-BAG reconstructs SCO UNIX and XENIX from hard disk failures. The AIR-BAG will completely recreate all data, partitions, device 
	drivers, kernal link, symbolic links, empty directories and more.  It is fully menu driven and offers an automatic restore mode for the
	 UNIX and XENIX impaired.  The SCO UNIX version allows restoring to a completely different type of hard drive or hard disk controller. 
	 No other crash recovery software on the market is as safe and reliable, or offers as many features.  Twenty-four hour support is 
	available for emergencies.

Host Adapters Tested
AHA®-1510  
AHA®-1520/2  
AHA®-1540/2/F/P  
AHA®-1640  
AHA®-1740/2/4  
AHA®-2740/2/4/T/W

Cactus International, Inc.
13987 West Annapolis Court
Mt. Airy, MD 21771
USA
Phone	(301) 829-1622
Fax	(301) 829-1623
Toll free	(800) 525-UNIX
E-mail	cowboy@cactus.com

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

DATA BACKUP SOLUTIONS	5

Winter, 1996

Cheyenne Software, Inc.

	ARCserve

	The ARCserve family of Products features backup and data management for DOS, Windows, Windows NT, NetWare, and Unix environments.  
	Optional Modules provide protection of open files, mission critical databases, messaging servers and disaster recovery.  ARCserve 
	enables network administrators to provide small, medium, and enterprise-wide backup and restore.  ARCserve can back up and restore DOS,
	 Windows, Windows NT, Windows 95, OS/2, Macintosh and UNIX   
	workstations attached to the server.

Host Adapters Tested
APA™-348  
AVA™-1505  
AHA®-1510  
AVA™-1515  
AHA®-1520/2  
AHA®-1540/2/F/P  
AHA®-1640  
AHA®-1740/2/4  
AHA®-2740/2/4/T/W  
AHA®-2840/2VL  
AHA®-2940/4/W  
AHA®-2940/4/U/UW  
AHA®-3940/W

Cheyenne Software, Inc.
3 Expressway Plaza
Roslyn Heights, NY 11577
Phone	1 800 CHEY-INC
Fax	(516) 484-3446
Toll free	1 800 CHEY-INC
E-mail	webmaster@cheyenne.com
URL	www.cheyenne.com

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

DATA BACKUP SOLUTIONS	6

Winter, 1996

Chi Corporation

	Outright

	OutRight™ SCSI Software Package for NineTrack and 3480, 3490 (IDRC), and 3490E tape drive is designed to reliably expand the data 
	storage and interchange of power PCs. Add the OutRight for DOS or Windows software package to a PC and have a universal interface for 
	data backup, archiving and transfer.  Using the package, PC users have the flexibility to access on-site or off-site IBM, Unisys®, DEC®
	 and numerous other mainframes, mini computers, and PCs.  OutRight for DOS and Windows also supports 4mm, 8mm, and DLT tape drives.

Host Adapters Tested
APA™-348  
APA™-1460  
AVA™-1505  
AHA®-1510  
AVA™-1515  
AHA®-1520/2  
AHA®-1530/2P  
AHA®-1540/2/F/P  
AHA®-1640  
AHA®-1740/2/4  
AHA®-2740/2/4/T/W  
AHA®-2840/2VL  
AHA®-2940/4/W  
AHA®-3940/W

Chi Corporation
31200 Carter Street
Solon, OH 44139
USA
Phone	(216) 349-8605
Fax	(216) 349-8609
Toll free	(800) 828-0599

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

DATA BACKUP SOLUTIONS	7

Winter, 1996

Cirrus Technology, Inc.

	Unite CD-Maker

	Unite® CD-Maker is a 32-bit software package for creating custom CDs.  Unite CD-Maker allows users to quickly and easily make audio CDs
	 as well as create CD-ROMs for backup, archiving and distribution of data.  Included with Unite CD-Maker is a 32-Bit API set for 
	automating the recording process.  Advanced features include multisession support, enhanced CD and mixed mode support and a visual 
	buffer meter to monitor the burn. Many recorders are supported and Windows 95, Windows NT and OS/2 are supported.

Host Adapters Tested
AVA™-1505  
AHA®-1510  
AVA™-1515  
AHA®-1520/2  
AHA®-1530/2P  
AHA®-1540/2/F/P  
AHA®-1640  
AHA®-1740/2/4  
AHA®-2740/2/4/T/W  
AHA®-2825VL  
AHA®-2840/2VL  
AHA®-2910A/Ai  
AHA®-2940/4/W  
AHA®-3940/W  
AHA®-3980/5/W

Cirrus Technology, Inc.
5301 Buckeystown Pike, 4th floor
Frederick, MD 21704
US
Phone	(301)698-1900
Fax	(301)698-1909
E-mail	sales@cirunite.com
URL	http://www.cirunite.com

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

DATA BACKUP SOLUTIONS	8

Winter, 1996

Corel Corporation

	CorelSCSI

	CorelSCSI® software provides easy connection of SCSI devices. CorelSCSI includes device drivers for virtually every SCSI peripheral on 
	the market. CorelSCSI software also includes: Corel CD-Audio, Corel Tape Backup software, SCSI Tools for Windows and more. CorelSCSI is
	 multi-platform, with operating system support for DOS, Windows, OS/2 and Novell® NetWare 386. CorelSCSI is included in Adaptec’s SCSI 
	Direction® Plus kit and SCSI Master™ Plus kit.

Host Adapters Tested
AHA®-1520/2  
AHA®-1540/2/F/P  
AHA®-1640

Corel Corporation
1600 Carling Avenue
Ottawa, Ontario K1Z 8R7
Canada
Phone	(613) 728-8200
Fax	(613) 728-9790
Toll free	(800) 836-7274

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

DATA BACKUP SOLUTIONS	9

Winter, 1996

Corel Corporation

	CorelSCSI Pro

	CorelSCSI Pro® is a high-performance software product designed to maximize SCSI performance.  CorelSCSI Pro provides: support for SCSI 
	scanners to scan images into any TWAIN-compliant graphics program; a CD-ROM server application that allows network users to retrieve 
	recently-accessed information with essentially no delay; and a utility that writes information to a compact disc using a CD-Recorder. 
	These features and others are available using an intuitive and friendly interface.

Host Adapters Tested
AHA®-1520/2  
AHA®-1540/2/F/P  
AHA®-1640

Corel Corporation
1600 Carling Avenue
Ottawa, Ontario K1Z 8R7
Canada
Phone	(613) 728-8200
Fax	(613) 728-9790
Toll free	(800) 836-7274

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

DATA BACKUP SOLUTIONS	10

Winter, 1996

Creative Digital Research

	CDR Publisher

	CDR Publisher is cross-platform and multi-platform desktop CD-ROM recording software that organizes data from the user's computer 
	system and generates CD-ROMs.  With the unique HyCD (tm) capability, CDR Publisher is the only software in the market today that 
	enables the user to develop Hybrid CD-ROMs integrating PC (ISO 9660), Macintosh (HFS) and UNIX (RRIP) formats on a single CD-ROM.

Host Adapters Tested
AHA®-1520/2  
AHA®-1540/2/F/P  
AHA®-2740/2/4/T/W  
AHA®-2825VL  
AHA®-2840/2VL  
AHA®-2940/4/W

Creative Digital Research
7291 Coronado Drive
San Jose, CA 95129
Phone	408-255-0999
Fax	408-255-1011

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

DATA BACKUP SOLUTIONS	11

Winter, 1996

Delphi Data

	TapeBox

	The TapeBox™ series of tape arrays provides a unique hardware solution for medium to large computer systems and networks.  Adaptec 
	controllers are combined with hardware and software to provide a flexible high performance data storage and retrieval system.  
	Configurations include Multi-single drive (with independent IDs), mirroring, cascade, and striping.  Offline tape duplication and 
	testing is also possible.  Our patented concurrent backup can copy data to tape without the need to shut down running applications.  
	All systems include an integrated data cache which greatly improves performance.

Host Adapters Tested
AHA®-1510  
AHA®-1520/2  
AHA®-2740/2/4/T/W  
AHA®-2840/2VL  
AHA®-2940/4/W

Delphi Data
9069 Cajalco Road
Corona, CA 91719
Phone	(909) 279-7955
Fax	(909) 279-7957
Toll free	(800) -DELPHI5
E-mail	76470.1544@compuserve.com

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

DATA BACKUP SOLUTIONS	12

Winter, 1996

Florida Datamation

	SCSItp

	SCSItp™ provides tape support to Adaptec SCSI host adapters for the QNX 4 operating system.  SCSItp supports POSIX utilities such as 
	PAX, TAR, and CP I/O.

Host Adapters Tested
AHA®-1540/2/F/P  
AHA®-1640  
AHA®-1740/2/4

Florida Datamation
AMTEC Center, 6405 Congress Ave, Suite 140
Boca Raton, FL 33487
Phone	(407) 241-2966
Fax	(407) 241-3108
Toll free	(800) 642-5938
E-mail	sales@fdma.com

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

DATA BACKUP SOLUTIONS	13

Winter, 1996

Gazelle Systems

	Back-It

	Gazelle Systems offers Back-It™ and Back-It for Windows backup software for DOS, Windows, NetWare and other NetBIOS networks.  These 
	backup products are remarkably quick, reliable, and user friendly.  Gazelle’s backup products include comprehensive support for a 
	multitude of archival storage devices and tape systems, including:  Alliance, Archive®, Maynard, Teac®, Aiwa, Tecmar, Sankyo, Tandberg,
	 HP®, Insight, Interpreter, Everex, Y-E Data, and many more.

Host Adapters Tested
APA™-348  
APA™-1460  
AHA®-1510  
AHA®-1520/2  
AHA®-1540/2/F/P  
AHA®-1640  
AHA®-1740/2/4  
AHA®-2740/2/4/T/W  
AHA®-2840/2VL

Gazelle Systems
289 E. 950  S
Orem, UT 84058-5004
USA
Phone	(801) 377-1288
Fax	(801) 373-6933
Toll free	(800) 786-3278

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

DATA BACKUP SOLUTIONS	14

Winter, 1996

HCL Hewlett Packard Ltd.

	Busy Bee and Meteor

	The HCL-Hewlett Packard Busy Bee and Meteor Systems are developed in India for use in the Indian market.  They are highly scalable 
	designs starting from home PC low-end configurations to large business UNIX and NetWare servers.

Host Adapters Tested
AHA®-1520/2  
AHA®-1540/2/F/P  
AHA®-1740/2/4  
AHA®-2740/2/4/T/W  
AHA®-2940/4/W  
AHA®-2940/4/U/UW

HCL Hewlett Packard Ltd.
E4, E5, E6 Sector 11, Noida
Dist Ghaziabad,  201301
India
Phone	91-11-8531353
Fax	91-11-8521113

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

DATA BACKUP SOLUTIONS	15

Winter, 1996

Hewlett-Packard Company

	HP SureStore T4i

	The HP SureStore T4i is a 5 1/4", 1/2 height internal drive designed  to integrate easily into HP's NetServer E series, Compaq's 
	ProSignia Series, and other low-end network servers.  
	  
	The product comes complete with the necessary software drivers and mounting hardware for simple set up onto the above mentioned servers
	 running current versions of NetWare and Windows® NT.  
	  
	Key Features:  
	  
	* Network-ready backup solution  
	* 4GB native capacity on a single tape  
	* Travan (TR-4) technology  
	* Includes drivers for NetWare and Windows® NT  
	* Legendary HP service and support

Host Adapters Tested

Hewlett-Packard Company
Computer Peripherals Bristol, Filton Road, Stoke Gifford
Bristol, Avon BS12 6QZ
England
Phone	(44) 117-9228304
Fax	(44)117-9799910
E-mail	adrian_kerton@hp.com
URL	http://www.hp.com/go/dat

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

DATA BACKUP SOLUTIONS	16

Winter, 1996

Hewlett-Packard Company

	HP SureStore DLT40e

	The HP SureStore DLT40e is a digital linear tape drive offering up to 40GB capacity on a single tape, a sustained transfer rate of up 
	to 3MB/s, and outstanding reliability with an 80,000 hour MTBF at 100% duty cycle.  It includes advanced error detection and 
	correction.  The DLT40e is tested for connectivity for most servers, for use on all major operating systems, and with all main backup 
	software.  It also comes with HP's two year Express Exchange Warranty.

Host Adapters Tested
AHA®-2940/4/W  
AHA®-2940/4/U/UW

Hewlett-Packard Company
Computer Peripherals Bristol, Filton Road, Stoke Gifford
Bristol, Avon BS12 6QZ
England
Phone	(44) 117-9228304
Fax	(44)117-9799910
E-mail	adrian_kerton@hp.com
URL	http://www.hp.com/go/dat

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

DATA BACKUP SOLUTIONS	17

Winter, 1996

Hewlett-Packard Company

	HP SureStore DLT30e

	The HP SureStore DLT30e is a digital linear tape drive offering up to 30GB capacity on a single tape, a sustained transfer rate of up 
	to 2.5MB/s, and outstanding reliability with an 80,000 hour MTBF at 100% duty cycle.  It includes advanced error detection and 
	correction.  The DLT30e is tested for connectivity for most servers, for use on all major operating systems, and with all main backup 
	software.  It also comes with HP's two year Express Exchange Warranty.

Host Adapters Tested
AHA®-2940/4/W  
AHA®-2940/4/U/UW

Hewlett-Packard Company
Computer Peripherals Bristol, Filton Road, Stoke Gifford
Bristol, Avon BS12 6QZ
England
Phone	(44) 117-9228304
Fax	(44)117-9799910
E-mail	adrian_kerton@hp.com
URL	http://www.hp.com/go/dat

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

DATA BACKUP SOLUTIONS	18

Winter, 1996

HI-COMP America, Inc.

	HIBACK

	HIBACK® is a backup and archival product designed to support multi-platform, automated backup over the network.  HIBACK supports most 
	UNIX platforms and most peripherals, including optical autochangers and DAT drives.

Host Adapters Tested
AHA®-1510  
AHA®-1520/2

HI-COMP America, Inc.
P.O. Box 22758
Houston, TX 77227-2758
US
Phone	(713) 626-3842
Fax	(713) 626-3654
Toll free	(800) 323-8863

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

DATA BACKUP SOLUTIONS	19

Winter, 1996

Interface Data

	DX-SCSI

	DX-SCSI is a tape drive subsystem for backup and data exchange including interactive, menu-driven software.  It supports character set 
	conversion, fixed and variable length records, various record separators, and several standard tape formats.  It is compatible with 
	most SCSI tape drives and ideal for exchange of tapes with mainframes.

Host Adapters Tested
AHA®-1510  
AHA®-1520/2  
AHA®-1540/2/F/P  
AHA®-1640  
AHA®-1740/2/4

Interface Data
600 West Cummings Park, Suite 3100
Woburn, MA 01801
USA
Phone	(617) 938-6333
Fax	(617) 938-0626
Toll free	(800) 370-3282

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

DATA BACKUP SOLUTIONS	20

Winter, 1996

Kraft Enterprises, Inc.

	AP/SCSI

	The Kraft AP/SCSI software package provides the ability to interface reliable SCSI tape drives to the Advanced Pick/Native operating 
	system. The device driver software supports popular Adaptec® SCSI controllers and many SCSI tape drives. Compatibility with standard 
	Pick tape operations is assured. All Advanced Pick tape functions including file-save, account-save, sel-restore, account-restore, 
	t-verify, t-dump/load and basic tape I/O are supported. QIC compatible SCSI tape drives allow data interchange with QIC-02 tape drives.
	 High capacity 4mm and 8mm tape drives with data compression can provide storage capacities up to 8GB. Backup data rates up to 
	16MB/minute can be achieved with fast systems and tape drives.

Host Adapters Tested
AVA™-1505  
AHA®-1520/2  
AHA®-1540/2/F/P

Kraft Enterprises, Inc.
5200 Char-Mar Lane
Evansville, IN 47720
Phone	(812) 963-5732
Fax	(812) 963-8973

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

DATA BACKUP SOLUTIONS	21

Winter, 1996

Legacy Storage Systems

	Legacy Tape Drives

	Legacy manufactures a complete line of Legacy Tape Drives that can incorporate 8mm Helical-Scan, DAT (Digital Audio Tape) or QIC 
	(Quarter-Inch Cartridge) tape technologies.  All of Legacy’s tape solutions are tested and developed to ensure successful integration 
	with a customer’s primary disk storage.  Some of the family’s many features include:  capacities ranging from 60 MB to over 10 GB; QFA 
	(Quick File Access) capabilities for fast file retrieval; and data transfer rates approaching over 72 MB/minute for Legacy’s higher-end
	 tape family members.  

	  
	  
	Canadian  Corporate Headquarters  
	43 Riviera Drive  
	Markham, Ontario L3R 5J6  
	Canada  
	Tel:  (905)475-1077  
	Fax:  (905)475-1088

Host Adapters Tested
AVA™-1505  
AHA®-1510  
AVA™-1515  
AHA®-1520/2  
AHA®-1530/2P  
AHA®-1540/2/F/P  
AHA®-1640  
AHA®-1740/2/4  
AHA®-2740/2/4/T/W  
AHA®-2840/2VL  
AHA®-2940/4/W

Legacy Storage Systems
138 River Road, Suite 204
Andover, MA 01810
USA
Phone	(508) 681-8400
Fax	(508) 689-9004
Toll free	(800) 966-6442

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

DATA BACKUP SOLUTIONS	22

Winter, 1996

Legato Systems, Inc.

	NetWorker

	NetWorker® is a client/server backup and recovery application, independent of operating system, tape system and network.  Networker 
	supports Novell NetWare, IBM RS/6000 and Sun Sparc servers.  NetWorker supports 4 ClientPaks™.  Client Pak for UNIX support clients for
	 AIX/6000, SunSparc, DEC ULTRIX, HP/UX, SCO UNIX, SGI IRIX and UnixWare.  ClientPak for PC desktops support clients for DOS, Windows®, 
	OS/2 and Windows® NT workstations.  There is also a ClientPak for NetWare and a ClientPak for Windows NT.

Host Adapters Tested
AHA®-1510  
AHA®-1520/2  
AHA®-1540/2/F/P  
AHA®-1640  
AHA®-1740/2/4  
AHA®-2740/2/4/T/W  
AHA®-2840/2VL  
AHA®-2940/4/W

Legato Systems, Inc.
3145 Porter Drive
Palo Alto, CA 94804
US
Phone	(415) 812-6000
Fax	(415) 812-6032
E-mail	sales@legato.com

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

DATA BACKUP SOLUTIONS	23

Winter, 1996

Lone Star Software Corporation

	Lone-Tar

	Lone-Tar® is a reliable back-up software for UNIX.  It has built-in compression that is guaranteed to at least double the capacity of 
	any backup device.  It also includes Intelligent Bit Level Verification that compares every byte of data on your backup to every 
	matching byte of data on your hard disk.  Lone-Tar’s TAPE-TELL monitors every backup and lets you know which tape you are overwriting. 
	 Best of all, Lone-Tar is hardware independent and has a user friendly menu interface that includes source code for the UNIX impaired.

Host Adapters Tested
AHA®-1510  
AHA®-1520/2  
AHA®-1540/2/F/P  
AHA®-1640  
AHA®-1740/2/4  
AHA®-2740/2/4/T/W

Lone Star Software Corporation
13987 West Annapolis Court
Mt. Airy, MD 21771
USA
Phone	(301) 829-1622
Fax	(301) 829-1623
Toll free	(800) LONETAR
E-mail	cowboy@cactus.com

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

DATA BACKUP SOLUTIONS	24

Winter, 1996

Lookout Geophysical Company

	SeiScope/SeaScope

	Subsurface geo-technical images (Seismic, sonar, ground penetrating radar, etc.) are processed and displayed in real time and written 
	to SCSI tape drives (4mm, 8mm, DLT, 3480) and processed from tape after acquisition.

Host Adapters Tested
AHA®-1520/2  
AHA®-1540/2/F/P  
AHA®-2940/4/W  
AHA®-2940/4/U/UW

Lookout Geophysical Company
433 Park Point Drive, Suite 250
Golden, CO 80401
USA
Phone	303-526-5108
Fax	303-526-5150
E-mail	vgoebel@aol.com

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

DATA BACKUP SOLUTIONS	25

Winter, 1996

Maxoptix Corporation

	T4-2600

	The T4-2600 is a new 5.25" multifunction optical disk drive with 2.6GB capacity.  It provides unlimited transportable storage at an 
	excellent value, offering unparalleled reliability, a fast seek rate up to 4.0 MB/second transfer rate and with 1 read/write cache, it 
	delivers an outstanding performance.  The T4-2600 drive conforms to ISO specifications and accepts three ISO standard media formats - 
	2.6GB, 1.3GB and 650MB.  
	This drive is reliable, affordable and high performance.  The media can be written and erased more than 10,000,000 times.

Host Adapters Tested
AHA®-1540/2/F/P  
AHA®-1640  
AHA®-1740/2/4  
AHA®-2740/2/4/T/W  
AHA®-2940/4/W  
AHA®-3940/W

Maxoptix Corporation
3342 Gateway Blvd.
Fremont, CA 94538
USA
Phone	(510) 353-9700
Fax	(510) 353-1845
Toll free	(800) 848-3092

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

DATA BACKUP SOLUTIONS	26

Winter, 1996

Maxoptix Corporation

	MaxLyb

	The Maxoptix MaxLyb family of optical auto changers utilizes the T4-2600 drives to deliver high performance and reliable 
	specifications.  The MaxLyb family covers a wide range of capacities - 26GB to over 600GB, which ensures the most useful library is 
	available for a variety of applications.  
	  
	With the MaxLyb family of optical storage libraries, Maxoptix offers the widest selection of optical library solutions and fills the 
	price-performance gaps left by other storage technologies.  With the fastest on-line access to stored data and information, they are 
	the logical choice for those who need top performance, demonstrated reliability and future expandability at competitive prices.

Host Adapters Tested
AHA®-1540/2/F/P  
AHA®-1640  
AHA®-1740/2/4  
AHA®-2740/2/4/T/W  
AHA®-2940/4/W  
AHA®-3940/W

Maxoptix Corporation
3342 Gateway Blvd.
Fremont, CA 94538
USA
Phone	(510) 353-9700
Fax	(510) 353-1845
Toll free	(800) 848-3092

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

DATA BACKUP SOLUTIONS	27

Winter, 1996

MicroText Systems Inc.

	DOSTAR

	DOSTAR offers a comprehensive backup/restore solution for DOS-based PCs.  Rather than a proprietary format, DOSTAR uses the “tar” 
	format, a standard for years on all UNIX systems.  This product provides full, bi-directional compatibility between MS-DOS® and 
	virtually any UNIX or XENIX® system.  Versions are available for SCSI tapes, QIC-02 and QIC-36 tapes, and floppy diskettes of over 40 
	different types.

Host Adapters Tested
AHA®-1520/2  
AHA®-1540/2/F/P  
AHA®-2740/2/4/T/W  
AHA®-2825VL  
AHA®-2840/2VL  
AHA®-2940/4/W  
AHA®-2940/4/U/UW  
AHA®-2940AU  
AHA®-3940/W  
AHA®-3940U/UW  
AHA®-3980/5/W

MicroText Systems Inc.
507 Corbin Court
Mississauga, Ontario L5A 1M2
Canada
Phone	(905) 276-1257
Fax	(905) 276-7236
E-mail	sales@msitxt.gts.org

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

DATA BACKUP SOLUTIONS	28

Winter, 1996

Mountain Network Solutions, Inc.

	Mountain FileSafe for Windows

Host Adapters Tested
AHA®-1510  
AHA®-1520/2  
AHA®-1530/2P  
AHA®-1540/2/F/P  
AHA®-1640  
AHA®-1740/2/4

Mountain Network Solutions, Inc.
11205 Knott Ave, STE D
Cypress, CA 90630-5489
Phone	(408) 438-6650
Fax	(408) 438-7623
Toll free	(800) 458-0300

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

DATA BACKUP SOLUTIONS	29

Winter, 1996

NCE Storage Solutions (Emerald Systems)

	Emerald Systems Xpress Librarian

	Emerald Systems products are now sold through NCE Storage Solutions.  Xpress Librarian™ is a fully automated workstation-based, restore
	 and data storage management application for use with NetWare 2.x, 3.1x or 4.1x. It supports both Windows and Windows for Workgroups 
	and LANtastic. Xpress Librarian is easy to install and easy to customize. Restoration of files is quick and easy. Key features include:
	 disk grooming with file aging/usage reports; support for full, incremental and differential backups; support for a broad range of 
	popular backup devices; and optional peer-to-peer and AutoLoader modules.

Host Adapters Tested
AHA®-1510  
AHA®-1520/2  
AHA®-1540/2/F/P  
AHA®-1640  
AHA®-1740/2/4  
AHA®-2740/2/4/T/W  
AHA®-2840/2VL  
AHA®-2940/4/W

NCE Storage Solutions (Emerald Systems)
9717 Pacific Heights Blvd.
San Diego, CA 92121
USA
Phone	(619) 452-7974
Fax	(619) 673-2288
Toll free	(800) 767-2587

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

DATA BACKUP SOLUTIONS	30

Winter, 1996

NCE Storage Solutions (Emerald Systems)

	Emerald Systems EmSAVE

	EmSAVE™ is a workstation-based backup and restore software product and is now sold through NCE Storage Solutions.  The ideal choice for
	 small to mid-range Novell NetWare 2.x, 3.1x or 4.0x networks, it is easy to learn and use.  It has a Windows interface and also 
	supports Microsoft’s® Windows for Workgroups.  Key features include:  support for full, incremental and differential backups; scheduled
	 unattended backups;  daisy-chain for added capacity; editable batch files; and support for a broad range of popular backup devices.

Host Adapters Tested
AHA®-1510  
AHA®-1520/2  
AHA®-1540/2/F/P  
AHA®-1640  
AHA®-1740/2/4  
AHA®-2740/2/4/T/W  
AHA®-2840/2VL  
AHA®-2940/4/W  
AHA®-2940/4/U/UW

NCE Storage Solutions (Emerald Systems)
9717 Pacific Heights Blvd.
San Diego, CA 92121
USA
Phone	(619) 452-7974
Fax	(619) 673-2288
Toll free	(800) 767-2587

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

DATA BACKUP SOLUTIONS	31

Winter, 1996

NCE Storage Solutions (Emerald Systems)

	Mountain FileSafe for Windows

	Mountain FILESAFE products are now sold through NCE Storage Solutions.  This Windows®-based network data management software features 
	Mountain Rescue.  It supports all NetWare 2.x and 3.1x networks.  Key features include: data management capabilities through automated 
	tape rotation schemes, a librarian to track all backups and file occurrences, and Rescue, an innovative disaster recovery feature that 
	monitors user-selected volumes and provides a quick, easy-to-use method for recovery of data.

Host Adapters Tested
AHA®-1510  
AHA®-1520/2  
AHA®-1530/2P  
AHA®-1540/2/F/P  
AHA®-1640  
AHA®-1740/2/4

NCE Storage Solutions (Emerald Systems)
9717 Pacific Heights Blvd.
San Diego, CA 92121
USA
Phone	(619) 452-7974
Fax	(619) 673-2288
Toll free	(800) 767-2587

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

DATA BACKUP SOLUTIONS	32

Winter, 1996

NovaStor Corporation

	NovaBack for Windows 95”

	A powerful all purpose data protection utility for your PC, workstation or network.  NovaBack for Windows 95 offers a wide range of 
	high-end features including the backup of Windows 95 registry data, long file names and more.  NovaBack offers a true 32-bit mode that 
	supports over 300 different types of tape drives, including all SCSI drives 1/4", 4mm, 8mm, DLT, and 1/2", and QIC Travan, 3010, 3020 
	and QIC 80.

Host Adapters Tested
APA™-348  
AVA™-1505  
AHA®-1510  
AVA™-1515  
AHA®-1520/2  
AHA®-1530/2P  
AHA®-1540/2/F/P  
AHA®-1640  
AHA®-1740/2/4  
AHA®-2740/2/4/T/W  
AHA®-2840/2VL  
AHA®-2940/4/W  
AHA®-3940/W

NovaStor Corporation
80-B West Cochran Street
Simi Valley, CA 93065
Phone	(805) 579-6700
Fax	(805) 579-6710

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

DATA BACKUP SOLUTIONS	33

Winter, 1996

NovaStor Corporation

	NovaBack

	A powerful all purpose data protection utility for your PC, workstation or network.  NovaBack for Windows NT” offers a wide range of 
	high-end features including the backup of Windows NT” registry data, Windows NTAS servers, long file names and more.  NovaBack offers a
	 true 32-bit mode that supports over 300 different types of tape drives, including all SCSI drives 1/4", 4mm, 8mm, DLT, and 1/2".

Host Adapters Tested
APA™-348  
AVA™-1505  
AHA®-1510  
AVA™-1515  
AHA®-1520/2  
AHA®-1530/2P  
AHA®-1540/2/F/P  
AHA®-1640  
AHA®-1740/2/4  
AHA®-2740/2/4/T/W  
AHA®-2840/2VL  
AHA®-2940/4/W  
AHA®-3940/W

NovaStor Corporation
80-B West Cochran Street
Simi Valley, CA 93065
Phone	(805) 579-6700
Fax	(805) 579-6710

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

DATA BACKUP SOLUTIONS	34

Winter, 1996

NovaStor Corporation

	NovaNet

	NovaNet-NLM for Novell Netware provides backuup and restore for your 3.XX, or 4.XX Novell Netware fileserver and DOS, OS/2, Windows and
	 Macintosh workstations.  It is a true SMS and client/server application that allows any user on the network to initiate a backup or 
	restore procedure that runs in the background.  NovaNet-NLM archives data to any SCSI tape unit, or autoloaders.

Host Adapters Tested
APA™-348  
AVA™-1505  
AHA®-1510  
AVA™-1515  
AHA®-1520/2  
AHA®-1530/2P  
AHA®-1540/2/F/P  
AHA®-1640  
AHA®-1740/2/4  
AHA®-2740/2/4/T/W  
AHA®-2840/2VL  
AHA®-2940/4/W  
AHA®-3940/W

NovaStor Corporation
80-B West Cochran Street
Simi Valley, CA 93065
Phone	(805) 579-6700
Fax	(805) 579-6710

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

DATA BACKUP SOLUTIONS	35

Winter, 1996

NovaStor Corporation

	NovaBack

	NovaBack for OS/2 provides backup and restore for your OS/2 based PC.  NovaBack for OS/2 provides support for HPFS and FAT file systems
	 including all extended attributes and long file names.  If your PC is a workstation for Novell or LanManager, NovaBack will allow you 
	to easily backup your file server as well as the workstation.  NovaBack for OS/2 supports both 1.3, 2.xx, and 3.xx versions of OS/2.  
	NovaBack for OS/2 archives data to any SCSI, autoloader, QIC-80, QIC-3010-20, or Travan tape drives.  NovaBack for OS/2 is available in
	 a Presentation Manager and a Character Based Interface.

Host Adapters Tested
APA™-348  
AVA™-1505  
AHA®-1510  
AVA™-1515  
AHA®-1520/2  
AHA®-1530/2P  
AHA®-1540/2/F/P  
AHA®-1640  
AHA®-1740/2/4  
AHA®-2740/2/4/T/W  
AHA®-2840/2VL  
AHA®-2940/4/W  
AHA®-3940/W

NovaStor Corporation
80-B West Cochran Street
Simi Valley, CA 93065
Phone	(805) 579-6700
Fax	(805) 579-6710

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

DATA BACKUP SOLUTIONS	36

Winter, 1996

NovaStor Corporation

	NovaBack

	NovaBack for Windows provides backup and restore for your Windows based PC.  If your PC is a workstation for Novell, Lantastic, Windows
	 for Workgroups, or Banyan network, NovaBack will allow you to easily backup your file server as well as the workstation.  NovaBack for
	 Windows archives data to any SCSI, autoloader, QIC-80, QIC-3010/20, or Travan tape drives.

Host Adapters Tested
AVA™-1505  
AHA®-1510  
AVA™-1515  
AHA®-1520/2  
AHA®-1530/2P  
AHA®-1540/2/F/P  
AHA®-1640  
AHA®-1740/2/4  
AHA®-2740/2/4/T/W  
AHA®-2840/2VL  
AHA®-2940/4/W  
AHA®-2940/4/U/UW

NovaStor Corporation
80-B West Cochran Street
Simi Valley, CA 93065
Phone	(805) 579-6700
Fax	(805) 579-6710

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

DATA BACKUP SOLUTIONS	37

Winter, 1996

NovaStor Corporation

	NovaMac

	NovaMac for Macintosh is backup and restore software for your Macintosh.  If your Mac is a workstation for Novell, Appleshare, 
	Appletalk, Tokentalk and Ethertalk network, NovaMac will allow you to easily backup your fileserver as well as the workstations.

Host Adapters Tested
APA™-348  
AVA™-1505  
AHA®-1510  
AVA™-1515  
AHA®-1520/2  
AHA®-1530/2P  
AHA®-1540/2/F/P  
AHA®-1640  
AHA®-1740/2/4  
AHA®-2740/2/4/T/W  
AHA®-2840/2VL  
AHA®-2940/4/W  
AHA®-3940/W

NovaStor Corporation
80-B West Cochran Street
Simi Valley, CA 93065
Phone	(805) 579-6700
Fax	(805) 579-6710

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

DATA BACKUP SOLUTIONS	38

Winter, 1996

NovaStor Corporation

	NovaBack

	NovaBack for DOS provides backup and restore for your MS DOS based PC.  If your PC is a workstation for Novell, Lantastic, Windows for 
	Workgroups, or Banyan network, NovaBack will allow you to easily backup your fileserver as well as the workstation.  NovaBack for DOS 
	archives data to any SCSI tape unit, as well as autoloaders.

Host Adapters Tested
APA™-348  
AVA™-1505  
AHA®-1510  
AVA™-1515  
AHA®-1520/2  
AHA®-1530/2P  
AHA®-1540/2/F/P  
AHA®-1640  
AHA®-1740/2/4  
AHA®-2740/2/4/T/W  
AHA®-2840/2VL  
AHA®-2940/4/W  
AHA®-2940/4/U/UW  
AHA®-3940/W

NovaStor Corporation
80-B West Cochran Street
Simi Valley, CA 93065
Phone	(805) 579-6700
Fax	(805) 579-6710

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

DATA BACKUP SOLUTIONS	39

Winter, 1996

PCX

	BakupWiz

	BakupWiz™ quickly and reliably backs up your local and networked drives to SCSI tape from a DOS or OS/2 platform.  It is very flexible:
	 it can back up all files, any files you select, or any files that have changed since a specified date and time.  Novell NetWare and 
	any NetBIOS-compatible networks are supported.  Under NetWare, BakupWiz will back up and restore both file and network security 
	information without sacrificing speed, and the network file server may be backed up while users are still logged onto the system.  
	NetWare 286 and 386 as well as Apple® File Protocol are supported.

Host Adapters Tested
APA™-348  
APA™-358  
APA™-1460  
AVA™-1505  
AHA®-1510  
AVA™-1515  
AHA®-1520/2  
AHA®-1530/2P  
AHA®-1540/2/F/P  
AHA®-1640  
AHA®-1740/2/4  
AHA®-2740/2/4/T/W  
AHA®-2840/2VL  
AHA®-2940/4/W  
AHA®-3940/W

PCX
4874 Alberson Court
San Diego, CA 92130
Phone	(619) 259-6300
Fax	(619) 481-6474
Toll free	(800) 800-4PCX
E-mail	support@pcx.com

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

DATA BACKUP SOLUTIONS	40

Winter, 1996

Performance Technology

	POWERsave

	POWERsave™ 3.2 for Banyan® backs up all Vines® file services, supports Vines 5.5 for extended directory-level and file-level ARLs, 
	supports all StreetTalk associated records and automatically recreates lost services and groups when restoring the StreetTalk database.
	  It has up to twice the workstation performance with NetBIOS replacement and no need to configure Banyan NetBIOS.    
	  
	POWERsave 4.0 for NetWare automatically backs up all bindery and trustee files from a Windows® workstation; supports extended file 
	attributes, Macintosh files, NDS support, and last access date; allows a named user, other than the supervisor, to do the backup; and 
	updates last archived date.  
	  
	POWERsave 4.0 for POWERLan™ (now with support for Windows) and LANtastic 3.2 are complete backup and restore solutions for POWERLan and
	 LANtastic networks.

Host Adapters Tested
AHA®-1510  
AHA®-1520/2  
AHA®-1540/2/F/P  
AHA®-1640  
AHA®-1740/2/4

Performance Technology
7800 IH 10 West, Suite 800
San Antonio, TX 78230
US
Phone	(210) 979-2000
Fax	(210) 979-2002
Toll free	(800) FAST-LAN

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

DATA BACKUP SOLUTIONS	41

Winter, 1996

Pioneer Hi-Fi (GB) Ltd.

	PIONEER

	Pioneer, the leading manufacturer of optical disc technology has developed a solution utilizing it's high storage CD-ROM autochanger.  
	This solution provides stored video clips directly to designated PC's.  The Video Browse Server enables users to view the whole of a 
	video library on a PC.  This application has a user friendly and logical GUI.  The video clips never physically leave the library, 
	hence no time lost tracing material.  All of the video is held on CD-ROMs locked away in a 500 disk autochanger.  Initially by the use 
	of alphanumeric entries a search can be narrowed down to several titles. A selected title gives further indexed information on the clip
	 and also more importantly at least two thumbnails.  The chosen clip can then be viewed on a PC terminal.  By selecting various clips 
	the user automatically generates a clip list.  This file can then be sent to the compiling station on the network.  The compiling 
	station then assembles the request on any chosen broadcast medium- D1, D2, D3, D5, Digital Betacam, Betacam, Disc etc.

Host Adapters Tested
AHA®-2940/4/U/UW  
AHA®-3940/W  
AHA®-3940U/UW

Pioneer Hi-Fi (GB) Ltd.
Pioneer House, Hollybush Hill
Stoke Poges, Slough SL2 4QP
England
Phone	144-01753-789732
Fax	144-01753-789539

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

DATA BACKUP SOLUTIONS	42

Winter, 1996

Pixelab, Inc.

	DATMAN

	DATMAN™ is a revolutionary DAT control software which provides an MS-DOS compatible file system with up to 8-GB and a quarter million 
	files.  Unlike typical tape backup programs, most MS-DOS and Windows applications can directly read and write files on the tape.  
	DATMAN makes the DAT drive operate very much like the familiar floppy drive.  Once it is installed, it is extremely easy to use.  Also,
	 it removes the common access bottleneck to the huge online storage.  With the sophisticated adaptive cache algorithm, DATMAN provides 
	high-performance file access.

Host Adapters Tested
APA™-358  
APA™-1460  
AVA™-1505  
AHA®-1510  
AVA™-1515  
AHA®-1520/2  
AHA®-1530/2P  
AHA®-1540/2/F/P

Pixelab, Inc.
1212 S. Naper Blvd.  Ste. #119
Naperville, IL 60540
Phone	(708) 369-7112
Fax	(708) 369-7113
E-mail	sales@datman.com
URL	http://www.datman.com

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

DATA BACKUP SOLUTIONS	43

Winter, 1996

Seagate Software, Storage Management Group

	Network Archivist

	Palindrome’s NetWare Archivist™, available on workstation or file server platforms, provides a comprehensive approach to intelligently 
	automate the data protection process.  LAN storage management functions include determining how and when data is backed up, archiving, 
	disaster recovery and file server grooming.  Software is sold separately or combined with tape drives with capacities ranging from 
	250MB to 50GB.

Host Adapters Tested
APA™-358  
APA™-1460  
AHA®-1510  
AHA®-1520/2  
AHA®-1540/2/F/P  
AHA®-1640  
AHA®-1740/2/4  
AHA®-2740/2/4/T/W  
AHA®-2940/4/W

Seagate Software, Storage Management Group
(formerly Palindrome Corp.), 600 East Diehl Road
Naperville, IL 60563
Phone	(708) 505-3300
Fax	(708) 505-7917
Toll free	(800) 288-4912
E-mail	sales@palindrome.com

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

DATA BACKUP SOLUTIONS	44

Winter, 1996

Seagate Software, Storage Management Group

	Backup Exec

	The Arcada Backup Exec family of products includes tape backup software for DOS, Windows, Windows for Workgroups, Windows NT, NetWare® 
	and OS/2®. Arcada Backup Exec supports all popular SCSI tape drives, along with the DC2000 mini-cartridge drives. Some important 
	features of Arcada Backup Exec include automatic/unattended backup, disk grooming, cataloging, fast file access and much more.

Host Adapters Tested
AVA™-1505  
AHA®-1510  
AVA™-1515  
AHA®-1520/2  
AHA®-1530/2P  
AHA®-1540/2/F/P  
AHA®-1640  
AHA®-1740/2/4  
AHA®-2740/2/4/T/W  
AHA®-2825VL  
AHA®-2840/2VL  
AHA®-2940/4/W

Seagate Software, Storage Management Group
(formerly Arcada Software), 37 Skyline Drive, Suite 1101
Lake Mary, FL 32746
Phone	(800) 327-2232
Fax	(407) 333-7730
Toll free	(800) 327-2232
E-mail	sales@arcada.com

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

DATA BACKUP SOLUTIONS	45

Winter, 1996

Seagate Software, Storage Management Group

	Palindrome Backup Director

	Palindrome™ Backup Director is the complete backup and restore software for any size LAN.  Backup Director provides everything you need
	 to protect your Netware software, applications, and data safely and reliably.  The software includes proactive alerting and 
	error-correction systems.  Backup Director's scalable performance, up to 700 Mb per minute, gives you the fastest, most automated and 
	reliable backup possible.  Backup Director supports the widest array of backup devices and platforms and gives you the flexibility to 
	customize your own backup schedule or use a predefined media rotation scheme.  With the unique Windows® Control Console Interface, you 
	can monitor all operations and complete tasks with a few simple mouse clicks.  Palindrome File Manager makes it easy and safe for users
	 to restore their own files ensuring full network security is maintained.  For restoring entire servers, Backup Director helps you 
	create a recovery diskette that automates the process, and eliminates the need to fully reinstall NetWare or Backup Director.  Native 
	NetWare Directory Services (NDS) and full SMS compliance makes it the best backup for both Netware 4.x and 3.x users.

Host Adapters Tested
APA™-358  
APA™-1460  
AHA®-1510  
AHA®-1520/2  
AHA®-1540/2/F/P  
AHA®-1640  
AHA®-1740/2/4  
AHA®-2740/2/4/T/W  
AHA®-2940/4/W

Seagate Software, Storage Management Group
(formerly Palindrome Corp.), 600 East Diehl Road
Naperville, IL 60563
Phone	(708) 505-3300
Fax	(708) 505-7917
Toll free	(800) 288-4912
E-mail	sales@palindrome.com

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

DATA BACKUP SOLUTIONS	46

Winter, 1996

Seagate Software, Storage Management Group

	Palindrome Storage Manager

	Palindrome™ Storage Manager is the integrated backup, archiving and HSM software for growing networks.  Built on the powerful backup 
	and restore capabilities found in Palindrome Backup Director, Storage Manager delivers powerful capacity management features, including
	 migration, file tracking and retrieval, archiving and Heirarchical Storage Management (HSM).  Storage Manager lets you take a 
	step-by-step approach to capacity management based on your needs and resources.  You can start by migrating files manually, then move 
	to scheduled migration schemes that automate the process for you and ensures disc space availability.  By moving to continuous disc 
	monitoring with event-triggered, real-time migration and recall, you have a full HSM system that optimizes your administrative 
	resources and hardware investment.

Host Adapters Tested
APA™-358  
APA™-1460  
AHA®-1510  
AHA®-1520/2  
AHA®-1540/2/F/P  
AHA®-1640  
AHA®-1740/2/4  
AHA®-2740/2/4/T/W  
AHA®-2940/4/W

Seagate Software, Storage Management Group
(formerly Palindrome Corp.), 600 East Diehl Road
Naperville, IL 60563
Phone	(708) 505-3300
Fax	(708) 505-7917
Toll free	(800) 288-4912
E-mail	sales@palindrome.com

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

DATA BACKUP SOLUTIONS	47

Winter, 1996

Seagate Software, Storage Management Group

	SYTOS PREMIUM

	Sytos Premium is a high performance backup and disaster recovery software offering complete OS/2 workstation and network server 
	protection.  For standalone workstations or network servers running LAN Server.  Sytos Premium offers the most flexibility, reliability
	 and performance without compromising ease of use.  Complete system protection is provided by a disaster recovery utility.  Should your
	 hard disk become corrupt, Sytos Premium reinstalls OS/2 and performs a restore from the last full backup automatically, restoring your
	 system within minutes.  Includes extensive QIC, SCSI and minicartridge support.

Host Adapters Tested
AVA™-1505  
AHA®-1510  
AVA™-1515  
AHA®-1520/2  
AHA®-1540/2/F/P  
AHA®-1640  
AHA®-1740/2/4  
AHA®-2740/2/4/T/W  
AHA®-2840/2VL  
AHA®-2940/4/W

Seagate Software, Storage Management Group
(formerly Arcada Software), 37 Skyline Drive, Suite 1101
Lake Mary, FL 32746
Phone	(800) 327-2232
Fax	(407) 333-7730
Toll free	(800) 327-2232
E-mail	sales@arcada.com

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

DATA BACKUP SOLUTIONS	48

Winter, 1996

Seagate Software, Storage Management Group

	SYTOS AUTOLOADER

	Sytos Autoloader is a device support utility for multiple tape backup devices attached to OS/2 workstations or servers including IBM 
	LAN Server and Microsoft LAN Manager.  As an add-on support module for Sytos Premium, Sytos Autoloader automates the backup process for
	 autoloaders, and gives you the flexibility to configure your device as a single backup device or as a set of backup devices.  With 
	Sytos Autoloader, you can run large multi-tape backups or several smaller backups without user intervention.  The software 
	automatically selects tapes, changes tapes and runs scheduled operations completely unattended.

Host Adapters Tested
AVA™-1505  
AHA®-1510  
AVA™-1515  
AHA®-1520/2  
AHA®-1540/2/F/P  
AHA®-1640  
AHA®-1740/2/4  
AHA®-2740/2/4/T/W  
AHA®-2840/2VL  
AHA®-2940/4/W

Seagate Software, Storage Management Group
(formerly Arcada Software), 37 Skyline Drive, Suite 1101
Lake Mary, FL 32746
Phone	(800) 327-2232
Fax	(407) 333-7730
Toll free	(800) 327-2232
E-mail	sales@arcada.com

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

DATA BACKUP SOLUTIONS	49

Winter, 1996

Software 2000

	Print Magic

	Print Magic™ is a high-speed, high-quality printing system for Microsoft Windows 3.x and Windows 95. It is available to OEMs for use 
	with SCSI and non-SCSI printer peripherals. The product supports both the ASPI and Adaptec EZ-SCSI interface to color printers (dye 
	sub, inkjet and thermal wax transfer). Print Magic™ is easily customizable and quick to develop advanced drivers. Diffusion printing, 
	CMY, CMYK, 24-bit color, bi-di and color match options are all standard.

Host Adapters Tested
AHA®-1510  
AHA®-1530/2P  
AHA®-1640  
AHA®-1740/2/4

Software 2000
The Magdalen Centre, Oxford Science Park
Oxford, Oxon,  OX4 4GA
England
Phone	44-0-865-784200
Fax	44-0-865-784201

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

DATA BACKUP SOLUTIONS	50

Winter, 1996

Symantec-Peter Norton Product Group

	Norton Backup™ v3.0 for Windows

	The Norton Backup 3.0 for Windows backs up your files quickly, reliably and painlessly.  Norton Backup can even restore data from 
	damaged backup disks that other products can’t.  Norton Backup provides different interfaces for various levels of use: Step-by-Step 
	for basic fool-proof backup and Advanced for more sophisticated users.  Plus, Norton Backup offers true compatibility as well as major 
	advantages not found in DOS 6.0.

Host Adapters Tested
AHA®-1520/2  
AHA®-1540/2/F/P  
AHA®-1640  
AHA®-1740/2/4  
AHA®-2740/2/4/T/W

Symantec-Peter Norton Product Group
2500 Broadway, Suite 200
Santa Monica, CA 90404
Phone	(310) 453-4600
Fax	(310) 829-1028

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

DATA BACKUP SOLUTIONS	51

Winter, 1996

Systems Axis plc

	Stream

	Stream release 3.1 tape backup software is designed to backup single user and multi user systems quickly and reliably.  The software 
	supports Fast SCSI-2 DDS2 DAT drives as well as DC6000 SCSI drives, allowing backup speeds of up to 60MB/minute with data compression. 
	 Features of  Stream include:  unattended backup; backup log; ability to backup local or network drives; wide range of Adaptec® SCSI 
	controllers supported; ASPI drivers used to communicate with the SCSI controller and drive allowing large block transfers at the 
	maximum possible rate; support for tape drives from 250MB to 8GB.

Host Adapters Tested
APA™-358  
AVA™-1505  
AHA®-1510  
AHA®-1540/2/F/P  
AHA®-1640  
AHA®-1740/2/4  
AHA®-2740/2/4/T/W  
AHA®-2940/4/W  
AHA®-2940/4/U/UW

Systems Axis plc
53/55 St. Mary Street
Bridgewater, Somerset,  TA6  3EQ
UK
Phone	(44) 278-422-219
Fax	(44) 278-451-198

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

DATA BACKUP SOLUTIONS	52

Winter, 1996

Systems Enhancement Corporation

	Total Network® Recall

	Total Network Recall (TNR) is a 100% Novell SMS-compatible tape back up software package.  The product features a server-based NLM; 
	multiple auto backup sessions; and support of all Novell TSAs. TNR supports NetWare 3.1x and 4.0x. Additional features include 
	compatibility with Powermon software, built-in batch file scheduler and autochanger support.

Host Adapters Tested
AHA®-1510  
AHA®-1520/2  
AHA®-1540/2/F/P  
AHA®-1640  
AHA®-1740/2/4

Systems Enhancement Corporation
174 Chesterfield Industrial Blvd
Chesterfield, MO 63005
USA
Phone	(314) 532-2855
Fax	(314) 532-2037

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

DATA BACKUP SOLUTIONS	53

Winter, 1996

Tandberg Data S.A.

	Tape Storage Solutions: Panther

	The Panther Family of tape backup systems offers a full range of backup solutions from 250 MB up to 13/26 GB.  The Panther Family 
	provides turnkey solutions for all major OS and network environments with industry leaders such as Adaptec®, Arcada, Cheyenne, JMR,  
	3M, and Sony.

Host Adapters Tested
APA™-348  
APA™-358  
APA™-1460  
AVA™-1505  
AHA®-1510  
AVA™-1515  
AHA®-1520/2  
AHA®-1530/2P  
AHA®-1540/2/F/P  
AHA®-1640  
AHA®-1740/2/4  
AHA®-2740/2/4/T/W  
AHA®-2840/2VL  
AHA®-2940/4/W

Tandberg Data S.A.
16-18 Avenue Morane Saulnier, Bat A
F-78941 Velizy,
France
Phone	33-1-39260101
Fax	33-1-34650289
URL	www.tandberg.com

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

DATA BACKUP SOLUTIONS	54

Winter, 1996

Tandberg Data S.A.

	Streaming Tape Drives

	Tandberg Data DC600 and mini cartridges QIC tape drives are the ultimate choice for hard disk backup, archival storage and data 
	interchange for PC, workstation and mid-range computer.

Host Adapters Tested
APA™-348  
APA™-358  
APA™-1460  
AVA™-1505  
AHA®-1510  
AVA™-1515  
AHA®-1520/2  
AHA®-1530/2P  
AHA®-1540/2/F/P  
AHA®-1640  
AHA®-1740/2/4  
AHA®-2740/2/4/T/W  
AHA®-2825VL  
AHA®-2840/2VL  
AHA®-2940/4/U/UW  
AHA®-3940/W  
AHA®-3980/5/W

Tandberg Data S.A.
16-18 Avenue Morane Saulnier, Bat A
F-78941 Velizy,
France
Phone	33-1-39260101
Fax	33-1-34650289
URL	www.tandberg.com

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

DATA BACKUP SOLUTIONS	55

Winter, 1996

Tandberg Data S.A.

	Panther 250 (TDC 3660)

	Tandberg data tape drives series offers one of the most affordable backup choices for Power PC and LAN users.  Low cost per megabyte 
	coupled with significant growth potential provide outstanding backup value.

Host Adapters Tested
APA™-348  
APA™-358  
APA™-1460  
AVA™-1505  
AHA®-1510  
AVA™-1515  
AHA®-1520/2  
AHA®-1530/2P  
AHA®-1540/2/F/P  
AHA®-1640  
AHA®-1740/2/4  
AHA®-2740/2/4/T/W  
AHA®-2825VL  
AHA®-2840/2VL  
AHA®-2940/4/W  
AHA®-2940W MAC  
AHA®-3940/W  
AHA®-3980/5/W

Tandberg Data S.A.
16-18 Avenue Morane Saulnier, Bat A
F-78941 Velizy,
France
Phone	33-1-39260101
Fax	33-1-34650289
URL	www.tandberg.com

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

DATA BACKUP SOLUTIONS	56

Winter, 1996

Tandberg Data S.A.

	Panther 525 (TDC 3820)

	Tandberg data tape drives series offers one of the most affordable backup choices for Power PC and LAN users.  Low cost per megabyte 
	coupled with significant growth potential provide outstanding backup value.

Host Adapters Tested
APA™-348  
APA™-358  
APA™-1460  
AVA™-1505  
AHA®-1510  
AVA™-1515  
AHA®-1520/2  
AHA®-1530/2P  
AHA®-1540/2/F/P  
AHA®-1640  
AHA®-1740/2/4  
AHA®-2740/2/4/T/W  
AHA®-2825VL  
AHA®-2840/2VL  
AHA®-2940/4/W  
AHA®-2940W MAC  
AHA®-3940/W  
AHA®-3980/5/W

Tandberg Data S.A.
16-18 Avenue Morane Saulnier, Bat A
F-78941 Velizy,
France
Phone	33-1-39260101
Fax	33-1-34650289
URL	www.tandberg.com

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

DATA BACKUP SOLUTIONS	57

Winter, 1996

Tandberg Data S.A.

	Panther 1200 (TDC 4120)

	Tandberg data tape drives series offers one of the most affordable backup choices for Power PC and LAN users.  Low cost per megabyte 
	coupled with significant growth potential provide outstanding backup value.

Host Adapters Tested
APA™-348  
APA™-358  
APA™-1460  
AVA™-1505  
AHA®-1510  
AVA™-1515  
AHA®-1520/2  
AHA®-1530/2P  
AHA®-1540/2/F/P  
AHA®-1640  
AHA®-1740/2/4  
AHA®-2740/2/4/T/W  
AHA®-2825VL  
AHA®-2840/2VL  
AHA®-2940/4/W  
AHA®-2940W MAC  
AHA®-3940/W  
AHA®-3980/5/W

Tandberg Data S.A.
16-18 Avenue Morane Saulnier, Bat A
F-78941 Velizy,
France
Phone	33-1-39260101
Fax	33-1-34650289
URL	www.tandberg.com

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

DATA BACKUP SOLUTIONS	58

Winter, 1996

Tandberg Data S.A.

	Panther 2500 (TDC 4220)

	Tandberg data tape drives series offers one of the most affordable backup choices for Power PC and LAN users.  Low cost per megabyte 
	coupled with significant growth potential provide outstanding backup value.

Host Adapters Tested
APA™-348  
APA™-358  
APA™-1460  
AVA™-1505  
AHA®-1510  
AVA™-1515  
AHA®-1520/2  
AHA®-1530/2P  
AHA®-1540/2/F/P  
AHA®-1640  
AHA®-1740/2/4  
AHA®-2740/2/4/T/W  
AHA®-2825VL  
AHA®-2840/2VL  
AHA®-2940/4/W  
AHA®-2940W MAC  
AHA®-3940/W  
AHA®-3980/5/W

Tandberg Data S.A.
16-18 Avenue Morane Saulnier, Bat A
F-78941 Velizy,
France
Phone	33-1-39260101
Fax	33-1-34650289
URL	www.tandberg.com

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

DATA BACKUP SOLUTIONS	59

Winter, 1996

Tandberg Data S.A.

	Panther 5000 (TDC 4222)

	Tandberg data tape drives series offers one of the most affordable backup choices for Power PC and LAN users.  Low cost per megabyte 
	coupled with significant growth potential provide outstanding backup value.

Host Adapters Tested
APA™-348  
APA™-358  
APA™-1460  
AVA™-1505  
AHA®-1510  
AVA™-1515  
AHA®-1520/2  
AHA®-1530/2P  
AHA®-1540/2/F/P  
AHA®-1640  
AHA®-1740/2/4  
AHA®-2740/2/4/T/W  
AHA®-2825VL  
AHA®-2840/2VL  
AHA®-2940/4/W  
AHA®-2940W MAC  
AHA®-3940/W  
AHA®-3980/5/W

Tandberg Data S.A.
16-18 Avenue Morane Saulnier, Bat A
F-78941 Velizy,
France
Phone	33-1-39260101
Fax	33-1-34650289
URL	www.tandberg.com

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

DATA BACKUP SOLUTIONS	60

Winter, 1996

Tandberg Data S.A.

	Panther Mini 2000 (TDC 3520)

	Tandberg data tape drives series offers one of the most affordable backup choices for Power PC and LAN users.  Low cost per megabyte 
	coupled with significant growth potential provide outstanding backup value.

Host Adapters Tested
APA™-348  
APA™-358  
APA™-1460  
AVA™-1505  
AHA®-1510  
AVA™-1515  
AHA®-1520/2  
AHA®-1530/2P  
AHA®-1540/2/F/P  
AHA®-1640  
AHA®-1740/2/4  
AHA®-2740/2/4/T/W  
AHA®-2825VL  
AHA®-2840/2VL  
AHA®-2940/4/W  
AHA®-2940W MAC  
AHA®-3940/W  
AHA®-3980/5/W

Tandberg Data S.A.
16-18 Avenue Morane Saulnier, Bat A
F-78941 Velizy,
France
Phone	33-1-39260101
Fax	33-1-34650289
URL	www.tandberg.com

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

DATA BACKUP SOLUTIONS	61

Winter, 1996

Tandberg Data S.A.

	Panther Mini 4600 (TDC 3720)

	Tandberg data tape drives series offers one of the most affordable backup choices for Power PC and LAN users.  Low cost per megabyte 
	coupled with significant growth potential provide outstanding backup value.

Host Adapters Tested
APA™-348  
APA™-358  
APA™-1460  
AVA™-1505  
AHA®-1510  
AVA™-1515  
AHA®-1520/2  
AHA®-1530/2P  
AHA®-1540/2/F/P  
AHA®-1640  
AHA®-1740/2/4  
AHA®-2740/2/4/T/W  
AHA®-2825VL  
AHA®-2840/2VL  
AHA®-2940/4/W  
AHA®-2940W MAC  
AHA®-3940/W  
AHA®-3980/5/W

Tandberg Data S.A.
16-18 Avenue Morane Saulnier, Bat A
F-78941 Velizy,
France
Phone	33-1-39260101
Fax	33-1-34650289
URL	www.tandberg.com

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

DATA BACKUP SOLUTIONS	62

Winter, 1996

Tandberg Data S.A.

	Tandberg MLR 1

	The Tandberg MLR series tape drive is the ultimate choice today and in the future for data storage, backup, archival storage and data 
	interchange on your workstation, network server or mid-range computer.

Host Adapters Tested
AVA™-1505  
AHA®-1510  
AVA™-1515  
AHA®-1520/2  
AHA®-1530/2P  
AHA®-1540/2/F/P  
AHA®-1640  
AHA®-1740/2/4  
AHA®-2740/2/4/T/W  
AHA®-2840/2VL  
AHA®-2910A/Ai  
AHA®-2940/4/W  
AHA®-2940/4/U/UW  
AHA®-3940/W  
AHA®-3940U/UW

Tandberg Data S.A.
16-18 Avenue Morane Saulnier, B at A
F-78941 Velizy,
France
Phone	33-1-34650289
Toll free	33-1-34650289
URL	www.tandberg.com

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

DATA BACKUP SOLUTIONS	63

Winter, 1996

TAPEDISK Corporation

	TapeDisk® Professional

	TAPEDISK earned PC Computing Magazine’s Most Valuable Product Finalist status for 1994. TapeDisk turns your SCSI (DAT/DDS-2, 8MM, and 
	some QIC) tape drive into a logical disk drive by assigning a drive letter!  DOS/Windows/Windows 95 applications can write data 
	directly to, and read data directly from tape.  Backup of an entire disk with DOS commands like XCOPY, or move files with File Manager 
	or Explorer. Unlike traditional backup software, files do not have to be restored to the hard drive:  open, edit and print files 
	directly from the tape.  Long file names are now supported.  TAPEDISK files are accessible across peer-to-peer networks like Windows 
	for Workgroups, Lantastic, InvisibleLAN and POWERLan.  A SCSI tape drive, using TAPEDISK, can be "mapped" from a client to a Novell 
	server just like a hard drive.

Host Adapters Tested
APA™-358  
AHA®-1510  
AHA®-1520/2  
AHA®-1540/2/F/P  
AHA®-2740/2/4/T/W  
AHA®-2840/2VL  
AHA®-2940/4/W

TAPEDISK Corporation
P.O. Box 379, 85 Cove Lane
Oshkosh, WI 54902-0379
Phone	(800) 827-3372
Fax	(414) 233-8699
Toll free	(800) 827-3372

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

DATA BACKUP SOLUTIONS	64

Winter, 1996

TAPEDISK Corporation

	TAPEDISK AL

	TAPEDISK AL adds autoloader support to TAPEDISK Professional.  Currently supported is the Hewlett-Packard C1533A 6-tape auotloader, 
	also known as the SureStore 12000E.  TAPEDISK AL automatically locates, inserts and loads the requested 4MM DAT tape from the six slot 
	tape magazine.  Within the time it takes to load a tape cartridge, up to 21 gigabytes of uncompressed data is available.  Other 
	autoloader tape drives will be supported.  TAPEDISK AL is sold separately or is available as an add-on to TAPEDISK Professional.

Host Adapters Tested
APA™-358  
AHA®-1510  
AHA®-1520/2  
AHA®-1540/2/F/P  
AHA®-2740/2/4/T/W  
AHA®-2840/2VL  
AHA®-2940/4/W

TAPEDISK Corporation
P.O. Box 379, 85 Cove Lane
Oshkosh, WI 54902-0379
Phone	(800) 827-3372
Fax	(414) 233-8699
Toll free	(800) 827-3372

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

DATA BACKUP SOLUTIONS	65

Winter, 1996

Valitek, Inc.

	PST 2 Series Tape Backup

	Valitek manufactures portable tape backups that work through the parallel, serial or SCSI port and are designed to be shared among 
	multiple PCs, laptops, and file servers.  Valitek ships its tape backups with the Valitek Tape Backup Software—a DOS application that 
	drives the unit—either parallel or serial.  The drives can be used on the SCSI port via a third party tape backup software package 
	(Cheyenne, ARCSERVE, Central Point backup, Norton Backup for Windows, etc.)  The PST2 Series of tape drives is available in eight 
	models: the PST2 500, 1000, 2400, 5000, M2000, DAT2, DAT2+ and the DAT4+ with capacities ranging from 250MB to 4GB (uncompressed).

Host Adapters Tested
AHA®-1510  
AHA®-1540/2/F/P  
AHA®-1640  
AHA®-2840/2VL  
AHA®-2940/4/W  
AHA®-2940/4/U/UW

Valitek, Inc.
100 University Drive
Amherst, MA 01002
USA
Phone	(413) 549-2700
Fax	(413) 549-2900
E-mail	acer18@aol.com
URL	http://www.contagious.com/valitek/va

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

DATA BACKUP SOLUTIONS	66

Winter, 1996

Vitek Danmark

	ViTape

	ViTape is a backup/restore utility for SunSoft’s Interactive UNIX, version 3.0, with QFA and CPIO tape format. Backups made by ViTape 
	can be restored on other machines with “CPIO” programs (no QFA). The program is intended for use with DAT tape streamers.

Host Adapters Tested
AHA®-1510  
AHA®-1540/2/F/P

Vitek Danmark
Liljevej 45
Hvalsoe,  DK-4330
Denmark
Phone	(45)46-49-25-61
Fax	(45)46-49-20-90

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

DATA BACKUP SOLUTIONS	67

Winter, 1996

Vitek Danmark

	TAR2DOS

	TAR2DOS is a program which reads a “TAR” format tape on a SCSI tape streamer and extracts its contents to similar DOS files.  The 
	program is useful to transfer data from UNIX machines to DOS.

Host Adapters Tested
AHA®-1510  
AHA®-1540/2/F/P

Vitek Danmark
Liljevej 45
Hvalsoe,  DK-4330
Denmark
Phone	(45)46-49-25-61
Fax	(45)46-49-20-90

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

DATA BACKUP SOLUTIONS	68

Winter, 1996

Vitek Danmark

	DOS2TAR

	DOS2TAR is a program which backs up a DOS machine on a SCSI tape streamer in “TAR” tape format.  The program is useful to transfer data
	 from DOS machines to UNIX.

Host Adapters Tested
AHA®-1510  
AHA®-1540/2/F/P

Vitek Danmark
Liljevej 45
Hvalsoe,  DK-4330
Denmark
Phone	(45)46-49-25-61
Fax	(45)46-49-20-90

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

DATA BACKUP SOLUTIONS	69

Winter, 1996

Yosemite Technologies, Inc.

	TapeWare®

	TapeWare offers a potent, cost-effective backup system for file servers and workstations.  TapeWare is a Novell NetWare-based LAN 
	archival management system.  It backs up and restores files while giving managers significant flexibility in designing their backup 
	schedules.  Special features include: Administrator for Windows®95/Windows NT; automatic detection of ASPI controllers & devices; 
	NetWare Loadable Module; autoloader support; macros; TapeWare BASIC; unattended job scheduler and more.  TapeWare supports multiple 
	environments, protocols, machine types and file systems.

Host Adapters Tested
AHA®-1510  
AHA®-1520/2  
AHA®-1540/2/F/P  
AHA®-1640  
AHA®-1740/2/4  
AHA®-2740/2/4/T/W

Yosemite Technologies, Inc.
2750 North Clovis Avenue
Fresno, CA 93727
USA
Phone	(209) 292-8888
Fax	(209) 292-8908
Toll free	(800) 228-9236

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

FAULT TOLERANCE/PERFORMANCE SOLUTIONS	70

Winter, 1996

1776, Inc.

	1776 Disk Array Software

	1776 Disk Array Software™ enhances system availability and disk performance under UNIX (on AT® bus, EISA and Micro Channel® systems) by
	 providing on-line storage management, mirroring, striping, RAID arrays and dual-computer fault tolerance using Adaptec® intelligent 
	host adapters.  1776 software achieves maximum performance and dependable recovery from disk errors, due to its built-in device driver 
	written specifically for Adaptec SCSI host adapters.

Host Adapters Tested
AHA®-1540/2/F/P  
AHA®-1640  
AHA®-1740/2/4  
AHA®-2740/2/4/T/W  
AHA®-2840/2VL  
AHA®-2940/4/W

1776, Inc.
8632 South Sepulveda Boulevard
Los Angeles, CA 90045
Phone	(310) 215-1776
Fax	(310) 216-1107
URL	http://1776soft.com/adaptec.htm

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

FAULT TOLERANCE/PERFORMANCE SOLUTIONS	71

Winter, 1996

1776, Inc.

	1776 Multi Host Software

	1776 Multi-Host provides a new higher level of high-availability using Adaptec® host adapters under SCO operating systems.  Two systems
	 are connected so that if one fails, the other takes over.  Also, the user load can be shared between the two systems for higher 
	performance.  This is done by connecting the servers to a common SCSI bus and thus share common disk storage.  If one system should 
	fail, the other can take over its operations automatically and almost instantly, and have immediate access to up-to-date user data.  By
	 including fault-tolerant device drivers designed specifically for Adaptec host adapters, a very high level of reliability is achieved.

Host Adapters Tested
AHA®-1540/2/F/P  
AHA®-1640  
AHA®-1740/2/4  
AHA®-2740/2/4/T/W  
AHA®-2840/2VL  
AHA®-2940/4/W

1776, Inc.
8632 South Sepulveda Boulevard
Los Angeles, CA 90045
Phone	(310) 215-1776
Fax	(310) 216-1107
URL	http://1776soft.com/adaptec.htm

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

FAULT TOLERANCE/PERFORMANCE SOLUTIONS	72

Winter, 1996

Adaptec, Inc.

	ADAPTEC® CI/O™

	With easy to use Adaptec® CI/O™ software, managers can monitor all SCSI peripheral devices connected to servers by Adaptec® host 
	adapters.    
	  
	Using Adaptec® CI/O™ software on any Windows® client, managers can remotely monitor the I/O performance of any server on the network 
	from a single central location.  Managers can install the latest device drivers from a remote location as well.  
	  
	Adaptec® CI/O™ software automatically detects failure of any SCSI device on a network server and notifies the manager immediately.  
	With a clear view of I/O traffic, managers can spot bottlenecks and act quickly to balance I/O loads to optimize performance among SCSI
	 devices.  Adaptec® CI/O™ improves the manageability of any size network--from a single server to a global network.

Host Adapters Tested
AHA®-1540/2/F/P  
AHA®-2740/2/4/T/W  
AHA®-2840/2VL  
AHA®-2940/4/W  
AHA®-2940AU  
AHA®-3940/W  
AHA®-3980/5/W

Adaptec, Inc.
691 S Milpitas Blvd
Milpitas, CA
USA
Phone	1-800-934-2766
Fax	408-262-2533
Toll free	1-800-934-2766
E-mail	sales@adaptec.com
URL	http://www.adaptec.com

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

FAULT TOLERANCE/PERFORMANCE SOLUTIONS	73

Winter, 1996

Cactus International, Inc.

	LONE-OPTIMIZER

	LONE-OPTIMIZER is a UNIX and Xenix disk optimizer that increases the speed of your system by 20% to 75%. It is fully menu driven for 
	the UNIX impaired making it extremely easy-to-use. The LONE-OPTIMIZER offers a practice mode to let you see exactly what happens before
	 an actual optimization begins. With LONE-OPTIMIZER you can change the high-level interleave on the fly. This feature alone can double 
	system performance. It consolidates all directory information and keeps it next to the inode table for maximum file lookup performance.

Host Adapters Tested
AHA®-1510  
AHA®-1520/2  
AHA®-1540/2/F/P  
AHA®-1640  
AHA®-1740/2/4  
AHA®-2740/2/4/T/W

Cactus International, Inc.
13987 West Annapolis Court
Mt. Airy, MD 21771
USA
Phone	(301) 829-1622
Fax	(301) 829-1623
Toll free	(800) 525-UNIX
E-mail	cowboy@cactus.com

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

FAULT TOLERANCE/PERFORMANCE SOLUTIONS	74

Winter, 1996

Corel Corporation

	CorelRAID

	CorelRAID™, a software solution for data security, is a cost-effective way to safeguard your network data. At a fraction of the cost of
	 proprietary hardware solutions, CorelRAID provides fault-tolerant network performance with minimum disk space overhead.  CorelRAID 
	supports RAID levels 4 and 5 in the NetWare 3.11 environment.  With a minimum of three SCSI hard drives and any ASPI-compatible SCSI 
	controller, you can install several arrays in minutes. If a drive failure occurs, arrays are repaired with no downtime using either the
	 “hot swap” or “hot standby” features.

Host Adapters Tested
AHA®-1520/2  
AHA®-1540/2/F/P  
AHA®-1640

Corel Corporation
1600 Carling Avenue
Ottawa, Ontario K1Z 8R7
Canada
Phone	(613) 728-8200
Fax	(613) 728-9790
Toll free	(800) 836-7274

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

FAULT TOLERANCE/PERFORMANCE SOLUTIONS	75

Winter, 1996

Delphi Data

	RAIDer EO Arrays

	The RAIDer™ series of disk arrays and EO disk arrays provide unique hardware solutions for desktop to mainframe computer systems. 
	Configurations include RAID 0, 1, or 1+ and 10+. Our patented concurrent backup can copy data to tape or optical media without the need
	 to shutdown running applications.  
	  
	The RAIDer series of JukeBox arrays have configurations including one (1) or more JukeBox mechanisms. A single SCSI ID can control a 
	mirrored set of mechanisms providing transparent redundancy.  Tape backup of a JukeBox can be performed offline or concurrently during 
	normal operation.  
	  
	All systems include an integrated data cache, up to 256Mb per CacheBox, which greatly improves performance.

Host Adapters Tested
AHA®-1510  
AHA®-1520/2  
AHA®-1740/2/4  
AHA®-2740/2/4/T/W  
AHA®-2840/2VL  
AHA®-2940/4/W

Delphi Data
9069 Cajalco Road
Corona, CA 91719
Phone	(909) 279-7955
Fax	(909) 279-7957
Toll free	(800) -DELPHI5
E-mail	76470.1544@compuserve.com

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

FAULT TOLERANCE/PERFORMANCE SOLUTIONS	76

Winter, 1996

Delphi Data

	RAIDer JukeBox Arrays

	The RAIDer™ series of disk arrays and EO disk arrays provide unique hardware solutions for desktop to mainframe computer systems. 
	Configurations include RAID 0, 1, or 1+ and 10+. Our patented concurrent backup can copy data to tape or optical media without the need
	 to shutdown running applications.  
	  
	The RAIDer series of JukeBox arrays have configurations including one (1) or more JukeBox mechanisms. A single SCSI ID can control a 
	mirrored set of mechanisms providing transparent redundancy.  Tape backup of a JukeBox can be performed offline or concurrently during 
	normal operation.  
	  
	All systems include an integrated data cache, up to 256Mb per CacheBox, which greatly improves performance.

Host Adapters Tested
AHA®-1510  
AHA®-1520/2  
AHA®-1740/2/4  
AHA®-2740/2/4/T/W  
AHA®-2840/2VL  
AHA®-2940/4/W

Delphi Data
9069 Cajalco Road
Corona, CA 91719
Phone	(909) 279-7955
Fax	(909) 279-7957
Toll free	(800) -DELPHI5
E-mail	76470.1544@compuserve.com

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

FAULT TOLERANCE/PERFORMANCE SOLUTIONS	77

Winter, 1996

Delphi Data

	RAIDer CacheBox Arrays  
	RAIDer Writable CD Arrays

	The RAIDer™ series of disk arrays and EO disk arrays provide unique hardware solutions for desktop to mainframe computer systems.   
	Configurations include RAID 0, 1, or 1+ and 10+. Our patented concurrent backup can copy data to tape or optical media without the need
	 to shutdown running applications.  
	  
	The RAIDer series of JukeBox arrays have configurations including one (1) or more JukeBox mechanisms. A single SCSI ID can control a 
	mirrored set of mechanisms providing transparent redundancy. Tape backup of a JukeBox can be performed offline or concurrently during 
	normal operation.  
	  
	All systems include an integrated data cache, up to 256 Mb per CacheBox, which greatly improves performance.

Host Adapters Tested
AHA®-1510  
AHA®-1520/2  
AHA®-1740/2/4  
AHA®-2740/2/4/T/W  
AHA®-2840/2VL  
AHA®-2940/4/W

Delphi Data
9069 Cajalco Road
Corona, CA 91719
Phone	(909) 279-7955
Fax	(909) 279-7957
Toll free	(800) -DELPHI5
E-mail	76470.1544@compuserve.com

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

FAULT TOLERANCE/PERFORMANCE SOLUTIONS	78

Winter, 1996

Florida Datamation

	Data On Demand

	Data On Demand is a fault tolerance disk array with user programmable RAID 0, 3 and 5. It supports up to 24GB with desk side and 96GB 
	with rack mount. Features include hot swap data and power modules, and redundant fan and I/O control.

Host Adapters Tested
AHA®-1540/2/F/P  
AHA®-1640  
AHA®-1740/2/4  
AHA®-2740/2/4/T/W  
AHA®-2840/2VL  
AHA®-2940/4/W

Florida Datamation
AMTEC Center, 6405 Congress Ave, Suite 140
Boca Raton, FL 33487
Phone	(407) 241-2966
Fax	(407) 241-3108
Toll free	(800) 642-5938
E-mail	sales@fdma.com

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

FAULT TOLERANCE/PERFORMANCE SOLUTIONS	79

Winter, 1996

HCL Hewlett Packard Ltd.

	Busy Bee and Meteor

	The HCL-Hewlett Packard Busy Bee and Meteor Systems are developed in India for use in the Indian market.  They are highly scalable 
	designs starting from home PC low-end configurations to large business UNIX and NetWare servers.

Host Adapters Tested
AHA®-1520/2  
AHA®-1540/2/F/P  
AHA®-1740/2/4  
AHA®-2740/2/4/T/W  
AHA®-2940/4/W  
AHA®-2940/4/U/UW

HCL Hewlett Packard Ltd.
E4, E5, E6 Sector 11, Noida
Dist Ghaziabad,  201301
India
Phone	91-11-8531353
Fax	91-11-8521113

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

FAULT TOLERANCE/PERFORMANCE SOLUTIONS	80

Winter, 1996

Legacy Storage Systems

	Smart Array®, Smart Array XE

	Legacy's SmartArray® family of disk array subsystems offer the best combination of performance and fault tolerance for mission-critical
	 servers.  Available as either a storage tower or rack-mount, SmartArray subsystems accommodate every major storage technology:  hard 
	disk, CD-ROM, and tape (DAT, QIC, and 8mm).  Devices and power supplies are hot-swappable for zero-downtime applications.  The advanced
	 intelligent monitor displays device, power supply, temperature, and fan status.  It also monitors RAID rebuilds and detects duplicate 
	SCSI IDs.  Visual and audio alarms indicate error conditions, and messages can be broadcast by MHS or SNMP, or via pager.    
	  
	SmartArray supports up to 6 SCSI-3 Fast/Wide buses, and all major operating systems.  

	  
	Canadian  Corporate Headquarters  
	43 Riviera Drive  
	Markham, Ontario L3R 5J6  
	Canada  
	Tel:  (905)475-1077  
	Fax:  (905)475-1088

Host Adapters Tested
AHA®-1640  
AHA®-1740/2/4  
AHA®-2740/2/4/T/W  
AHA®-2940/4/W  
AHA®-3940/W

Legacy Storage Systems
138 River Road, Suite 204
Andover, MA 01810
USA
Phone	(508) 681-8400
Fax	(508) 689-9004
Toll free	(800) 966-6442

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

FAULT TOLERANCE/PERFORMANCE SOLUTIONS	81

Winter, 1996

Logicraft Information Systems

	The Jukebox Manager

	The Jukebox Manager™ option for Logicraft's LanCD™ network server software provides a versatile solution for networked access to 
	archived CD-ROM storage.  It is modular in design, hardware independent and non-vendor specific for jukebox support.  Features include 
	Document Image Management, static directory or platter caching and DDC (dynamic hard disk cache), asynchronous access, multiple jukebox
	 support, Intelligent Optical Reader Selection, local on-line management, and support for up to 1280 platters and 56 readers per LanCD 
	server.  With up to 10 servers per client, each user could have access to more than 12 thousand CD-ROM discs.

Host Adapters Tested
AHA®-1540/2/F/P  
AHA®-1740/2/4  
AHA®-2740/2/4/T/W  
AHA®-2940/4/W  
AHA®-3940/W

Logicraft Information Systems
22 Cotton Road
Nashua, NH 03063
Phone	603-880-0300
Fax	(603) 880-7229
Toll free	800-880-5644
E-mail	sales@logicraft.com
URL	http://www.logicraft.com

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

FAULT TOLERANCE/PERFORMANCE SOLUTIONS	82

Winter, 1996

Logicraft Information Systems

	FastCD™, LanCD

	FastCD™ is an option available with Logicraft's LanCD™ networking software for providing multiple concurrent access to CD-ROM 
	applications in a multi-platform, multi-protocol networking environment.  FastCD creates "virtual CD-ROM discs" on fast, high 
	performance SCSI hard drives by caching the entire contents of a CD-ROM in its native format onto a FastCD partition of the hard disk, 
	providing users with easy access to their CD-ROM applications at hard disk speeds up to 300 times faster than standard CD-ROM drives.  
	FastCD software includes comprehensive status reports, multimedia support, and asynchronous disk access for higher throughput during 
	multiple concurrent accessing.

Host Adapters Tested
AHA®-1540/2/F/P  
AHA®-1740/2/4  
AHA®-2740/2/4/T/W  
AHA®-2940/4/W  
AHA®-3940/W

Logicraft Information Systems
22 Cotton Road
Nashua, NH 03063
Phone	603-880-0300
Fax	(603) 880-7229
Toll free	800-880-5644
E-mail	sales@logicraft.com
URL	http://www.logicraft.com

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

FAULT TOLERANCE/PERFORMANCE SOLUTIONS	83

Winter, 1996

Logicraft Information Systems

	CDexecutive™ CD-ROM Network Server

	The CDexecutive /XF5500 CD-ROM network server provides a turnkey solution for multiple concurrent accesses to CD-ROM applications in a 
	multi-platform, multi-protocol environment.  The Pentium™ based XF hardware architecture is bundled with Logicraft's high performance 
	CDexecutive Management Center software that automatically monitors and manages CD-ROM applications as a background Windows NT™ service.
	  Client support includes Windows® 95, Windows® for Workgroups, Macintosh® and NetWare clients.  The XF server holds up to 14 SCSI 
	devices and comes equipped with IDE hard drive, network interface card, floppy drive and SCSI host adapters.  It runs at 120MHz, has 
	32MB of RAM and supports up to 56 SCSI devices.

Host Adapters Tested
AHA®-2740/2/4/T/W

Logicraft Information Systems
22 Cotton Road
Nashua, NH 03063
Phone	603-880-0300
Fax	(603) 880-7229
Toll free	800-880-5644
E-mail	sales@logicraft.com
URL	http://www.logicraft.com

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

FAULT TOLERANCE/PERFORMANCE SOLUTIONS	84

Winter, 1996

Logicraft Information Systems

	LanCD™ CD-ROM Network Servers

	The LanCD/XF family of CD-ROM network servers provides a turnkey solution for multiple concurrent accesses to CD-ROM applications in a 
	multi-platform, multi-protocol environment.  The Pentium™ based XF hardware architecture is bundled with Logicraft's high-performance 
	LanCD and FastCD™ software that supports DOS, Windows® and Windows® 95 clients.  Optional support is available for Windows NT® and 
	Macintosh clients.  Each chassis holds up to 14 SCSI devices and comes equipped with IDE hard drive, network interface card, floppy 
	drive and SCSI host adapters.  The XF5300 runs at 75MHz, has 16MB of RAM and expands to 28 drives.  The XF5500 runs at 120MHz, has 32MB
	 and supports up to 56 drives.

Host Adapters Tested
AHA®-1520/2  
AHA®-1540/2/F/P  
AHA®-1640  
AHA®-1740/2/4  
AHA®-2740/2/4/T/W  
AHA®-2940/4/W  
AHA®-3940/W

Logicraft Information Systems
22 Cotton Road
Nashua, NH 03063
Phone	603-880-0300
Fax	(603) 880-7229
Toll free	800-880-5644
E-mail	sales@logicraft.com
URL	http://www.logicraft.com

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

FAULT TOLERANCE/PERFORMANCE SOLUTIONS	85

Winter, 1996

Media Integration, Inc.

	Intelligent Storage

	Intelligent Storage™ is a fault-tolerant SCSI storage subsystem for hard disks, optical disks and tape drives.  Features include 
	distributed power with redundant, hot removable and replaceable power supplies and removable storage devices, including those with 
	removable media.  It provides the highest level of fault tolerant, redundant power and removability while continuing full operation.  
	It will accept any standard 5.25" or 3.5" storage device.

Host Adapters Tested
AHA®-1510  
AHA®-1520/2  
AHA®-1540/2/F/P  
AHA®-1640  
AHA®-1740/2/4  
AHA®-2740/2/4/T/W

Media Integration, Inc.
3949 Research Park Court, Suite 190
Soquel, CA 95073
USA
Phone	(408) 475-9400
Fax	(408) 475-0110
Toll free	(800) 824-7385

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

FAULT TOLERANCE/PERFORMANCE SOLUTIONS	86

Winter, 1996

Optisys

	GlobalNet

	GlobalNet™ storage servers provide Novell Network access to optical jukeboxes, including CD-ROM, Erasable and WORM (Write Once Read 
	Many) technologies.  Notable for its ease of installation, use and its speed.

Host Adapters Tested
AHA®-1540/2/F/P  
AHA®-2840/2VL  
AHA®-3940/W

Optisys
9250 North 43rd Avenue, Suite 12
Glendale, AZ 85302
Phone	(602) 997-9699
Fax	(602) 944-4051
Toll free	(800) 327-1271

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

FAULT TOLERANCE/PERFORMANCE SOLUTIONS	87

Winter, 1996

Symbios Logic

	MetaStor

	MetaStor disk array products provide high performance RAID in addition to other features that contribute to continuous data 
	availability.

Host Adapters Tested
AHA®-2940/4/W

Symbios Logic
3718 N Rock Road
Wichita, KS 67226
USA
Phone	(316) 636-8000
Fax	(316) 636-8889
Toll free	(800) 440-5606

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

FAULT TOLERANCE/PERFORMANCE SOLUTIONS	88

Winter, 1996

Unitrol Data Protection Systems, Inc.

	Immunity

	Immunity® Disk Mirroring Software v2.2 is a cost-effective RAID 1 product that provides system fault tolerance for DOS and Windows 
	based PCs and LANs.  The device driver duplicates (or mirrors) every “save” to two hard disks through one or two (duplexed) 
	controllers/host adapters.  If one of the hard disks fails, the device driver instantly re-routes all reads and writes to the remaining
	 hard disk with no loss of time, defaults or data.

Host Adapters Tested
AHA®-1520/2  
AHA®-1540/2/F/P  
AHA®-1640  
AHA®-1740/2/4  
AHA®-2740/2/4/T/W  
AHA®-2940/4/W  
AHA®-3940/W

Unitrol Data Protection Systems, Inc.
777-1177 West Hastings Street
Vancouver, BC V6E 2K3
Canada
Phone	(604) 681-3611
Fax	(604) 681-3615
Toll free	(800) 665-2212

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

IMAGING SOLUTIONS	89

Winter, 1996

Adaptec, Inc.

	ADAPTEC® EZ-SCSI®

	If you have, or are planning to add, SCSI peripherals like tape or disk drives, CD-ROM drives, recordable CD-R drives, magneto-optical 
	drives, or scanners, Adaptec EZ-SCSI® software provides everything you need to manage and take full advantage of each device.  
	  
	Adaptec EZ-SCSI software is a suite of 32-bit practical applications and power tools that are remarkably easy to install and use.  
	Simple desktop controls give you immediate access to any fuction.  A unique online tutorial explains everything you need to know about 
	SCSI in easy-to-understand terms.  
	  
	Key benefits:  
	* Easiest way to manage SCSI peripherals  
	* For Windows operating systems  
	* Includes these practical applications:  Adaptec Easy-CD Backup™, QuickScan™, Audio CD player, Photo CD Viewer, CD Writer, and CD 
	Copier  
	* Includes these powerful tools:  SCSI Explorer™ (Power Management, SCSI Interrogator™, Read/Write Disk Cashe tool), SCSI Tutor™, SCSI 
	Bench™ and Drive Light™.

Host Adapters Tested
APA™-348  
APA™-358  
APA™-1460  
AVA™-1505  
AHA®-1510  
AVA™-1515  
AHA®-1520/2  
AHA®-1530/2P  
AHA®-1540/2/F/P  
AHA®-1640  
AHA®-1740/2/4  
AHA®-2740/2/4/T/W  
AHA®-2840/2VL  
AHA®-2920  
AHA®-2940/4/W  
AHA®-2940AU  
AHA®-3940/W  
AHA®-3940U/UW

Adaptec, Inc.
691 S Milpitas Blvd
Milpitas, CA
USA
Phone	1-800-934-2766
Fax	408-262-2533
Toll free	1-800-934-2766
E-mail	sales@adaptec.com
URL	http://www.adaptec.com

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

IMAGING SOLUTIONS	90

Winter, 1996

Analogic Corporation

	DASM-VIP

	The DASM-VIP Video Image Processor combines a video frame grabber and a 33-Megaflop DSP into an external unit that attachs to a SCSI 
	port.  The DASM-VIP acquires, processes and displays 24-bit color or 8-bit monochrome video images.  Imaging functions can run on the 
	DSP using an on-board real-time operating system.  The DASM-VIP is a cost-effective solution for commercial OEM and scientific 
	applications.  Captures at 30fps from RGB, NTSC, S-Video or RS-170 video sources. Supported on DOS, Windows and UNIX operating systems.

Host Adapters Tested
AHA®-1540/2/F/P

Analogic Corporation
8 Centennial Drive
Peabody, Mass 01960
USA
Phone	(508) 977-3000
Fax	(508) 977-6813

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

IMAGING SOLUTIONS	91

Winter, 1996

Binary Image Pty Ltd.

	Telemedicine

	Telemedicine is based on the ‘genuine’ Intel microcomputer and the Microsoft Windows operating system. It provides the ability to 
	digitally capture, archive, transmit, network, enhance and print images from all diagnostic imaging modalities, including x-ray, 
	pathology, C.T., ultrasound, M.R.I., and nuclear medicine.

Host Adapters Tested
AHA®-1510  
AHA®-1520/2  
AHA®-1540/2/F/P  
AHA®-1640  
AHA®-1740/2/4  
AHA®-2740/2/4/T/W

Binary Image Pty Ltd.
184 Warrigal Road
Oakleigh, Victoria 3166
Australia
Phone	61-3-9563-8699
Fax	61-3-9563-7446
E-mail	baker@melbpc.org.au

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

IMAGING SOLUTIONS	92

Winter, 1996

Cirrus Technology, Inc.

	UNITE Net®

	Unite Net®  is a PC LAN-based document/image management system and available for the Windows NT or OS/2 environment.  Unite Net® is a 
	complete solution for data capturing, purifying and storage management. Various optional components are available to direct the flow of
	 data throughout the system such as OCR, COLD and Workflow.

Host Adapters Tested
AVA™-1505  
AHA®-1510  
AVA™-1515  
AHA®-1520/2  
AHA®-1530/2P  
AHA®-1540/2/F/P  
AHA®-1640  
AHA®-1740/2/4  
AHA®-2740/2/4/T/W  
AHA®-2825VL  
AHA®-2840/2VL  
AHA®-2910A/Ai  
AHA®-2940/4/W  
AHA®-3940/W  
AHA®-3980/5/W

Cirrus Technology, Inc.
5301 Buckeystown Pike, 4th floor
Frederick, MD 21704
US
Phone	(301)698-1900
Fax	(301)698-1909
E-mail	sales@cirunite.com
URL	http://www.cirunite.com

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

IMAGING SOLUTIONS	93

Winter, 1996

Cirrus Technology, Inc.

	UniteLite®

	UniteLite is a folder and document management application designed for personal or small workgroup use.  With UnitLite, users can scan,
	 view, print and fax images.  Many image formats are supported.  Advanced features include zooming, rotating and annotation images.

Host Adapters Tested
AVA™-1505  
AHA®-1510  
AVA™-1515  
AHA®-1520/2  
AHA®-1530/2P  
AHA®-1540/2/F/P  
AHA®-1640  
AHA®-1740/2/4  
AHA®-2740/2/4/T/W  
AHA®-2825VL  
AHA®-2840/2VL  
AHA®-2910A/Ai  
AHA®-2940/4/W  
AHA®-3940/W  
AHA®-3980/5/W

Cirrus Technology, Inc.
5301 Buckeystown Pike, 4th floor
Frederick, MD 21704
US
Phone	(301)698-1900
Fax	(301)698-1909
E-mail	sales@cirunite.com
URL	http://www.cirunite.com

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

IMAGING SOLUTIONS	94

Winter, 1996

Corel Corporation

	CorelSCSI Pro

	CorelSCSI Pro® is a high-performance software product designed to maximize SCSI performance.  CorelSCSI Pro provides: support for SCSI 
	scanners to scan images into any TWAIN-compliant graphics program; a CD-ROM server application that allows network users to retrieve 
	recently-accessed information with essentially no delay; and a utility that writes information to a compact disc using a CD-Recorder. 
	These features and others are available using an intuitive and friendly interface.

Host Adapters Tested
AHA®-1520/2  
AHA®-1540/2/F/P  
AHA®-1640

Corel Corporation
1600 Carling Avenue
Ottawa, Ontario K1Z 8R7
Canada
Phone	(613) 728-8200
Fax	(613) 728-9790
Toll free	(800) 836-7274

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

IMAGING SOLUTIONS	95

Winter, 1996

Cornerstone Imaging, Inc.   Storage Division

	MDMI

	The Optical File System (OFS) for optical drives software package provides access to standalone and daisy-chained optical disk drives 
	or rapidchangers under DOS- and PC-based networks, including all versions of NetWare, Banyan, 3Com®, LAN Manager, LANtastic, OS/2 2.x, 
	3.x and Warp, Windows 95 and Windows NT.  MDMI supports most 5.25- and 12-inch optical disk drives.  Data stored on optical disks using
	 the OFS are transportable to jukebox versions of the Optical File System software.  The software treats a single or entire daisy-chain
	 of optical drives as one drive designator under Novell DOS and the network systems supported.  Each side of an optical disk platter 
	under the assigned drive letter then appears as a subdirectory and is fully accessible through normal operating system commands.

Host Adapters Tested
APA™-1460  
AHA®-1510  
AHA®-1520/2  
AHA®-1530/2P  
AHA®-1540/2/F/P  
AHA®-1640  
AHA®-2840/2VL  
AHA®-2940/4/W

Cornerstone Imaging, Inc.   Storage Division
1600 South Main Street
Walnut Creek, CA 94596
Phone	(510) 938-5340
Fax	(510) 938-5341

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

IMAGING SOLUTIONS	96

Winter, 1996

Cornerstone Imaging, Inc.   Storage Division

	OJMI

	The Optical File System (OFS) for optical drives software package provides access to standalone and daisy-chained optical disk drives 
	or rapidchangers under DOS- and PC-based networks, including all versions of NetWare, Banyan, 3Com®, LAN Manager, LANtastic, OS/2 2.x, 
	3.x and Warp, Windows 95 and Windows NT.  MDMI supports most 5.25- and 12-inch optical disk drives.  Data stored on optical disks using
	 the OFS are transportable to jukebox versions of the Optical File System software.  The software treats a single or entire daisy-chain
	 of optical drives as one drive designator under Novell DOS and the network systems supported.  Each side of an optical disk platter 
	under the assigned drive letter then appears as a subdirectory and is fully accessible through normal operating system commands.

Host Adapters Tested
APA™-1460  
AHA®-1510  
AHA®-1520/2  
AHA®-1540/2/F/P  
AHA®-1640  
AHA®-2840/2VL  
AHA®-2940/4/W

Cornerstone Imaging, Inc.   Storage Division
1600 South Main Street
Walnut Creek, CA 94596
Phone	(510) 938-5340
Fax	(510) 938-5341

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

IMAGING SOLUTIONS	97

Winter, 1996

Courtland Group, Inc.

	Courtland Intelligent Image Caching System

	The Courtland Intelligent Image Caching System (IICS) is designed for multiuser and jukebox-based optical imaging systems.  IICS 
	eliminates the workflow bottlenecks which occur when there are multiple requests for images or when optical redirectors are needed.  
	The IICS system performs three simultaneous tasks: operating as an image caching server, high-speed print server, and network FAX 
	server.  IICS operates on Courtland’s popular Ultra PLUS and Ultra optical platforms in either DOS or Windows and interfaces with a 
	wide range of optical drives and jukeboxes.  IICS is also available in a ‘remote’ version for support of additional jukebox, faxing or 
	high-speed printing locations.

Host Adapters Tested
AHA®-1510  
AHA®-1520/2  
AHA®-1540/2/F/P  
AHA®-1640

Courtland Group, Inc.
10500 Little Patuxent Pkwy, Suite 850
Columbia, MD 21044
US
Phone	(410) 730-7668
Fax	(410) 730-8271

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

IMAGING SOLUTIONS	98

Winter, 1996

Danmar Systems, Inc.

	SCSISCAN

	SCSISCAN™ software consists of an ASPI module which allows an HP ScanJet® IIc, HP ScanJet IIcx, or HP ScanJet IIP scanner to be 
	controlled directly from an Adaptec® SCSI host adapter.  The driver allows applications that are compatible with the HP driver and 
	controller to be used with non-HP controllers.  This design frees up a slot in the computer and also increases performance.  The 
	SCSISCAN driver uses only 4K of RAM and can be loaded into high memory (UMBs) using most popular memory managers.  The retail price of 
	the SCSISCAN software is $89.95.  An OS/2 version of the software is also available.

Host Adapters Tested
APA™-348  
APA™-358  
AHA®-1510  
AHA®-1520/2  
AHA®-1540/2/F/P  
AHA®-1640  
AHA®-1740/2/4  
AHA®-2740/2/4/T/W  
AHA®-2840/2VL

Danmar Systems, Inc.
6031 S.W. 128 Court
Miami, FL 33183
Phone	(305) 388-4671
Fax	(305) 388-5326

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

IMAGING SOLUTIONS	99

Winter, 1996

ECRM Inc.

	Scriptsetter

	The ECRM Scriptsetter product line encompasses a range of Postscript imagesetters starting at the entry-level VR30 at 12 inches wide.  
	The top of the line is the Knockout which images up to 18 inches wide and includes productivity features such as built in registration 
	punches and buffering for on-line film processing.  The software Postscript RIP is available for the MAC, PoweMAC, Windows® and 
	Windows® NT.  (DEC Alpha  and Intel)

Host Adapters Tested
AHA®-1540/2/F/P

ECRM Inc.
554 Clark Road
Tewksbury, MA 01876
USA
Phone	1-800-537-3276
Fax	508-851-7016
Toll free	1-800-537-3276
E-mail	@ecrm.com

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

IMAGING SOLUTIONS	100

Winter, 1996

Fast Forward Video

	Outlaw/Bandit

	Bandit™, the first product in the Outlaw series, is a digital peripheral device that interfaces to a variety of host computers (PC, 
	Macintosh, SGI, Amiga).  Animators can transfer image files directly to Bandit via SCSI, then play the sequence in real time, 
	eliminating the need for expensive single-frame VTRs and controllers.  It uses JPEG compression.

Host Adapters Tested
AHA®-1510

Fast Forward Video
18200-C West McDurmott
Irvine, CA 92714
USA
Phone	(714) 852-8404
Fax	(714) 852-1226

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

IMAGING SOLUTIONS	101

Winter, 1996

Image Machines

	IMageCenter

	IMageCenter is a full-featured imaging software for large-format documents.  IMageCenter capabilities include raster editing, 
	redlining, CAD overlays and batch processing of A-J size documents.  IMageCenter offers easy integration of your favorite Adaptec SCSI 
	device through their Advanced SCSI Programming Interface (ASPI).  IMageCenter supports the Vidar TruScan and Contex FSS large-format 
	scanners.  IMageCenter also supports the Photomatrix & Vidar Aperture Card Scanners and high-speed, small-format scanners like the 
	Fujitsu M3096GX.  In addition, all TWAIN compatible scanners are supported.

Host Adapters Tested
AHA®-1520/2  
AHA®-1540/2/F/P

Image Machines
590 Herndon Parkway
Herndon, VA 20170
USA
Phone	703-709-7475
Fax	703-709-8966
URL	www.imagemachines.com

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

IMAGING SOLUTIONS	102

Winter, 1996

Image Technologies Developments plc

	Wisp-PS

	PostScript Level 2 interpreters and drivers for over 60 different colour and monochrome copiers/printers.  Implementations using Fast 
	and Wide SCSI offer considerably increased printing/scanning speeds compared with standard SCSI 1 & 2 interfaces, both are supported.  
	Wisp-PS offers PrintServer capabilities thereby facilitating both multiple printing devices from a single PrintServer and sharing of 
	SCSI printers for printing over both local and wide area networks.  ITD specializes in writing device drivers for SCSI devices,  be 
	they printers or scanners under Windows 95 and NT and offers manufacturers and distributors programming expertise and advice on how to 
	maximize the efficiency of their SCSI printing devices.

Host Adapters Tested
AVA™-1505  
AHA®-1510  
AVA™-1515  
AHA®-1640  
AHA®-1740/2/4  
AHA®-2940/4/W

Image Technologies Developments plc
Pyramid House, 1 Martindale Road
Hounslow West, Middlesex,  TW4 7EW
UK
Phone	44-181-572-5900
Fax	44-181-572-5188

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

IMAGING SOLUTIONS	103

Winter, 1996

Image-In Incorporated

	Image-In Color Professional

	Image-In Color Professional offers the most advanced scanning, image editing and photo retouching tools available.  Mask unique areas 
	with the resize, add, subtract, intersect, and inverse options.  Powerful tool options include control of size, shape and pressure 
	(including Windows for Pen), spacing, fadeout, paint mode, repeat rate and tool edge with the right mouse button feature.  Over 20 
	special effect and photographic filters are included.  Color separate images.  Over 50 scanners are supported, as well as Twain 
	compliant scanners.  Import images from the Kodak PhotoCD, as well as TIFF, PCX, BMP, GIF, TGA, and JPEG files.  Supports the Kodak 
	XL/7700 and XLT 7720 printers through a direct export module.

Host Adapters Tested
AHA®-1510  
AHA®-1520/2  
AHA®-1540/2/F/P  
AHA®-1640  
AHA®-1740/2/4

Image-In Incorporated
1820 Gateway Drive, Building 3, Suite 370
San Mateo, CA 94404
USA
Phone	(415) 358-8500
Fax	(415) 358-9535

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

IMAGING SOLUTIONS	104

Winter, 1996

Interlinear Technology, Inc.

	AEDIS

	AEDIS (Agile Electronic Document Information Solution) is an open and distributed UNIX-based electronic data management system.  
	Functions include file search, revision control, archiving, and access security.  Document work-flow features include user-configurable
	 review, approval, and routing procedures for documents, drawings of any size, faxes, photos, folders (groups of files), etc.  AEDIS 
	software modules integrate with a wide variety of commercially available hardware, relational databases, and off-the-shelf software 
	packages.  AEDIS utilizes client/server architecture, distributing data processing loads across TCP/IP networks, and supports X and MS 
	Windows user interfaces.  Compliant with the CALS, type II (TRIF) raster image standard.

Host Adapters Tested
AHA®-1520/2  
AHA®-1540/2/F/P

Interlinear Technology, Inc.
1420 Harbor Bay Parkway, Suite 281
Alameda, CA 94502
USA
Phone	(510) 522-5077
Fax	(510) 522-1228
E-mail	augie@ilt.com

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

IMAGING SOLUTIONS	105

Winter, 1996

Koch Software Industries, Inc.

	Image AWL

	ImageAWL® is a device- independent API for scanners, designed to provide a seamless union between imaging hardware and software.  By 
	policing the device in multitasking and multiuser environments, it relieves the device conflicts with multiple applications or users, 
	and prevents system lock outs when these conflicts arise.

Host Adapters Tested
AHA®-1520/2  
AHA®-1540/2/F/P  
AHA®-1640  
AHA®-1740/2/4

Koch Software Industries, Inc.
P.O. Box 3194, 1097 Glencrest Drive
Bannington, IL 60010
USA
Phone	(708) 304-5544
Fax	(708) 304-4624

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

IMAGING SOLUTIONS	106

Winter, 1996

Laser Today International, Inc.

	LaserLink

	LaserLink™ CJ-10 for Windows is an application specifically designed for Canon CJ-10 (CLC/10) digital color copier.  The features 
	include: scanning and printing 400 dpi full-page color images; built-in color correction to adjust RGB; contrast; brightness; and gamma
	 for both scan and print.  Support for popular industry image file formats includes: BMP, TIFF, Targa and PCX.  The built-in page 
	layout function supports multiple-image layout in one page.

Host Adapters Tested
AHA®-1510  
AHA®-1520/2  
AHA®-1540/2/F/P  
AHA®-1740/2/4

Laser Today International, Inc.
1924 Old Middlefield Way
Mountain View, CA 94043
USA
Phone	(415) 961-3015
Fax	(415) 961-7631

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

IMAGING SOLUTIONS	107

Winter, 1996

Laser Today International, Inc.

	ColorLink

	ColorLink™ for Windows is an application designed for the Canon CJ-10 (CLC-10) digital color copier.  Capabilities include: scanning 
	and printing 400-dpi color images, faxing color images from CJ-10 flat-bed scanner, video source or the image files from the hard disk 
	in the computer.  After receiving the color FAX, the software can print the image right away, save it to print later, etc.  It supports
	 TIFF, Targa, BMP, PCX and RGB file formats.

Host Adapters Tested
AHA®-1510  
AHA®-1520/2  
AHA®-1540/2/F/P  
AHA®-1740/2/4

Laser Today International, Inc.
1924 Old Middlefield Way
Mountain View, CA 94043
USA
Phone	(415) 961-3015
Fax	(415) 961-7631

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

IMAGING SOLUTIONS	108

Winter, 1996

Logicraft Information Systems

	The Jukebox Manager

	The Jukebox Manager™ option for Logicraft's LanCD™ network server software provides a versatile solution for networked access to 
	archived CD-ROM storage.  It is modular in design, hardware independent and non-vendor specific for jukebox support.  Features include 
	Document Image Management, static directory or platter caching and DDC (dynamic hard disk cache), asynchronous access, multiple jukebox
	 support, Intelligent Optical Reader Selection, local on-line management, and support for up to 1280 platters and 56 readers per LanCD 
	server.  With up to 10 servers per client, each user could have access to more than 12 thousand CD-ROM discs.

Host Adapters Tested
AHA®-1540/2/F/P  
AHA®-1740/2/4  
AHA®-2740/2/4/T/W  
AHA®-2940/4/W  
AHA®-3940/W

Logicraft Information Systems
22 Cotton Road
Nashua, NH 03063
Phone	603-880-0300
Fax	(603) 880-7229
Toll free	800-880-5644
E-mail	sales@logicraft.com
URL	http://www.logicraft.com

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

IMAGING SOLUTIONS	109

Winter, 1996

Logicraft Information Systems

	FastCD™, LanCD

	FastCD™ is an option available with Logicraft's LanCD™ networking software for providing multiple concurrent access to CD-ROM 
	applications in a multi-platform, multi-protocol networking environment.  FastCD creates "virtual CD-ROM discs" on fast, high 
	performance SCSI hard drives by caching the entire contents of a CD-ROM in its native format onto a FastCD partition of the hard disk, 
	providing users with easy access to their CD-ROM applications at hard disk speeds up to 300 times faster than standard CD-ROM drives.  
	FastCD software includes comprehensive status reports, multimedia support, and asynchronous disk access for higher throughput during 
	multiple concurrent accessing.

Host Adapters Tested
AHA®-1540/2/F/P  
AHA®-1740/2/4  
AHA®-2740/2/4/T/W  
AHA®-2940/4/W  
AHA®-3940/W

Logicraft Information Systems
22 Cotton Road
Nashua, NH 03063
Phone	603-880-0300
Fax	(603) 880-7229
Toll free	800-880-5644
E-mail	sales@logicraft.com
URL	http://www.logicraft.com

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

IMAGING SOLUTIONS	110

Winter, 1996

Logicraft Information Systems

	CDexecutive™ CD-ROM Network Server

	The CDexecutive /XF5500 CD-ROM network server provides a turnkey solution for multiple concurrent accesses to CD-ROM applications in a 
	multi-platform, multi-protocol environment.  The Pentium™ based XF hardware architecture is bundled with Logicraft's high performance 
	CDexecutive Management Center software that automatically monitors and manages CD-ROM applications as a background Windows NT™ service.
	  Client support includes Windows® 95, Windows® for Workgroups, Macintosh® and NetWare clients.  The XF server holds up to 14 SCSI 
	devices and comes equipped with IDE hard drive, network interface card, floppy drive and SCSI host adapters.  It runs at 120MHz, has 
	32MB of RAM and supports up to 56 SCSI devices.

Host Adapters Tested
AHA®-2740/2/4/T/W

Logicraft Information Systems
22 Cotton Road
Nashua, NH 03063
Phone	603-880-0300
Fax	(603) 880-7229
Toll free	800-880-5644
E-mail	sales@logicraft.com
URL	http://www.logicraft.com

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

IMAGING SOLUTIONS	111

Winter, 1996

Logicraft Information Systems

	LanCD™ CD-ROM Network Servers

	The LanCD/XF family of CD-ROM network servers provides a turnkey solution for multiple concurrent accesses to CD-ROM applications in a 
	multi-platform, multi-protocol environment.  The Pentium™ based XF hardware architecture is bundled with Logicraft's high-performance 
	LanCD and FastCD™ software that supports DOS, Windows® and Windows® 95 clients.  Optional support is available for Windows NT® and 
	Macintosh clients.  Each chassis holds up to 14 SCSI devices and comes equipped with IDE hard drive, network interface card, floppy 
	drive and SCSI host adapters.  The XF5300 runs at 75MHz, has 16MB of RAM and expands to 28 drives.  The XF5500 runs at 120MHz, has 32MB
	 and supports up to 56 drives.

Host Adapters Tested
AHA®-1520/2  
AHA®-1540/2/F/P  
AHA®-1640  
AHA®-1740/2/4  
AHA®-2740/2/4/T/W  
AHA®-2940/4/W  
AHA®-3940/W

Logicraft Information Systems
22 Cotton Road
Nashua, NH 03063
Phone	603-880-0300
Fax	(603) 880-7229
Toll free	800-880-5644
E-mail	sales@logicraft.com
URL	http://www.logicraft.com

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

IMAGING SOLUTIONS	112

Winter, 1996

Lookout Geophysical Company

	SeiScope/SeaScope

	Subsurface geo-technical images (Seismic, sonar, ground penetrating radar, etc.) are processed and displayed in real time and written 
	to SCSI tape drives (4mm, 8mm, DLT, 3480) and processed from tape after acquisition.

Host Adapters Tested
AHA®-1520/2  
AHA®-1540/2/F/P  
AHA®-2940/4/W  
AHA®-2940/4/U/UW

Lookout Geophysical Company
433 Park Point Drive, Suite 250
Golden, CO 80401
USA
Phone	303-526-5108
Fax	303-526-5150
E-mail	vgoebel@aol.com

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

IMAGING SOLUTIONS	113

Winter, 1996

Lynx System Developers, Inc.

	FinishLynx

	FinishLynx™ is the first film-less, fully digital “photo-finish” system.  FinishLynx is a SCSI peripheral which, when attached to your 
	PC, allows the user to time and generate results for track & field, cycling, speedskating, horse racing, and other competitive events. 
	 On-screen image processing without developing film, along with instant integration into an entrant database allow users to generate 
	results quickly and accurately.  The high bandwidth of SCSI allows input from multiple image sources to be captured simultaneously and 
	in real time.  Use of the SCSI standard enables easy platform independence.

Host Adapters Tested
APA™-1460  
AHA®-1520/2

Lynx System Developers, Inc.
175 N New Boston Street
Woburn, MA 01801
USA
Phone	(617) 935-6959
Fax	(617) 938-0580
Toll free	(800) 989-LYNX
E-mail	info@finishlynx.com
URL	http://www.finishlynx.com

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

IMAGING SOLUTIONS	114

Winter, 1996

Maxoptix Corporation

	T4-2600

	The T4-2600 is a new 5.25" multifunction optical disk drive with 2.6GB capacity.  It provides unlimited transportable storage at an 
	excellent value, offering unparalleled reliability, a fast seek rate up to 4.0 MB/second transfer rate and with 1 read/write cache, it 
	delivers an outstanding performance.  The T4-2600 drive conforms to ISO specifications and accepts three ISO standard media formats - 
	2.6GB, 1.3GB and 650MB.  
	This drive is reliable, affordable and high performance.  The media can be written and erased more than 10,000,000 times.

Host Adapters Tested
AHA®-1540/2/F/P  
AHA®-1640  
AHA®-1740/2/4  
AHA®-2740/2/4/T/W  
AHA®-2940/4/W  
AHA®-3940/W

Maxoptix Corporation
3342 Gateway Blvd.
Fremont, CA 94538
USA
Phone	(510) 353-9700
Fax	(510) 353-1845
Toll free	(800) 848-3092

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

IMAGING SOLUTIONS	115

Winter, 1996

Maxoptix Corporation

	MaxLyb

	The Maxoptix MaxLyb family of optical auto changers utilizes the T4-2600 drives to deliver high performance and reliable 
	specifications.  The MaxLyb family covers a wide range of capacities - 26GB to over 600GB, which ensures the most useful library is 
	available for a variety of applications.  
	  
	With the MaxLyb family of optical storage libraries, Maxoptix offers the widest selection of optical library solutions and fills the 
	price-performance gaps left by other storage technologies.  With the fastest on-line access to stored data and information, they are 
	the logical choice for those who need top performance, demonstrated reliability and future expandability at competitive prices.

Host Adapters Tested
AHA®-1540/2/F/P  
AHA®-1640  
AHA®-1740/2/4  
AHA®-2740/2/4/T/W  
AHA®-2940/4/W  
AHA®-3940/W

Maxoptix Corporation
3342 Gateway Blvd.
Fremont, CA 94538
USA
Phone	(510) 353-9700
Fax	(510) 353-1845
Toll free	(800) 848-3092

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

IMAGING SOLUTIONS	116

Winter, 1996

Optical Document Technologies

	DocuManager

	DocuManager® is a document management solution.  DocuManager software provides GUI-based document scanning, indexing, storage, and 
	retrieval services.  It has an optional set of image-enabling customization tools called KeyStuffer.  Typically, the software is 
	integrated with high performance hardware to provide a complete system.  With DocuManager, customers transform paper documents into 
	electronic images, and then create automated work processes or filing systems.  The primary benefits of using DocuManager are 
	significant cost savings and increased process productivity.

Host Adapters Tested
AHA®-1520/2  
AHA®-1540/2/F/P  
AHA®-1740/2/4  
AHA®-2740/2/4/T/W

Optical Document Technologies
9390 Research Blvd., Suite 415
Austin, TX 78759
Phone	512-794-9829
Fax	(512) 794-0393

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

IMAGING SOLUTIONS	117

Winter, 1996

Optical Document Technologies

	JBC Optical Disk Manager

	JBC™ is a Windows NT based-application for optical jukebox control.  JBC is an API-based system that provides highly optimized sector 
	level writing to optical media.  This provides outstanding system throughput regardless of the number of image files on the media.  JBC
	 manages all aspects of the storage and retrieval of data on optical media over networks and internetworks, including data queuing and 
	distributed caching.

Host Adapters Tested
AHA®-1520/2  
AHA®-1540/2/F/P  
AHA®-1740/2/4  
AHA®-2740/2/4/T/W  
AHA®-2940/4/W

Optical Document Technologies
9390 Research Blvd., Suite 415
Austin, TX 78759
Phone	512-794-9829
Fax	(512) 794-0393

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

IMAGING SOLUTIONS	118

Winter, 1996

Paabo Consulting Group AB

	JVC CD-R

	The JVC CD-R is a CD-ROM burner/reader for integration with PCG Software into PC -- networks or standalone machines. The JVC CD-R can 
	be used directly for MPEG-1 compressed video recording. Playback is done over the SCSI interface.

Host Adapters Tested
AHA®-1510  
AVA™-1515  
AHA®-1540/2/F/P  
AHA®-2740/2/4/T/W  
AHA®-2940/4/W

Paabo Consulting Group AB
P.O. Box 6144, Nya Tanneforsvagen 55
S-58006 Linkoping,
Sweden
Phone	46-13-100-500
Fax	46-13-103-013
E-mail	info@pcgab.se
URL	http://www.pcgab.se

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

IMAGING SOLUTIONS	119

Winter, 1996

Paperclip Imaging Software, Inc.

	PaperClip

	PaperClip for Windows is a Windows-based software application for standalone-and network-based users.  It provides an integrated 
	solution to easily organize and manage a wide range of information, including word processing, spreadsheet and multimedia files, faxes,
	 and scanned documents - all within a user-definable folder structure.  
	  
	Users can retrieve documents and folders directly from any off-the-shelf or custom-built application, as well as via host-based 
	terminal emulation programs.  An intuitive file cabinet interface provides a seamless system to centrally store information scattered 
	throughout directories and in file cabinets.  Application files and scanned documents stored in PaperClip can be viewed on-the-fly, 
	without manually launching the associated software.

Host Adapters Tested
AHA®-1520/2  
AHA®-1540/2/F/P

Paperclip Imaging Software, Inc.
3 University Plaza
Hackensack, NJ 07601
Phone	201-487-3503
Fax	201-487-0613

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

IMAGING SOLUTIONS	120

Winter, 1996

Paperless Corporation

	Paperless Filer 2.3

	PaperLess Filer™ 2.3 electronic document storage software allows MS-DOS PC users to manage, display, print and FAX scanned document 
	images.  PF 2.3 software works with the user’s PC to electronically file large quantities of paper or FAX documents.  PF 2.3 uses 
	intelligent software compression, enabling documents to be compressed while being scanned in order to reduce storage requirements.  PF 
	2.3 can decompress and display documents instantly.  Features include zoom, pan, and rotate on display; plain paper output; optical 
	disk support; FAX board support; and TIFF/PCX file import/export.  PF 2.3 supports all MS-DOS-compatible storage devices, and more than
	 20 different scanners.

Host Adapters Tested
APA™-348  
AHA®-1540/2/F/P  
AHA®-2940/4/W

Paperless Corporation
1750 North Collins, Suite 104
Richardson, TX 75080
US
Phone	(214) 235-4008
Fax	(214) 680-2566
Toll free	(800) 658-6486
E-mail	paper@onramp.net
URL	http://www.onramp.net/~ paper

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

IMAGING SOLUTIONS	121

Winter, 1996

Paperless Corporation

	Paperless Filer Document Imaging Toolkit

	PaperLess Filer™ Document Imaging Toolkit™ allows developers of Clipper, FoxPro and other application programs to add complete document
	 imaging to their applications.  The toolkit is a series of MS-DOS-compatible EXE files (modules) that perform various functions.  
	These modules create, display or print compressed bi-tonal image files in Paperless Corporation’s proprietary file format.  They scan 
	and compress document images on over 40 scanners.  They also display document images in graphics mode; print document images on laser 
	printers; and export/import TIFF, PCX and DCX images.  Full network support and file sharing are provided.

Host Adapters Tested
APA™-348  
AHA®-1540/2/F/P  
AHA®-2940/4/W

Paperless Corporation
1750 North Collins, Suite 104
Richardson, TX 75080
US
Phone	(214) 235-4008
Fax	(214) 680-2566
Toll free	(800) 658-6486
E-mail	paper@onramp.net
URL	http://www.onramp.net/~ paper

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

IMAGING SOLUTIONS	122

Winter, 1996

Paperless Corporation

	PaperLess Filer Document Imaging Toolkit for WIN32

	PaperLess Filer™ 2.3 Document Imaging Toolkit for WIN32 allows developers of Windows NT and Windows 95 applications to add imaging 
	capabilites quickly and easily.  The Toolkit consists of OLE Custom Controls and Applications that may be called from any Windows 32 
	bit application.  Offering both OLE Automation and OCX controls allows the developer to add powerful multi-threaded 32 bit imaging 
	software without relying on 16 bit software.   
	  
	Features include support of Fujitsu, Ricoh and other high speed SCSI scanners, as well as TWAIN based scanners.  The Toolkit also 
	includes Windows 95-style controls to display and print images under full application control.  The high speed built-in compression and
	 decompression software supports CCITT Group III and IV fax, as well as TIFF, DCX and Microsoft At-Work Fax file formats.  Full network
	 support and file sharing is supported.

Host Adapters Tested
APA™-348  
AHA®-1540/2/F/P  
AHA®-2940/4/W

Paperless Corporation
1750 North Collins, Suite 104
Richardson, TX 75080
US
Phone	(214) 235-4008
Fax	(214) 680-2566
Toll free	(800) 658-6486
E-mail	paper@onramp.net
URL	http://www.onramp.net/~ paper

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

IMAGING SOLUTIONS	123

Winter, 1996

Paperless Corporation

	PaperLess Filer  Document Viewer

	PaperLess Filer Document Viewer™ can scan, display and print document images.  It can be run as a stand-alone application, as an 
	in-place OLE object, or driven from another program using OLE Automation.  Programs that support OLE can insert imaging objects by 
	using PFDV.  When invoked from OLE, PFDV adds its imaging capabilities to the application's menus and toolbars.  PFDV supports SCSI 
	scanners thru ASPI.  Any number of different scan settings can be saved and loaded by type of document.  PFDV features the Windows 95 
	style user interface; including dockable tool-bars, property sheets, drag and drop, context sensitive help and long file names.

Host Adapters Tested
APA™-348  
AHA®-1540/2/F/P  
AHA®-2940/4/W

Paperless Corporation
1750 North Collins, Suite 104
Richardson, TX 75080
US
Phone	(214) 235-4008
Fax	(214) 680-2566
Toll free	(800) 658-6486
E-mail	paper@onramp.net
URL	http://www.onramp.net/~ paper

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

IMAGING SOLUTIONS	124

Winter, 1996

Pioneer Hi-Fi (GB) Ltd.

	PIONEER

	Pioneer, the leading manufacturer of optical disc technology has developed a solution utilizing it's high storage CD-ROM autochanger.  
	This solution provides stored video clips directly to designated PC's.  The Video Browse Server enables users to view the whole of a 
	video library on a PC.  This application has a user friendly and logical GUI.  The video clips never physically leave the library, 
	hence no time lost tracing material.  All of the video is held on CD-ROMs locked away in a 500 disk autochanger.  Initially by the use 
	of alphanumeric entries a search can be narrowed down to several titles. A selected title gives further indexed information on the clip
	 and also more importantly at least two thumbnails.  The chosen clip can then be viewed on a PC terminal.  By selecting various clips 
	the user automatically generates a clip list.  This file can then be sent to the compiling station on the network.  The compiling 
	station then assembles the request on any chosen broadcast medium- D1, D2, D3, D5, Digital Betacam, Betacam, Disc etc.

Host Adapters Tested
AHA®-2940/4/U/UW  
AHA®-3940/W  
AHA®-3940U/UW

Pioneer Hi-Fi (GB) Ltd.
Pioneer House, Hollybush Hill
Stoke Poges, Slough SL2 4QP
England
Phone	144-01753-789732
Fax	144-01753-789539

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

MACINTOSH SOLUTIONS	125

Winter, 1996

Digital Instrumentation Technology

	TransferPro

	TransferPro™ allows you to read and write Macintosh files directly from your PC.  TransferPro is a fast and easy file transfer 
	solution.  TransferPro reads, writes and formats Macintosh media including SyQuest™ , Bernoulli ™, Iomega™  Zip, data shuttle drives, 
	Pinnacle Micro™, Sony™,  MOST™, Ricoh™  and other magneto-optical drives, SCSI hard drives and CD-ROM drives.  TransferPro features 
	graphics viewers and converters and a high quality, easy to use Windows-based installer with an automatic configuration feature.  
	TransferPro is available for Windows, Windows 95 and Windows NT.

Host Adapters Tested
APA™-1460  
AVA™-1505  
AHA®-1510  
AVA™-1515  
AHA®-1520/2  
AHA®-1530/2P  
AHA®-1540/2/F/P  
AHA®-1640  
AHA®-1740/2/4  
AHA®-2740/2/4/T/W  
AHA®-2840/2VL  
AHA®-2940/4/W  
AHA®-3940/W

Digital Instrumentation Technology
127 Eastgate Dr. #20500
Los Alamos, NM 87544
Phone	(505) 662-1459
Fax	(505) 662-0897
Toll free	(800) 467-1459
E-mail	tpro-request@dit.com
URL	hhttp://www.dit.com

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

MACINTOSH SOLUTIONS	126

Winter, 1996

Logicraft Information Systems

	FastCD™, LanCD

	FastCD™ is an option available with Logicraft's LanCD™ networking software for providing multiple concurrent access to CD-ROM 
	applications in a multi-platform, multi-protocol networking environment.  FastCD creates "virtual CD-ROM discs" on fast, high 
	performance SCSI hard drives by caching the entire contents of a CD-ROM in its native format onto a FastCD partition of the hard disk, 
	providing users with easy access to their CD-ROM applications at hard disk speeds up to 300 times faster than standard CD-ROM drives.  
	FastCD software includes comprehensive status reports, multimedia support, and asynchronous disk access for higher throughput during 
	multiple concurrent accessing.

Host Adapters Tested
AHA®-1540/2/F/P  
AHA®-1740/2/4  
AHA®-2740/2/4/T/W  
AHA®-2940/4/W  
AHA®-3940/W

Logicraft Information Systems
22 Cotton Road
Nashua, NH 03063
Phone	603-880-0300
Fax	(603) 880-7229
Toll free	800-880-5644
E-mail	sales@logicraft.com
URL	http://www.logicraft.com

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

MACINTOSH SOLUTIONS	127

Winter, 1996

Logicraft Information Systems

	CDexecutive™ CD-ROM Network Server

	The CDexecutive /XF5500 CD-ROM network server provides a turnkey solution for multiple concurrent accesses to CD-ROM applications in a 
	multi-platform, multi-protocol environment.  The Pentium™ based XF hardware architecture is bundled with Logicraft's high performance 
	CDexecutive Management Center software that automatically monitors and manages CD-ROM applications as a background Windows NT™ service.
	  Client support includes Windows® 95, Windows® for Workgroups, Macintosh® and NetWare clients.  The XF server holds up to 14 SCSI 
	devices and comes equipped with IDE hard drive, network interface card, floppy drive and SCSI host adapters.  It runs at 120MHz, has 
	32MB of RAM and supports up to 56 SCSI devices.

Host Adapters Tested
AHA®-2740/2/4/T/W

Logicraft Information Systems
22 Cotton Road
Nashua, NH 03063
Phone	603-880-0300
Fax	(603) 880-7229
Toll free	800-880-5644
E-mail	sales@logicraft.com
URL	http://www.logicraft.com

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

MACINTOSH SOLUTIONS	128

Winter, 1996

Logicraft Information Systems

	LanCD™ CD-ROM Network Servers

	The LanCD/XF family of CD-ROM network servers provides a turnkey solution for multiple concurrent accesses to CD-ROM applications in a 
	multi-platform, multi-protocol environment.  The Pentium™ based XF hardware architecture is bundled with Logicraft's high-performance 
	LanCD and FastCD™ software that supports DOS, Windows® and Windows® 95 clients.  Optional support is available for Windows NT® and 
	Macintosh clients.  Each chassis holds up to 14 SCSI devices and comes equipped with IDE hard drive, network interface card, floppy 
	drive and SCSI host adapters.  The XF5300 runs at 75MHz, has 16MB of RAM and expands to 28 drives.  The XF5500 runs at 120MHz, has 32MB
	 and supports up to 56 drives.

Host Adapters Tested
AHA®-1520/2  
AHA®-1540/2/F/P  
AHA®-1640  
AHA®-1740/2/4  
AHA®-2740/2/4/T/W  
AHA®-2940/4/W  
AHA®-3940/W

Logicraft Information Systems
22 Cotton Road
Nashua, NH 03063
Phone	603-880-0300
Fax	(603) 880-7229
Toll free	800-880-5644
E-mail	sales@logicraft.com
URL	http://www.logicraft.com

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

MULTIMEDIA SOLUTIONS	129

Winter, 1996

Adaptec, Inc.

	ADAPTEC® EZ-SCSI®

	If you have, or are planning to add, SCSI peripherals like tape or disk drives, CD-ROM drives, recordable CD-R drives, magneto-optical 
	drives, or scanners, Adaptec EZ-SCSI® software provides everything you need to manage and take full advantage of each device.  
	  
	Adaptec EZ-SCSI software is a suite of 32-bit practical applications and power tools that are remarkably easy to install and use.  
	Simple desktop controls give you immediate access to any fuction.  A unique online tutorial explains everything you need to know about 
	SCSI in easy-to-understand terms.  
	  
	Key benefits:  
	* Easiest way to manage SCSI peripherals  
	* For Windows operating systems  
	* Includes these practical applications:  Adaptec Easy-CD Backup™, QuickScan™, Audio CD player, Photo CD Viewer, CD Writer, and CD 
	Copier  
	* Includes these powerful tools:  SCSI Explorer™ (Power Management, SCSI Interrogator™, Read/Write Disk Cashe tool), SCSI Tutor™, SCSI 
	Bench™ and Drive Light™.

Host Adapters Tested
APA™-348  
APA™-358  
APA™-1460  
AVA™-1505  
AHA®-1510  
AVA™-1515  
AHA®-1520/2  
AHA®-1530/2P  
AHA®-1540/2/F/P  
AHA®-1640  
AHA®-1740/2/4  
AHA®-2740/2/4/T/W  
AHA®-2840/2VL  
AHA®-2920  
AHA®-2940/4/W  
AHA®-2940AU  
AHA®-3940/W  
AHA®-3940U/UW

Adaptec, Inc.
691 S Milpitas Blvd
Milpitas, CA
USA
Phone	1-800-934-2766
Fax	408-262-2533
Toll free	1-800-934-2766
E-mail	sales@adaptec.com
URL	http://www.adaptec.com

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

MULTIMEDIA SOLUTIONS	130

Winter, 1996

Adaptec, Inc.

	EZ-CD Pro, EZ-CD Pro MM

	Easy CD Pro™ and Easy CD Pro MM™ are complete software products for creating, testing and simulating both real and virtual ISO 9660 
	images for CD-ROM, and for creating CD audio and mixed mode compact disks.  Complete compatibility with Windows 3.1®, including "drag 
	and drop" direct from File Manager, makes creating CD's easy, even for absolute beginners.

Host Adapters Tested
APA™-348  
APA™-358  
AHA®-1510  
AHA®-1520/2  
AHA®-1640

Adaptec, Inc.
691 S Milpitas Blvd
Milpitas, CA
USA
Phone	1-800-934-2766
Fax	408-262-2533
Toll free	1-800-934-2766
E-mail	sales@adaptec.com
URL	http://www.adaptec.com

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

MULTIMEDIA SOLUTIONS	131

Winter, 1996

Corel Corporation

	CorelSCSI

	CorelSCSI® software provides easy connection of SCSI devices. CorelSCSI includes device drivers for virtually every SCSI peripheral on 
	the market. CorelSCSI software also includes: Corel CD-Audio, Corel Tape Backup software, SCSI Tools for Windows and more. CorelSCSI is
	 multi-platform, with operating system support for DOS, Windows, OS/2 and Novell® NetWare 386. CorelSCSI is included in Adaptec’s SCSI 
	Direction® Plus kit and SCSI Master™ Plus kit.

Host Adapters Tested
AHA®-1520/2  
AHA®-1540/2/F/P  
AHA®-1640

Corel Corporation
1600 Carling Avenue
Ottawa, Ontario K1Z 8R7
Canada
Phone	(613) 728-8200
Fax	(613) 728-9790
Toll free	(800) 836-7274

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

MULTIMEDIA SOLUTIONS	132

Winter, 1996

Corel Corporation

	CorelSCSI Pro

	CorelSCSI Pro® is a high-performance software product designed to maximize SCSI performance.  CorelSCSI Pro provides: support for SCSI 
	scanners to scan images into any TWAIN-compliant graphics program; a CD-ROM server application that allows network users to retrieve 
	recently-accessed information with essentially no delay; and a utility that writes information to a compact disc using a CD-Recorder. 
	These features and others are available using an intuitive and friendly interface.

Host Adapters Tested
AHA®-1520/2  
AHA®-1540/2/F/P  
AHA®-1640

Corel Corporation
1600 Carling Avenue
Ottawa, Ontario K1Z 8R7
Canada
Phone	(613) 728-8200
Fax	(613) 728-9790
Toll free	(800) 836-7274

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

MULTIMEDIA SOLUTIONS	133

Winter, 1996

Delphi Data

	RAIDer Writable CD Arrays  
	RAIDer Writable CD Arrays

	The RAIDer™ series of CD-ROM arrays provide a unique hardware solution for minicomputer and network systems. Configurations include 
	multi-SCSI ID or LUNs with a maximum of 56 drives per controller.  
	  
	The RAIDer series of Writable CD disk arrays provide a unique hardware solution for the production of CDs. The system can be configured
	 for short run duplication of CDs. Configurations can include a mix of hard drives, EO transports, tape unit and multiple CD writers. 
	The system can perform offline from any source to multiple targets.  
	  
	All systems include an integrated data cache, up to 256Mb per CacheBox, which greatly improves performance.

Host Adapters Tested
AHA®-1510  
AHA®-1520/2  
AHA®-1740/2/4  
AHA®-2740/2/4/T/W  
AHA®-2840/2VL  
AHA®-2940/4/W

Delphi Data
9069 Cajalco Road
Corona, CA 91719
Phone	(909) 279-7955
Fax	(909) 279-7957
Toll free	(800) -DELPHI5
E-mail	76470.1544@compuserve.com

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

MULTIMEDIA SOLUTIONS	134

Winter, 1996

HCL Hewlett Packard Ltd.

	Busy Bee and Meteor

	The HCL-Hewlett Packard Busy Bee and Meteor Systems are developed in India for use in the Indian market.  They are highly scalable 
	designs starting from home PC low-end configurations to large business UNIX and NetWare servers.

Host Adapters Tested
AHA®-1520/2  
AHA®-1540/2/F/P  
AHA®-1740/2/4  
AHA®-2740/2/4/T/W  
AHA®-2940/4/W  
AHA®-2940/4/U/UW

HCL Hewlett Packard Ltd.
E4, E5, E6 Sector 11, Noida
Dist Ghaziabad,  201301
India
Phone	91-11-8531353
Fax	91-11-8521113

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

MULTIMEDIA SOLUTIONS	135

Winter, 1996

Logicraft Information Systems

	The Jukebox Manager

	The Jukebox Manager™ option for Logicraft's LanCD™ network server software provides a versatile solution for networked access to 
	archived CD-ROM storage.  It is modular in design, hardware independent and non-vendor specific for jukebox support.  Features include 
	Document Image Management, static directory or platter caching and DDC (dynamic hard disk cache), asynchronous access, multiple jukebox
	 support, Intelligent Optical Reader Selection, local on-line management, and support for up to 1280 platters and 56 readers per LanCD 
	server.  With up to 10 servers per client, each user could have access to more than 12 thousand CD-ROM discs.

Host Adapters Tested
AHA®-1540/2/F/P  
AHA®-1740/2/4  
AHA®-2740/2/4/T/W  
AHA®-2940/4/W  
AHA®-3940/W

Logicraft Information Systems
22 Cotton Road
Nashua, NH 03063
Phone	603-880-0300
Fax	(603) 880-7229
Toll free	800-880-5644
E-mail	sales@logicraft.com
URL	http://www.logicraft.com

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

MULTIMEDIA SOLUTIONS	136

Winter, 1996

Logicraft Information Systems

	FastCD™, LanCD

	FastCD™ is an option available with Logicraft's LanCD™ networking software for providing multiple concurrent access to CD-ROM 
	applications in a multi-platform, multi-protocol networking environment.  FastCD creates "virtual CD-ROM discs" on fast, high 
	performance SCSI hard drives by caching the entire contents of a CD-ROM in its native format onto a FastCD partition of the hard disk, 
	providing users with easy access to their CD-ROM applications at hard disk speeds up to 300 times faster than standard CD-ROM drives.  
	FastCD software includes comprehensive status reports, multimedia support, and asynchronous disk access for higher throughput during 
	multiple concurrent accessing.

Host Adapters Tested
AHA®-1540/2/F/P  
AHA®-1740/2/4  
AHA®-2740/2/4/T/W  
AHA®-2940/4/W  
AHA®-3940/W

Logicraft Information Systems
22 Cotton Road
Nashua, NH 03063
Phone	603-880-0300
Fax	(603) 880-7229
Toll free	800-880-5644
E-mail	sales@logicraft.com
URL	http://www.logicraft.com

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

MULTIMEDIA SOLUTIONS	137

Winter, 1996

Logicraft Information Systems

	CDexecutive™ CD-ROM Network Server

	The CDexecutive /XF5500 CD-ROM network server provides a turnkey solution for multiple concurrent accesses to CD-ROM applications in a 
	multi-platform, multi-protocol environment.  The Pentium™ based XF hardware architecture is bundled with Logicraft's high performance 
	CDexecutive Management Center software that automatically monitors and manages CD-ROM applications as a background Windows NT™ service.
	  Client support includes Windows® 95, Windows® for Workgroups, Macintosh® and NetWare clients.  The XF server holds up to 14 SCSI 
	devices and comes equipped with IDE hard drive, network interface card, floppy drive and SCSI host adapters.  It runs at 120MHz, has 
	32MB of RAM and supports up to 56 SCSI devices.

Host Adapters Tested
AHA®-2740/2/4/T/W

Logicraft Information Systems
22 Cotton Road
Nashua, NH 03063
Phone	603-880-0300
Fax	(603) 880-7229
Toll free	800-880-5644
E-mail	sales@logicraft.com
URL	http://www.logicraft.com

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

MULTIMEDIA SOLUTIONS	138

Winter, 1996

Logicraft Information Systems

	LanCD™ CD-ROM Network Servers

	The LanCD/XF family of CD-ROM network servers provides a turnkey solution for multiple concurrent accesses to CD-ROM applications in a 
	multi-platform, multi-protocol environment.  The Pentium™ based XF hardware architecture is bundled with Logicraft's high-performance 
	LanCD and FastCD™ software that supports DOS, Windows® and Windows® 95 clients.  Optional support is available for Windows NT® and 
	Macintosh clients.  Each chassis holds up to 14 SCSI devices and comes equipped with IDE hard drive, network interface card, floppy 
	drive and SCSI host adapters.  The XF5300 runs at 75MHz, has 16MB of RAM and expands to 28 drives.  The XF5500 runs at 120MHz, has 32MB
	 and supports up to 56 drives.

Host Adapters Tested
AHA®-1520/2  
AHA®-1540/2/F/P  
AHA®-1640  
AHA®-1740/2/4  
AHA®-2740/2/4/T/W  
AHA®-2940/4/W  
AHA®-3940/W

Logicraft Information Systems
22 Cotton Road
Nashua, NH 03063
Phone	603-880-0300
Fax	(603) 880-7229
Toll free	800-880-5644
E-mail	sales@logicraft.com
URL	http://www.logicraft.com

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

MULTIMEDIA SOLUTIONS	139

Winter, 1996

Optical Media International

	TOPiX

	TOPiX™ CD publishing software provides the ideal solution for getting software, databases, multimedia applications, images, and audio 
	onto a CD or premaster tape.  TOPiX supports the creation of ISO 9660, Hybrid (ISO + HFS) or disk image (such as Macintosh HFS) 
	formatted CDs to give you the option of preserving the native file system or taking advantage of the universal platform characteristics
	 of the ISO format.  The system is available on DOS/Windows, Macintosh, and UNIX workstations.

Host Adapters Tested
AHA®-1540/2/F/P  
AHA®-1640  
AHA®-1740/2/4  
AHA®-2840/2VL

Optical Media International
180 Knowles Drive
Los Gatos, CA 95030
USA
Phone	(408) 376-3511
Fax	(408) 376-3519
Toll free	(800) 347-2664

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

MULTIMEDIA SOLUTIONS	140

Winter, 1996

Optisys

	GlobalNet

	GlobalNet™ storage servers provide Novell Network access to optical jukeboxes, including CD-ROM, Erasable and WORM (Write Once Read 
	Many) technologies.  Notable for its ease of installation, use and its speed.

Host Adapters Tested
AHA®-1540/2/F/P  
AHA®-2840/2VL  
AHA®-3940/W

Optisys
9250 North 43rd Avenue, Suite 12
Glendale, AZ 85302
Phone	(602) 997-9699
Fax	(602) 944-4051
Toll free	(800) 327-1271

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

MULTIMEDIA SOLUTIONS	141

Winter, 1996

Pinnacle Systems, Inc.

	Alladin

	Alladin™ is an open architecture, multifunctional video tool. This dependable PC peripheral processes high quality, full resolution 
	video in real time. For making video transitions, Alladin includes a seven input switcher and true 3D DVE with curvilinear effects. Add
	 graphics and titles to your video with titling, character generation, still store, paint, 3D modeling and animation - all with 
	built-in Alpha channel.  Alladin’s layering capabilities include full linear input key, as well as luminance and chrominance keying.  
	Altogether, Alladin can process four video layers in a single pass.  And, since you can customize all Alladin effects, your video 
	productions will never have that “pre-canned” look.

Host Adapters Tested
AHA®-1510  
AVA™-1515  
AHA®-1520/2  
AHA®-1540/2/F/P  
AHA®-2740/2/4/T/W  
AHA®-2840/2VL  
AHA®-2940/4/W

Pinnacle Systems, Inc.
870 West Maude Avenue
Sunnyvale, CA 94086
Phone	(408) 720-9669
Fax	(408) 720-9674

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

MULTIMEDIA SOLUTIONS	142

Winter, 1996

Pioneer Hi-Fi (GB) Ltd.

	PIONEER

	Pioneer, the leading manufacturer of optical disc technology has developed a solution utilizing it's high storage CD-ROM autochanger.  
	This solution provides stored video clips directly to designated PC's.  The Video Browse Server enables users to view the whole of a 
	video library on a PC.  This application has a user friendly and logical GUI.  The video clips never physically leave the library, 
	hence no time lost tracing material.  All of the video is held on CD-ROMs locked away in a 500 disk autochanger.  Initially by the use 
	of alphanumeric entries a search can be narrowed down to several titles. A selected title gives further indexed information on the clip
	 and also more importantly at least two thumbnails.  The chosen clip can then be viewed on a PC terminal.  By selecting various clips 
	the user automatically generates a clip list.  This file can then be sent to the compiling station on the network.  The compiling 
	station then assembles the request on any chosen broadcast medium- D1, D2, D3, D5, Digital Betacam, Betacam, Disc etc.

Host Adapters Tested
AHA®-2940/4/U/UW  
AHA®-3940/W  
AHA®-3940U/UW

Pioneer Hi-Fi (GB) Ltd.
Pioneer House, Hollybush Hill
Stoke Poges, Slough SL2 4QP
England
Phone	144-01753-789732
Fax	144-01753-789539

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

MULTIMEDIA SOLUTIONS	143

Winter, 1996

Plasmon Data Ltd.

	DOS Manager!

	DOS Manager! provides single or multi jukebox support for WORM, rewritable, or multifunction units. File compatibility is offered with 
	Corel as well as ECMA. Full utilities are built in for jukebox and media management as well as worm audit features.

Host Adapters Tested
AHA®-1510  
AHA®-1520/2  
AHA®-1540/2/F/P  
AHA®-1640  
AHA®-1740/2/4

Plasmon Data Ltd.
Whiting Way
Melbourn, Herts SG8 6DN
ENGLAND
Phone	44 0 1763 262963
Fax	44 0 1763 264444

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

MULTIMEDIA SOLUTIONS	144

Winter, 1996

Plasmon Data Ltd.

	Multitasking Manager! for OS/2

	Multitasking Manager! for OS/2 provides single or multi jukebox support for worm, rewritable, or multifunction units. File 
	compatibility is offered with Corel as well as ECMA. Full utilities are built in for jukebox and media management as well as worm audit
	 features.

Host Adapters Tested
AHA®-1510  
AHA®-1520/2  
AHA®-1540/2/F/P  
AHA®-1640  
AHA®-1740/2/4

Plasmon Data Ltd.
Whiting Way
Melbourn, Herts SG8 6DN
ENGLAND
Phone	44 0 1763 262963
Fax	44 0 1763 264444

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

MULTIMEDIA SOLUTIONS	145

Winter, 1996

Steinberg Soft and Hardware GmbH

	Cubase

	Cubase is a professional music production tool integrating MIDI recording, notation editing and printout, and digital recording all 
	under one unified easy to use interface.

Host Adapters Tested
AVA™-1505  
AHA®-1510  
AVA™-1515  
AHA®-1520/2  
AHA®-1540/2/F/P  
AHA®-2840/2VL

Steinberg Soft and Hardware GmbH
Eiffe Str. 596
Hamburg,  20537
Germany
Phone	(040) 211-594
Fax	49 40 211-598

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

MULTIMEDIA SOLUTIONS	146

Winter, 1996

Vision Database Systems

	RAPIDCARD Photo Identification System

	RAPIDCARD software can capture color photos, store them in a dBase / Foxpro compatible database, in uncompressed or JPEG compressed 
	format, and print excellent photo quality ID cards directly to a plastic medium such as credit card.  Individual drivers or utilities 
	can be purchased as well as complete turnkey systems for universities, corporations and government entities. Requires low man-power but
	 high throughput. PhotoID creation under one badge per minute. Multiple printers and multiple workstations can be networked using 
	Novell or a similar network.

Host Adapters Tested
APA™-348  
AHA®-1510  
AHA®-1520/2  
AHA®-1530/2P  
AHA®-1540/2/F/P

Vision Database Systems
853 Donald Ross Road
Juno Beach, FL 33408
USA
Phone	(407) 694-2211
Fax	(407) 694-2220
E-mail	73302.3133@compuserve.com

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

MULTIUSER/NETWORKING SOLUTIONS	147

Winter, 1996

Adaptec, Inc.

	ADAPTEC® CI/O™

	With easy to use Adaptec® CI/O™ software, managers can monitor all SCSI peripheral devices connected to servers by Adaptec® host 
	adapters.    
	  
	Using Adaptec® CI/O™ software on any Windows® client, managers can remotely monitor the I/O performance of any server on the network 
	from a single central location.  Managers can install the latest device drivers from a remote location as well.  
	  
	Adaptec® CI/O™ software automatically detects failure of any SCSI device on a network server and notifies the manager immediately.  
	With a clear view of I/O traffic, managers can spot bottlenecks and act quickly to balance I/O loads to optimize performance among SCSI
	 devices.  Adaptec® CI/O™ improves the manageability of any size network--from a single server to a global network.

Host Adapters Tested
AHA®-1540/2/F/P  
AHA®-2740/2/4/T/W  
AHA®-2840/2VL  
AHA®-2940/4/W  
AHA®-2940AU  
AHA®-3940/W  
AHA®-3980/5/W

Adaptec, Inc.
691 S Milpitas Blvd
Milpitas, CA
USA
Phone	1-800-934-2766
Fax	408-262-2533
Toll free	1-800-934-2766
E-mail	sales@adaptec.com
URL	http://www.adaptec.com

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

MULTIUSER/NETWORKING SOLUTIONS	148

Winter, 1996

Florida Datamation

	SBackup

	SBackup™ is a backup compatible SCSI tape backup software for QNX2. It supports DAT, 8mm and QIC format SCSI tape drives.

Host Adapters Tested
AHA®-1540/2/F/P  
AHA®-1640  
AHA®-1740/2/4

Florida Datamation
AMTEC Center, 6405 Congress Ave, Suite 140
Boca Raton, FL 33487
Phone	(407) 241-2966
Fax	(407) 241-3108
Toll free	(800) 642-5938
E-mail	sales@fdma.com

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

MULTIUSER/NETWORKING SOLUTIONS	149

Winter, 1996

Logicraft Information Systems

	The Jukebox Manager

	The Jukebox Manager™ option for Logicraft's LanCD™ network server software provides a versatile solution for networked access to 
	archived CD-ROM storage.  It is modular in design, hardware independent and non-vendor specific for jukebox support.  Features include 
	Document Image Management, static directory or platter caching and DDC (dynamic hard disk cache), asynchronous access, multiple jukebox
	 support, Intelligent Optical Reader Selection, local on-line management, and support for up to 1280 platters and 56 readers per LanCD 
	server.  With up to 10 servers per client, each user could have access to more than 12 thousand CD-ROM discs.

Host Adapters Tested
AHA®-1540/2/F/P  
AHA®-1740/2/4  
AHA®-2740/2/4/T/W  
AHA®-2940/4/W  
AHA®-3940/W

Logicraft Information Systems
22 Cotton Road
Nashua, NH 03063
Phone	603-880-0300
Fax	(603) 880-7229
Toll free	800-880-5644
E-mail	sales@logicraft.com
URL	http://www.logicraft.com

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

MULTIUSER/NETWORKING SOLUTIONS	150

Winter, 1996

Logicraft Information Systems

	FastCD™, LanCD

	FastCD™ is an option available with Logicraft's LanCD™ networking software for providing multiple concurrent access to CD-ROM 
	applications in a multi-platform, multi-protocol networking environment.  FastCD creates "virtual CD-ROM discs" on fast, high 
	performance SCSI hard drives by caching the entire contents of a CD-ROM in its native format onto a FastCD partition of the hard disk, 
	providing users with easy access to their CD-ROM applications at hard disk speeds up to 300 times faster than standard CD-ROM drives.  
	FastCD software includes comprehensive status reports, multimedia support, and asynchronous disk access for higher throughput during 
	multiple concurrent accessing.

Host Adapters Tested
AHA®-1540/2/F/P  
AHA®-1740/2/4  
AHA®-2740/2/4/T/W  
AHA®-2940/4/W  
AHA®-3940/W

Logicraft Information Systems
22 Cotton Road
Nashua, NH 03063
Phone	603-880-0300
Fax	(603) 880-7229
Toll free	800-880-5644
E-mail	sales@logicraft.com
URL	http://www.logicraft.com

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

MULTIUSER/NETWORKING SOLUTIONS	151

Winter, 1996

Logicraft Information Systems

	CDexecutive™ CD-ROM Network Server

	The CDexecutive /XF5500 CD-ROM network server provides a turnkey solution for multiple concurrent accesses to CD-ROM applications in a 
	multi-platform, multi-protocol environment.  The Pentium™ based XF hardware architecture is bundled with Logicraft's high performance 
	CDexecutive Management Center software that automatically monitors and manages CD-ROM applications as a background Windows NT™ service.
	  Client support includes Windows® 95, Windows® for Workgroups, Macintosh® and NetWare clients.  The XF server holds up to 14 SCSI 
	devices and comes equipped with IDE hard drive, network interface card, floppy drive and SCSI host adapters.  It runs at 120MHz, has 
	32MB of RAM and supports up to 56 SCSI devices.

Host Adapters Tested
AHA®-2740/2/4/T/W

Logicraft Information Systems
22 Cotton Road
Nashua, NH 03063
Phone	603-880-0300
Fax	(603) 880-7229
Toll free	800-880-5644
E-mail	sales@logicraft.com
URL	http://www.logicraft.com

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

MULTIUSER/NETWORKING SOLUTIONS	152

Winter, 1996

Logicraft Information Systems

	LanCD™ CD-ROM Network Servers

	The LanCD/XF family of CD-ROM network servers provides a turnkey solution for multiple concurrent accesses to CD-ROM applications in a 
	multi-platform, multi-protocol environment.  The Pentium™ based XF hardware architecture is bundled with Logicraft's high-performance 
	LanCD and FastCD™ software that supports DOS, Windows® and Windows® 95 clients.  Optional support is available for Windows NT® and 
	Macintosh clients.  Each chassis holds up to 14 SCSI devices and comes equipped with IDE hard drive, network interface card, floppy 
	drive and SCSI host adapters.  The XF5300 runs at 75MHz, has 16MB of RAM and expands to 28 drives.  The XF5500 runs at 120MHz, has 32MB
	 and supports up to 56 drives.

Host Adapters Tested
AHA®-1520/2  
AHA®-1540/2/F/P  
AHA®-1640  
AHA®-1740/2/4  
AHA®-2740/2/4/T/W  
AHA®-2940/4/W  
AHA®-3940/W

Logicraft Information Systems
22 Cotton Road
Nashua, NH 03063
Phone	603-880-0300
Fax	(603) 880-7229
Toll free	800-880-5644
E-mail	sales@logicraft.com
URL	http://www.logicraft.com

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

MULTIUSER/NETWORKING SOLUTIONS	153

Winter, 1996

Maxoptix Corporation

	T4-2600

	The T4-2600 is a new 5.25" multifunction optical disk drive with 2.6GB capacity.  It provides unlimited transportable storage at an 
	excellent value, offering unparalleled reliability, a fast seek rate up to 4.0 MB/second transfer rate and with 1 read/write cache, it 
	delivers an outstanding performance.  The T4-2600 drive conforms to ISO specifications and accepts three ISO standard media formats - 
	2.6GB, 1.3GB and 650MB.  
	This drive is reliable, affordable and high performance.  The media can be written and erased more than 10,000,000 times.

Host Adapters Tested
AHA®-1540/2/F/P  
AHA®-1640  
AHA®-1740/2/4  
AHA®-2740/2/4/T/W  
AHA®-2940/4/W  
AHA®-3940/W

Maxoptix Corporation
3342 Gateway Blvd.
Fremont, CA 94538
USA
Phone	(510) 353-9700
Fax	(510) 353-1845
Toll free	(800) 848-3092

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

MULTIUSER/NETWORKING SOLUTIONS	154

Winter, 1996

Maxoptix Corporation

	MaxLyb

	The Maxoptix MaxLyb family of optical auto changers utilizes the T4-2600 drives to deliver high performance and reliable 
	specifications.  The MaxLyb family covers a wide range of capacities - 26GB to over 600GB, which ensures the most useful library is 
	available for a variety of applications.  
	  
	With the MaxLyb family of optical storage libraries, Maxoptix offers the widest selection of optical library solutions and fills the 
	price-performance gaps left by other storage technologies.  With the fastest on-line access to stored data and information, they are 
	the logical choice for those who need top performance, demonstrated reliability and future expandability at competitive prices.

Host Adapters Tested
AHA®-1540/2/F/P  
AHA®-1640  
AHA®-1740/2/4  
AHA®-2740/2/4/T/W  
AHA®-2940/4/W  
AHA®-3940/W

Maxoptix Corporation
3342 Gateway Blvd.
Fremont, CA 94538
USA
Phone	(510) 353-9700
Fax	(510) 353-1845
Toll free	(800) 848-3092

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

MULTIUSER/NETWORKING SOLUTIONS	155

Winter, 1996

Meridian Data, Inc.

	CD Net Software

	CD Net™ software provides shared LAN access to CD-ROMs, high performance, integrated data management tools, support for high-capacity 
	configurations, and compatibility with all published CDs.  These features result in lower cost, increased utilization of shared CD 
	resources and easy operation.  Versions available for use with Novell NetWare 3.12 & 4.1, Microsoft NT 3.51, Vines 4.0+, and MS-DOS 
	based servers, with clients for Windows 95, Windows NT Workstation, Windows 3.x, MS-DOS, and Macintosh.

Host Adapters Tested
AHA®-1510  
AHA®-1520/2  
AHA®-1530/2P  
AHA®-1540/2/F/P  
AHA®-1640  
AHA®-1740/2/4  
AHA®-2740/2/4/T/W  
AHA®-2825VL  
AHA®-2840/2VL  
AHA®-2940/4/W  
AHA®-3940/W  
AHA®-3980/5/W

Meridian Data, Inc.
5615 Scotts Valley Drive
Scotts Valley, CA 95066
Phone	(408) 438-3100
Fax	(408) 438-6816
Toll free	(800) 767-2537
E-mail	info@meridian-data.com
URL	http://www.meridian-data.com

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

MULTIUSER/NETWORKING SOLUTIONS	156

Winter, 1996

Novell, Inc.

	NetWare

	Novell’s® NetWare® network computing products manage and control the sharing of services, data and applications among computer 
	workgroups, departmental networks and business-wide information systems. NetWare v4.1x provides interoperability, network services, 
	high performance, reliability and security in a network operating system. It utilizes a 32-bit, multitasking architecture and supports 
	DOS, Windows, Macintosh, OS/2 and UNIX workstations. In addition, NetWare v4.1x offers reliability features such as disk duplexing, 
	read-after-write verfication and disk mirroring.

Host Adapters Tested
AHA®-1540/2/F/P  
AHA®-1740/2/4  
AHA®-2840/2VL  
AHA®-2910A/Ai  
AHA®-2940/4/W  
AHA®-3940/W  
AHA®-3980/5/W

Novell, Inc.
122 East 1700 South
Provo, UT 84606
Phone	800-NETWARE
Fax	(801)861-2665
Toll free	800-NETWARE
E-mail	hbasup@novell.com
URL	www.novell.com

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

MULTIUSER/NETWORKING SOLUTIONS	157

Winter, 1996

Optisys

	GlobalNet

	GlobalNet™ storage servers provide Novell Network access to optical jukeboxes, including CD-ROM, Erasable and WORM (Write Once Read 
	Many) technologies.  Notable for its ease of installation, use and its speed.

Host Adapters Tested
AHA®-1540/2/F/P  
AHA®-2840/2VL  
AHA®-3940/W

Optisys
9250 North 43rd Avenue, Suite 12
Glendale, AZ 85302
Phone	(602) 997-9699
Fax	(602) 944-4051
Toll free	(800) 327-1271

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

MULTIUSER/NETWORKING SOLUTIONS	158

Winter, 1996

Pioneer Hi-Fi (GB) Ltd.

	PIONEER

	Pioneer, the leading manufacturer of optical disc technology has developed a solution utilizing it's high storage CD-ROM autochanger.  
	This solution provides stored video clips directly to designated PC's.  The Video Browse Server enables users to view the whole of a 
	video library on a PC.  This application has a user friendly and logical GUI.  The video clips never physically leave the library, 
	hence no time lost tracing material.  All of the video is held on CD-ROMs locked away in a 500 disk autochanger.  Initially by the use 
	of alphanumeric entries a search can be narrowed down to several titles. A selected title gives further indexed information on the clip
	 and also more importantly at least two thumbnails.  The chosen clip can then be viewed on a PC terminal.  By selecting various clips 
	the user automatically generates a clip list.  This file can then be sent to the compiling station on the network.  The compiling 
	station then assembles the request on any chosen broadcast medium- D1, D2, D3, D5, Digital Betacam, Betacam, Disc etc.

Host Adapters Tested
AHA®-2940/4/U/UW  
AHA®-3940/W  
AHA®-3940U/UW

Pioneer Hi-Fi (GB) Ltd.
Pioneer House, Hollybush Hill
Stoke Poges, Slough SL2 4QP
England
Phone	144-01753-789732
Fax	144-01753-789539

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

MULTIUSER/NETWORKING SOLUTIONS	159

Winter, 1996

Reed Technology & Information Services, Inc.

	OPTI-NET

	The OPTI-NET® product family lets users share information on CD-ROM discs over a local area network.  Advanced performance features 
	include server and workstation XMS caching and data prefetch coupled with sophisticated administration features such as remote 
	management and license enforcement.  OPTI-NET for MS-DOS supports both Novell and NetBIOS LANs.    
	  
	OPTI-NET NLM allows the addition of CD-ROM drives onto a Novell NetWare 3.x or 4.x file server.  This NetWare Loadable Module (NLM), 
	certified by Novell Labs, extends the functionality of the file server by enhancing the ability to manage and administer CD-ROM drives.
	  This is a fast powerful solution now enhanced for CD jukeboxes and multilingual language support.    
	  
	OPTI-NET now provides a utility that fully automates CD-ROM applications for Windows clients accessing either a DOS or NLM CD-ROM 
	server.  After the initial installation and setup, end-users may launch networked CD-ROM titles by simply clicking on the desired 
	program icon.  
	  
	OPTI-NET's NLM version also supports the German, French, French Canadian and Spanish languages.

Host Adapters Tested
AHA®-1520/2  
AHA®-1540/2/F/P  
AHA®-1640  
AHA®-1740/2/4  
AHA®-2740/2/4/T/W

Reed Technology & Information Services, Inc.
20251 Century Boulevard
Germantown, MD 20874
Phone	(301) 428-3700
Fax	(301) 428-2903
Toll free	(800) 922-9204
E-mail	HelpDesk@ocs.com

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

MULTIUSER/NETWORKING SOLUTIONS	160

Winter, 1996

S&H Computer Systems, Inc.

	TSX-32

	TSX-32™ offers the power of real-time, multi-user UNIX operating system with the ease-of-use of DOS. It excels as an application server
	 for DOS (16-bit & DPMI) and 32-bit applications, an NFS file server, a communication server and a printer server. TSX-32 supports up 
	to 256 users and 400 concurrent tasks on a single PC. Or, up to 40 times that number on a TCP/IP LAN or WAN. Add the BBS engine for 
	advanced remote access functionality. Add full Internet connectivity. See the TSX-BBS also listed in this guide.

Host Adapters Tested
AHA®-1540/2/F/P  
AHA®-1740/2/4  
AHA®-2740/2/4/T/W  
AHA®-2840/2VL  
AHA®-2940/4/W

S&H Computer Systems, Inc.
1027 17th Avenue South
Nashville, TN 37212
USA
Phone	(615) 327-3670
Fax	(615) 321-5929

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

MULTIUSER/NETWORKING SOLUTIONS	161

Winter, 1996

S&H Computer Systems, Inc.

	TSX-BBS

	TSX-BBS™ serves remote access connectivity needs ranging from those of a 2-line entertainment BBS to those of an entire corporation. It
	 features full Internet support. TSX-BBS add-ins can be standard DOS applications, DBMSs and tools, as well as BBS “door” programs. It 
	is configured to support one SYSOP and from two to 256 users on one PC. In addition, TSX-BBS can support hundreds of users spread 
	across a TCP/IP LAN or WAN of TSX-BBS servers.

Host Adapters Tested
AHA®-1520/2  
AHA®-1540/2/F/P  
AHA®-1740/2/4  
AHA®-2740/2/4/T/W  
AHA®-2840/2VL  
AHA®-2940/4/W

S&H Computer Systems, Inc.
1027 17th Avenue South
Nashville, TN 37212
USA
Phone	(615) 327-3670
Fax	(615) 321-5929

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

MULTIUSER/NETWORKING SOLUTIONS	162

Winter, 1996

Silver Oak Systems, Inc.

	IronClad

	IronClad® is a highly Windows-integrated security program which provides comprehensive protection for both standalone and networked 
	PCs.  IronClad provides both data-security (access control down to the file level, DES/proprietary encryption, keyboard locking, virus 
	prevention, program/data auditing, boot protection, single sign-on and object reuse prevention) and application-security (auto 
	application protection, piracy prevention, public access and file purging).

Host Adapters Tested
AHA®-1740/2/4

Silver Oak Systems, Inc.
8209 Cedar Street
Silver Spring, MD 20910
USA
Phone	(301) 585-8641
Fax	(301) 588-6484

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

MULTIUSER/NETWORKING SOLUTIONS	163

Winter, 1996

SunSoft, Inc.

	Solaris 2.5 for x86

	Solaris leads the UNIX operating system market, running on an installed base of more than 2 million systems.  It is the fastest, most 
	secure and reliable 32-bit operating system for SPARC, Intel, and Power PC server and desktop systems.  
	  
	Solaris provides a foundation for highly - integrated enterprise network environments, supporting multi-vendor interoperability and 
	resource sharing.  The operating system fits seamlessly into existing computing environments, providing the network management and 
	configuration tools for customers' growing computing needs.  
	  
	Solaris includes advanced technologies for multithreading, symmetric multiprocessing, integrated TCP/IP-based networking, and 
	centralized network administration tools.  And, recognizing the diversity of customer needs, Solaris comes in a series of 
	configurations.

Host Adapters Tested
AHA®-1510  
AHA®-1520/2  
AHA®-1530/2P  
AHA®-1540/2/F/P  
AHA®-1640  
AHA®-1740/2/4  
AHA®-2740/2/4/T/W  
AHA®-2840/2VL  
AHA®-2940/4/W  
AHA®-2940/4/U/UW

SunSoft, Inc.
2550 Garcia Avenue
Mountain View, CA 94043
USA
Phone	(415) 960-3200
Fax	(415) 336-0555
URL	http://www.sun.com

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

MULTIUSER/NETWORKING SOLUTIONS	164

Winter, 1996

TAC Systems

	SCSI Shuttle

	The TAC Systems SCSI Shuttle™ product allows users to access CD-ROMs on DOS/Windows based platforms.  Also, our Novell based version 
	installs on any Netware 3.x or 4.x file server without the use of additional drivers or software on the workstations.

Host Adapters Tested
AHA®-1540/2/F/P  
AHA®-1640  
AHA®-1740/2/4  
AHA®-2740/2/4/T/W  
AHA®-2940/4/W

TAC Systems
1031 Putman Drive
Huntsville, AL 35816
Phone	(205) 721-1976
Fax	(205) 721-0242

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

MULTIUSER/NETWORKING SOLUTIONS	165

Winter, 1996

The Santa Cruz Operation, Inc.

	SCO/Open Desktop

	SCO Open Desktop combines the SCO UNIX System, an advanced GUI, networking, and DOS services in an integrated 32-bit, distributed 
	client/server platform.  Both the SCO UNIX System and SCO Open Desktop deliver unprecedented multi-user, multitasking performance on 
	today's 386/486 ISA, EISA, Micro Channel, and multiprocessor systems (with SCO MPX).

Host Adapters Tested
AHA®-1510  
AHA®-1520/2  
AHA®-1540/2/F/P  
AHA®-1640  
AHA®-1740/2/4  
AHA®-2740/2/4/T/W

The Santa Cruz Operation, Inc.
400 Encinal Street, P.O. Box 1900
Santa Cruz, CA 95061
Phone	(408) 425-7222
Fax	(408) 427-5432
Toll free	(800) SCO-UNIX

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

MULTIUSER/NETWORKING SOLUTIONS	166

Winter, 1996

THEOS Software Corporation

	THEOS NetServer

	THEOS NetServer® is a network operating system that integrates THEOS-based applications seamlessly with Novell and Microsoft platforms,
	 including Windows for Workgroups 3.11, Windows 95 and Windows NT.  As a dedicated application server, NetServer can support a mixed 
	Client/Server environment of terminals and graphics workstations, offering centralized data security and fast file access.  
	  
	The THEOS operating system is primarily used in vertical markets such as Dental, Veterinarian, Alarm Systems and Point-of-Sale.

Host Adapters Tested
AHA®-1540/2/F/P

THEOS Software Corporation
1777 Botelho Drive, Suite 110
Walnut Creek, CA 94596
Phone	(510) 935-1118
Fax	(510) 935-1177
Toll free	800-600-5660
E-mail	info@theos-software.com
URL	http://www.theos-software.com

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

MULTIUSER/NETWORKING SOLUTIONS	167

Winter, 1996

THEOS Software Corporation

	THEOS 32

	THEOS 32® is a 32-bit multiuser, multi-threaded, preemptive multitasking operating system.  Optimized to run on 486 and Pentium based 
	systems, THEOS can support over 200 users.  Built-in features include:  Windowing capabilities, RS-232 Communications tools, Tape 
	Backup Utilities, SCSI support.  Additional products include 32-bit C and BASIC development languages.  
	  
	The THEOS operating system is primarily used in vertical markets such as Dental, Veterinarian,  Alarm Systems and Point-of-Sale.

Host Adapters Tested
AHA®-1540/2/F/P

THEOS Software Corporation
1777 Botelho Drive, Suite 110
Walnut Creek, CA 94596
Phone	(510) 935-1118
Fax	(510) 935-1177
Toll free	800-600-5660
E-mail	info@theos-software.com
URL	http://www.theos-software.com

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

MULTIUSER/NETWORKING SOLUTIONS	168

Winter, 1996

Traakan

	NetServer

	NetServer software connects storage and peripheral resources to TCP/IP-NFS networks quickly, easily, and economically.  NetServer based
	 NFS file servers provide local and remote tape backup, rapid-restart file volumes, and local and remote menu-driven administration.  
	The streamlined firmware-like design manages terabytes of storage and delivers 1000+ SPEC-NFS operations per second.  NetServer is 
	available to qualified VARS/OEMS/ Integrators that service the Open Systems Market.

Host Adapters Tested
AHA®-1540/2/F/P  
AHA®-1740/2/4  
AHA®-2740/2/4/T/W  
AHA®-2940/4/W  
AHA®-3940/W

Traakan
111 Main Street, Suite 5
Los Altos, CA 94022
Phone	415-961-0900
Fax	415-941-0914
E-mail	info@traakan.com
URL	http://www.traakan.com

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

PERIPHERAL UTILITY	169

Winter, 1996

Adaptec, Inc.

	ADAPTEC® EZ-SCSI®

	If you have, or are planning to add, SCSI peripherals like tape or disk drives, CD-ROM drives, recordable CD-R drives, magneto-optical 
	drives, or scanners, Adaptec EZ-SCSI® software provides everything you need to manage and take full advantage of each device.  
	  
	Adaptec EZ-SCSI software is a suite of 32-bit practical applications and power tools that are remarkably easy to install and use.  
	Simple desktop controls give you immediate access to any fuction.  A unique online tutorial explains everything you need to know about 
	SCSI in easy-to-understand terms.  
	  
	Key benefits:  
	* Easiest way to manage SCSI peripherals  
	* For Windows operating systems  
	* Includes these practical applications:  Adaptec Easy-CD Backup™, QuickScan™, Audio CD player, Photo CD Viewer, CD Writer, and CD 
	Copier  
	* Includes these powerful tools:  SCSI Explorer™ (Power Management, SCSI Interrogator™, Read/Write Disk Cashe tool), SCSI Tutor™, SCSI 
	Bench™ and Drive Light™.

Host Adapters Tested
APA™-348  
APA™-358  
APA™-1460  
AVA™-1505  
AHA®-1510  
AVA™-1515  
AHA®-1520/2  
AHA®-1530/2P  
AHA®-1540/2/F/P  
AHA®-1640  
AHA®-1740/2/4  
AHA®-2740/2/4/T/W  
AHA®-2840/2VL  
AHA®-2920  
AHA®-2940/4/W  
AHA®-2940AU  
AHA®-3940/W  
AHA®-3940U/UW

Adaptec, Inc.
691 S Milpitas Blvd
Milpitas, CA
USA
Phone	1-800-934-2766
Fax	408-262-2533
Toll free	1-800-934-2766
E-mail	sales@adaptec.com
URL	http://www.adaptec.com

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

PERIPHERAL UTILITY	170

Winter, 1996

Adaptec, Inc.

	ADAPTEC® CI/O™

	With easy to use Adaptec® CI/O™ software, managers can monitor all SCSI peripheral devices connected to servers by Adaptec® host 
	adapters.    
	  
	Using Adaptec® CI/O™ software on any Windows® client, managers can remotely monitor the I/O performance of any server on the network 
	from a single central location.  Managers can install the latest device drivers from a remote location as well.  
	  
	Adaptec® CI/O™ software automatically detects failure of any SCSI device on a network server and notifies the manager immediately.  
	With a clear view of I/O traffic, managers can spot bottlenecks and act quickly to balance I/O loads to optimize performance among SCSI
	 devices.  Adaptec® CI/O™ improves the manageability of any size network--from a single server to a global network.

Host Adapters Tested
AHA®-1540/2/F/P  
AHA®-2740/2/4/T/W  
AHA®-2840/2VL  
AHA®-2940/4/W  
AHA®-2940AU  
AHA®-3940/W  
AHA®-3980/5/W

Adaptec, Inc.
691 S Milpitas Blvd
Milpitas, CA
USA
Phone	1-800-934-2766
Fax	408-262-2533
Toll free	1-800-934-2766
E-mail	sales@adaptec.com
URL	http://www.adaptec.com

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

PERIPHERAL UTILITY	171

Winter, 1996

Cirrus Technology, Inc.

	Unite® Objects

	The Unite® Objects include a set of development tools: the Unite Scanner Object, the Unite Image Viewer and the Unite Storager. The 
	Unite® Objects provides accessibility to functionality in a wide range of scanners as well as all functionality in the Unite Image 
	Viewer Object.  
	  
	The Unite Image Viewer Object is used to compress, decompress, view, scale, and manipulate color and grayscale photographic images and 
	bitonal document images.  
	  
	Unite Storager is provided as a GU, front-end for administrative tasks and an API set for customizing the storage system.

Host Adapters Tested
AVA™-1505  
AHA®-1510  
AVA™-1515  
AHA®-1520/2  
AHA®-1530/2P  
AHA®-1540/2/F/P  
AHA®-1640  
AHA®-1740/2/4  
AHA®-2740/2/4/T/W  
AHA®-2825VL  
AHA®-2840/2VL  
AHA®-2910A/Ai  
AHA®-2940/4/W  
AHA®-3940/W  
AHA®-3980/5/W

Cirrus Technology, Inc.
5301 Buckeystown Pike, 4th floor
Frederick, MD 21704
US
Phone	(301)698-1900
Fax	(301)698-1909
E-mail	sales@cirunite.com
URL	http://www.cirunite.com

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

PERIPHERAL UTILITY	172

Winter, 1996

Cirrus Technology, Inc.

	Unite® Storager

	Unite® Storager is a product which uses a Virtual Jukebox Object, a SCSI Changer (Jukebox) Object and SCSI Drive Object(s) to manage 
	the storage and retrieval of files from a variety of media such as rewriteable and WORM optical, and CD-ROM.

Host Adapters Tested
AHA®-1510  
AHA®-1520/2  
AHA®-1540/2/F/P  
AHA®-1740/2/4  
AHA®-2940/4/W

Cirrus Technology, Inc.
5301 Buckeystown Pike, 4th floor
Frederick, MD 21704
US
Phone	(301)698-1900
Fax	(301)698-1909
E-mail	sales@cirunite.com
URL	http://www.cirunite.com

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

PERIPHERAL UTILITY	173

Winter, 1996

Cirrus Technology, Inc.

	Unite CD-Maker

	Unite® CD-Maker is a 32-bit software package for creating custom CDs.  Unite CD-Maker allows users to quickly and easily make audio CDs
	 as well as create CD-ROMs for backup, archiving and distribution of data.  Included with Unite CD-Maker is a 32-Bit API set for 
	automating the recording process.  Advanced features include multisession support, enhanced CD and mixed mode support and a visual 
	buffer meter to monitor the burn. Many recorders are supported and Windows 95, Windows NT and OS/2 are supported.

Host Adapters Tested
AVA™-1505  
AHA®-1510  
AVA™-1515  
AHA®-1520/2  
AHA®-1530/2P  
AHA®-1540/2/F/P  
AHA®-1640  
AHA®-1740/2/4  
AHA®-2740/2/4/T/W  
AHA®-2825VL  
AHA®-2840/2VL  
AHA®-2910A/Ai  
AHA®-2940/4/W  
AHA®-3940/W  
AHA®-3980/5/W

Cirrus Technology, Inc.
5301 Buckeystown Pike, 4th floor
Frederick, MD 21704
US
Phone	(301)698-1900
Fax	(301)698-1909
E-mail	sales@cirunite.com
URL	http://www.cirunite.com

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

PERIPHERAL UTILITY	174

Winter, 1996

Corel Corporation

	CorelSCSI

	CorelSCSI® software provides easy connection of SCSI devices. CorelSCSI includes device drivers for virtually every SCSI peripheral on 
	the market. CorelSCSI software also includes: Corel CD-Audio, Corel Tape Backup software, SCSI Tools for Windows and more. CorelSCSI is
	 multi-platform, with operating system support for DOS, Windows, OS/2 and Novell® NetWare 386. CorelSCSI is included in Adaptec’s SCSI 
	Direction® Plus kit and SCSI Master™ Plus kit.

Host Adapters Tested
AHA®-1520/2  
AHA®-1540/2/F/P  
AHA®-1640

Corel Corporation
1600 Carling Avenue
Ottawa, Ontario K1Z 8R7
Canada
Phone	(613) 728-8200
Fax	(613) 728-9790
Toll free	(800) 836-7274

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

PERIPHERAL UTILITY	175

Winter, 1996

Corel Corporation

	CorelSCSI Pro

	CorelSCSI Pro® is a high-performance software product designed to maximize SCSI performance.  CorelSCSI Pro provides: support for SCSI 
	scanners to scan images into any TWAIN-compliant graphics program; a CD-ROM server application that allows network users to retrieve 
	recently-accessed information with essentially no delay; and a utility that writes information to a compact disc using a CD-Recorder. 
	These features and others are available using an intuitive and friendly interface.

Host Adapters Tested
AHA®-1520/2  
AHA®-1540/2/F/P  
AHA®-1640

Corel Corporation
1600 Carling Avenue
Ottawa, Ontario K1Z 8R7
Canada
Phone	(613) 728-8200
Fax	(613) 728-9790
Toll free	(800) 836-7274

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

PERIPHERAL UTILITY	176

Winter, 1996

Cornerstone Imaging, Inc.   Storage Division

	MDMI

	The Optical File System (OFS) for optical drives software package provides access to standalone and daisy-chained optical disk drives 
	or rapidchangers under DOS- and PC-based networks, including all versions of NetWare, Banyan, 3Com®, LAN Manager, LANtastic, OS/2 2.x, 
	3.x and Warp, Windows 95 and Windows NT.  MDMI supports most 5.25- and 12-inch optical disk drives.  Data stored on optical disks using
	 the OFS are transportable to jukebox versions of the Optical File System software.  The software treats a single or entire daisy-chain
	 of optical drives as one drive designator under Novell DOS and the network systems supported.  Each side of an optical disk platter 
	under the assigned drive letter then appears as a subdirectory and is fully accessible through normal operating system commands.

Host Adapters Tested
APA™-1460  
AHA®-1510  
AHA®-1520/2  
AHA®-1530/2P  
AHA®-1540/2/F/P  
AHA®-1640  
AHA®-2840/2VL  
AHA®-2940/4/W

Cornerstone Imaging, Inc.   Storage Division
1600 South Main Street
Walnut Creek, CA 94596
Phone	(510) 938-5340
Fax	(510) 938-5341

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

PERIPHERAL UTILITY	177

Winter, 1996

Cornerstone Imaging, Inc.   Storage Division

	OJMI

	The Optical File System (OFS) for optical drives software package provides access to standalone and daisy-chained optical disk drives 
	or rapidchangers under DOS- and PC-based networks, including all versions of NetWare, Banyan, 3Com®, LAN Manager, LANtastic, OS/2 2.x, 
	3.x and Warp, Windows 95 and Windows NT.  MDMI supports most 5.25- and 12-inch optical disk drives.  Data stored on optical disks using
	 the OFS are transportable to jukebox versions of the Optical File System software.  The software treats a single or entire daisy-chain
	 of optical drives as one drive designator under Novell DOS and the network systems supported.  Each side of an optical disk platter 
	under the assigned drive letter then appears as a subdirectory and is fully accessible through normal operating system commands.

Host Adapters Tested
APA™-1460  
AHA®-1510  
AHA®-1520/2  
AHA®-1540/2/F/P  
AHA®-1640  
AHA®-2840/2VL  
AHA®-2940/4/W

Cornerstone Imaging, Inc.   Storage Division
1600 South Main Street
Walnut Creek, CA 94596
Phone	(510) 938-5340
Fax	(510) 938-5341

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

PERIPHERAL UTILITY	178

Winter, 1996

Digital Instrumentation Technology

	TransferPro

	TransferPro™ allows you to read and write Macintosh files directly from your PC.  TransferPro is a fast and easy file transfer 
	solution.  TransferPro reads, writes and formats Macintosh media including SyQuest™ , Bernoulli ™, Iomega™  Zip, data shuttle drives, 
	Pinnacle Micro™, Sony™,  MOST™, Ricoh™  and other magneto-optical drives, SCSI hard drives and CD-ROM drives.  TransferPro features 
	graphics viewers and converters and a high quality, easy to use Windows-based installer with an automatic configuration feature.  
	TransferPro is available for Windows, Windows 95 and Windows NT.

Host Adapters Tested
APA™-1460  
AVA™-1505  
AHA®-1510  
AVA™-1515  
AHA®-1520/2  
AHA®-1530/2P  
AHA®-1540/2/F/P  
AHA®-1640  
AHA®-1740/2/4  
AHA®-2740/2/4/T/W  
AHA®-2840/2VL  
AHA®-2940/4/W  
AHA®-3940/W

Digital Instrumentation Technology
127 Eastgate Dr. #20500
Los Alamos, NM 87544
Phone	(505) 662-1459
Fax	(505) 662-0897
Toll free	(800) 467-1459
E-mail	tpro-request@dit.com
URL	hhttp://www.dit.com

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

PERIPHERAL UTILITY	179

Winter, 1996

Florida Datamation

	ReelPro

	ReelPro™ is a driver and utility set to read and write IBM standard labeled and unlabeled 9Track tapes.

Host Adapters Tested
AHA®-1540/2/F/P  
AHA®-1640  
AHA®-1740/2/4

Florida Datamation
AMTEC Center, 6405 Congress Ave, Suite 140
Boca Raton, FL 33487
Phone	(407) 241-2966
Fax	(407) 241-3108
Toll free	(800) 642-5938
E-mail	sales@fdma.com

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

PERIPHERAL UTILITY	180

Winter, 1996

Micro Design International, Inc.

	SCSI Express

	SCSI Express is a package of SCSI device drivers to support devices under AIX, DOS, Novell 386 and 286, OS/2, UNIX (AT&T, Interactive 
	and SCO) and SCO XENIX.  These device drivers are designed to transparently support MDI’s Laserbank line of CD-ROM, DAT, hard disks, 
	jukebox, multifunction, rewritable optical, and WORM devices from popular manufacturers.

Host Adapters Tested
AHA®-1540/2/F/P  
AHA®-1640  
AHA®-1740/2/4  
AHA®-2740/2/4/T/W  
AHA®-2840/2VL

Micro Design International, Inc.
6985 University Boulevard
Winter Park, FL 32792
USA
Fax	(407) 677-8365
Toll free	(800) 228-0891

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

PERIPHERAL UTILITY	181

Winter, 1996

MicroText Systems Inc.

	SCSIUTIL

	SCSIUTIL allows raw access to SCSI tape drives, disk drives and floptical drives.  Internal modepages of the devices can be examined 
	and changed.  Data blocks can be viewed in HEX and ASCII, and can be saved, modified, and re-written.  Disks can be formatted and 
	verified.  For tapes, files can be copied raw, to and from local storage.  Blocks sizes can be manually set, and automatic block-size 
	detection is supported.  Most tape functions are availiable.

Host Adapters Tested
AHA®-1520/2  
AHA®-1540/2/F/P  
AHA®-2740/2/4/T/W  
AHA®-2840/2VL  
AHA®-2940/4/W  
AHA®-2940/4/U/UW  
AHA®-3940/W  
AHA®-3940U/UW  
AHA®-3980/5/W

MicroText Systems Inc.
507 Corbin Court
Mississauga, Ontario L5A 1M2
Canada
Phone	(905) 276-1257
Fax	(905) 276-7236
E-mail	sales@msitxt.gts.org

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

PERIPHERAL UTILITY	182

Winter, 1996

Optisys

	OptiDriver 2000

	OptiDriver™ is an easy-to-install interface software product featuring a smooth migration path across all supported configurations.  
	OptiDriver supports virtually all optical drives and jukeboxes.  It does not patch the operating system and it supports any sector-size
	 media.

Host Adapters Tested
AHA®-1520/2  
AHA®-1540/2/F/P  
AHA®-1640  
AHA®-1740/2/4

Optisys
9250 North 43rd Avenue, Suite 12
Glendale, AZ 85302
Phone	(602) 997-9699
Fax	(602) 944-4051
Toll free	(800) 327-1271

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

PERIPHERAL UTILITY	183

Winter, 1996

Pacific Microelectronics, Inc.

	MAC-In-DOS Plus

	MAC-in-DOS® Plus enables an IBM-compatible PC to read, write and format Macintosh data on the removable drives of SyQuest and Bernoulli
	 and the magneto-optical drives of Sony, Hewlett Packard and Fujitsu.

Host Adapters Tested
AHA®-1540/2/F/P

Pacific Microelectronics, Inc.
201 San Antonio Circle, C250
Mountain View, CA 94040
Phone	(415) 948-6200
Fax	(415) 948-6296
E-mail	sales@netusa.com
URL	http://www.netusa.com

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

PERIPHERAL UTILITY	184

Winter, 1996

PC-Kwik Corporation

	PC-Kwik

	The Super PC-Kwik® disk cache provides acceleration of both disk reading and writing.  By default it uses a safe FIFO algorithm with no
	 time-delays.  It also features automatic lending of expanded and extended memory. The program provides a wide variety of options for 
	controlling the caching function.

Host Adapters Tested
AHA®-1520/2  
AHA®-1530/2P  
AHA®-1540/2/F/P  
AHA®-2840/2VL  
AHA®-2940/4/W

PC-Kwik Corporation
3800 SW Cedar Hills Boulevard
Beaverton, OR 97005
Phone	(503) 644-5644
Fax	(503) 646-8267
Toll free	(800) 234-5945

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

PERIPHERAL UTILITY	185

Winter, 1996

Peripheral Test Instruments, Inc.

	SCSI toolbox

	The SCSI toolbox™ is an ASPI compliant, menu-driven application for diagnosing, testing, exercising and setting up SCSI peripherals. 
	Total programming control from Mode Sense/Select, Flaw map interrogation and toggling cache bits are simple and painless. The SCSI 
	Toolbox supports disk, tape, optical and jukebox devices. Narrow, wide, single-ended or differential drives can be thoroughly diagnosed
	 and problems isolated quickly using the SCSI Toolbox. The SCSI Toolbox Base Tester allows for all diagnosing, testing and programming.
	 The Workstation Prep module lets the user automatically label/partition any SCSI drive for 7 different UNIX environments. Our 
	Multi-Drive and Multi-Drive Wide module allows the simultaneous exercising of up to 15 drives at once. The Jukebox module lets you 
	exercise and program the robotics of any optical or cartridge jukebox. The SCSI Toolbox is in use at over 9500 locations worldwide, and
	 is available for DOS, UNIX, and Windows.  PTI has several other products for SCSI peripheral integration and trouble-shooting.

Host Adapters Tested
APA™-348  
APA™-358  
APA™-1460  
AHA®-1510  
AHA®-1520/2  
AHA®-1530/2P  
AHA®-1540/2/F/P  
AHA®-1640  
AHA®-1740/2/4  
AHA®-2740/2/4/T/W  
AHA®-2840/2VL  
AHA®-2940/4/W

Peripheral Test Instruments, Inc.
3455 South Wadsworth Boulevard, Suite 220
Lakewood, CO 80227
Phone	(303) 763-7488
Fax	(303) 763-9488
Toll free	(800) 829-7274
E-mail	info@choice.com

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

PERIPHERAL UTILITY	186

Winter, 1996

Peripheral Test Instruments, Inc.

	SCSI Service Tool

	The SCSI Service Tool™ is a DOS and Windows based, ASPI compliant application for diagnosing, testing, exercising and programming SCSI 
	disk type devices.  Easily set mode page parameters, download firmware and exercise any SCSI disk type drive in minutes.  Capture mode 
	parameter information from one drive and compare it to any other, as well as download mode information to a "raw" drive from a preset 
	drive.

Host Adapters Tested
APA™-348  
APA™-358  
APA™-1460  
AHA®-1510  
AHA®-1520/2  
AHA®-1530/2P  
AHA®-1540/2/F/P  
AHA®-1640  
AHA®-1740/2/4  
AHA®-2740/2/4/T/W  
AHA®-2840/2VL  
AHA®-2940/4/W

Peripheral Test Instruments, Inc.
3455 South Wadsworth Boulevard, Suite 220
Lakewood, CO 80227
Phone	(303) 763-7488
Fax	(303) 763-9488
Toll free	(800) 829-7274
E-mail	info@choice.com

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

PERIPHERAL UTILITY	187

Winter, 1996

Peripheral Test Instruments, Inc.

	Dr. SCSI

	Dr. SCSI™ is a DOS and Windows based, ASPI compliant application for setting mode page paramenters on any SCSI drive for all 
	audio/video applications and any others that require custom mode page settings.  This application easily displays the necessary mode 
	bits in their acronym formats and default mnemonic values.  No more sifting through pages of hexidecimal data to try and optimize a 
	SCSI drive.  Once a drive is setup and optimized, the mode page data can be captured and recalled at any time.  Making the job of 
	resetting drives over and over again totally obsolete.  There are several performance tests that display the results of the 
	optimization.

Host Adapters Tested
APA™-348  
APA™-358  
APA™-1460  
AHA®-1510  
AHA®-1520/2  
AHA®-1530/2P  
AHA®-1540/2/F/P  
AHA®-1640  
AHA®-1740/2/4  
AHA®-2740/2/4/T/W  
AHA®-2840/2VL  
AHA®-2940/4/W

Peripheral Test Instruments, Inc.
3455 South Wadsworth Boulevard, Suite 220
Lakewood, CO 80227
Phone	(303) 763-7488
Fax	(303) 763-9488
Toll free	(800) 829-7274
E-mail	info@choice.com

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

PERIPHERAL UTILITY	188

Winter, 1996

Peripheral Test Instruments, Inc.

	SCSI Downloading Tool

	The SCSI Downloading Tool™ is a DOS and Windows based, ASPI compliant application for downloading firmware on to nearly every type of 
	SCSI drive. Upgrading or feature enhancement through firmware is easily accomplished with this simple-to-use utility.

Host Adapters Tested
APA™-348  
APA™-358  
APA™-1460  
AHA®-1510  
AHA®-1520/2  
AHA®-1530/2P  
AHA®-1540/2/F/P  
AHA®-1740/2/4  
AHA®-2740/2/4/T/W  
AHA®-2840/2VL  
AHA®-2940/4/W

Peripheral Test Instruments, Inc.
3455 South Wadsworth Boulevard, Suite 220
Lakewood, CO 80227
Phone	(303) 763-7488
Fax	(303) 763-9488
Toll free	(800) 829-7274
E-mail	info@choice.com

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

PERIPHERAL UTILITY	189

Winter, 1996

Pixelab, Inc.

	DATMAN

	DATMAN™ is a revolutionary DAT control software which provides an MS-DOS compatible file system with up to 8-GB and a quarter million 
	files.  Unlike typical tape backup programs, most MS-DOS and Windows applications can directly read and write files on the tape.  
	DATMAN makes the DAT drive operate very much like the familiar floppy drive.  Once it is installed, it is extremely easy to use.  Also,
	 it removes the common access bottleneck to the huge online storage.  With the sophisticated adaptive cache algorithm, DATMAN provides 
	high-performance file access.

Host Adapters Tested
APA™-358  
APA™-1460  
AVA™-1505  
AHA®-1510  
AVA™-1515  
AHA®-1520/2  
AHA®-1530/2P  
AHA®-1540/2/F/P

Pixelab, Inc.
1212 S. Naper Blvd.  Ste. #119
Naperville, IL 60540
Phone	(708) 369-7112
Fax	(708) 369-7113
E-mail	sales@datman.com
URL	http://www.datman.com

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

PERIPHERAL UTILITY	190

Winter, 1996

Plasmon Data Ltd.

	DOS Manager!

	DOS Manager! provides single or multi jukebox support for WORM, rewritable, or multifunction units. File compatibility is offered with 
	Corel as well as ECMA. Full utilities are built in for jukebox and media management as well as worm audit features.

Host Adapters Tested
AHA®-1510  
AHA®-1520/2  
AHA®-1540/2/F/P  
AHA®-1640  
AHA®-1740/2/4

Plasmon Data Ltd.
Whiting Way
Melbourn, Herts SG8 6DN
ENGLAND
Phone	44 0 1763 262963
Fax	44 0 1763 264444

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

PERIPHERAL UTILITY	191

Winter, 1996

Rambler Systems Limited

	RSPRINT

	RSPRINT is a printer driver which gives easy access to the Sony® UP-D7000E color printer.  The driver supports the printing of full 
	24-bit images in DOS and Windows.  RSPRINT is compatible with Adaptec® host adapters via the ASPI interface.

Host Adapters Tested
AHA®-1520/2

Rambler Systems Limited
51 West Bryson Road
Edinburgh,  EH11 1EH
Scotland
Phone	(44) 31-3132557
Fax	(44) 31-3134542

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

PERIPHERAL UTILITY	192

Winter, 1996

SHAFFSTALL Corporation

	QuickTape

	QuickTape™ is a tape conversion/transfer software product that allows users to read/write IBM/ANSI/ISO labeled/unlabeled tapes.  
	QuickTape supports 3480, 9-track, 8mm, 4mm DAT, QIC, AS/400, TK50 and TK85 formats.  It provides format conversion, tape-to-tape, 
	tape-to-disk, disk-to-tape transfer, EBCDIC/ASCII code conversion, and supports variable record and multi-volume tapes.

Host Adapters Tested
AHA®-1510  
AHA®-1520/2  
AHA®-1540/2/F/P  
AHA®-1640  
AHA®-1740/2/4  
AHA®-2740/2/4/T/W  
AHA®-2940/4/W  
AHA®-3940/W

SHAFFSTALL Corporation
7901 East 88th Street
Indianapolis, IN 46256
Phone	(317) 842-2077
Fax	(317) 842-8294
Toll free	(800) 248-3475
E-mail	sales@shaffstall.com
URL	http://www.shaffstall.com

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

PERIPHERAL UTILITY	193

Winter, 1996

SHAFFSTALL Corporation

	QuickCopy

	The SHAFFSTALL QuickCopy™ system supports multi-drive duplication of virtually every tape media in use today...QIC, 4mm DAT, 8mm, 
	TK50®, AS/400®, 9-track, and IBM® 3480.  QuickCopy features include tape mastering, network support, verification, error reporting, 
	drive status, byte count, user security, and comprehensive copy status display, including number of copies and average duplication 
	speed.  It also accommodates multiple cartridge autoloaders on 3480, 4 mm, and 8 mm drives.

Host Adapters Tested
AHA®-1510  
AHA®-1520/2  
AHA®-1540/2/F/P  
AHA®-1640  
AHA®-1740/2/4  
AHA®-2740/2/4/T/W  
AHA®-2940/4/W  
AHA®-3940/W

SHAFFSTALL Corporation
7901 East 88th Street
Indianapolis, IN 46256
Phone	(317) 842-2077
Fax	(317) 842-8294
Toll free	(800) 248-3475
E-mail	sales@shaffstall.com
URL	http://www.shaffstall.com

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

PERIPHERAL UTILITY	194

Winter, 1996

Spirit of Performance, Inc.

	Personal Measure

	Personal Measure™ monitors the resources used by live applications running in the MS-DOS environment.  It reports the usage of hardware
	 resources and when they have been used.  The PC hardware resources are classified as processor, local hard disk, LAN disk, keyboard, 
	printer, serial port, and SCSI.  Personal Measure is compatible with Windows 3.1 or later and with client software for the most popular
	 network operating systems:  NetWare, VINES, LAN Manager, and various NetBIOS-based network operating systems.  Personal Measure is 
	intended for high-level problem solving and isolation of system or application bottlenecks.

Host Adapters Tested
AHA®-1520/2  
AHA®-1540/2/F/P  
AHA®-1740/2/4  
AHA®-2740/2/4/T/W  
AHA®-2840/2VL  
AHA®-2940/4/W

Spirit of Performance, Inc.
73 Westcott Road
Harvard, MA 01451-1821
Phone	(508) 456-3889
Fax	(508) 456-3937
E-mail	3571400@mcimail.com

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

PERIPHERAL UTILITY	195

Winter, 1996

Spirit of Performance, Inc.

	Personal Measure Pro

	Personal Measure Pro™ adds a file usage report to Personal Measure.  It is used by network analysts, hardware designers and analysts, 
	and software development teams who need to understand exactly how files and devices are accessed.  It is also used to determine the 
	effects of access patterns on hardware systems and subsystems.  Using Personal Measure Pro, an analyst can find the causes for overall 
	system behavior within minutes.

Host Adapters Tested
AHA®-1520/2  
AHA®-1540/2/F/P  
AHA®-1740/2/4  
AHA®-2740/2/4/T/W  
AHA®-2840/2VL  
AHA®-2940/4/W

Spirit of Performance, Inc.
73 Westcott Road
Harvard, MA 01451-1821
Phone	(508) 456-3889
Fax	(508) 456-3937
E-mail	3571400@mcimail.com

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

PERIPHERAL UTILITY	196

Winter, 1996

Systems Enhancement Corporation

	Total Network Recall

	Total Network Recall (TNR) is a 100% Novell SMS-compatible tape back up software package.  The product features a server-based NLM; 
	multiple auto backup sessions; and support of all Novell TSAs.  TNR supports NetWare 3.1x and 4.0x.  Additional features include 
	compatibility wiht powermon software, built-in batch file scheduler and auto changer support.

Host Adapters Tested
AHA®-1510  
AHA®-1520/2  
AHA®-1540/2/F/P  
AHA®-1640  
AHA®-1740/2/4

Systems Enhancement Corporation
174 Chesterfield Industrial Blvd
Chesterfield, MO 63005
USA
Phone	(314) 532-2855
Fax	(314) 532-2037

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

PERIPHERAL UTILITY	197

Winter, 1996

Touchstone Software Corporation

	CheckIt Pro Set

	CheckIt Pro™ Set combines CheckIt Pro SysInfo with the Tests & Tools module.  Tests & Tools’ enhanced tests run from the command line 
	or mouse driven menu and include system board, memory, serial/parallel ports, hard/floppy drive(s), video (monitor/adapter), printer, 
	and input devices.  Tools include hard drive format utilities that format all drive types, and create rescue disk.  The advanced 
	anti-virus utility scans for over 2,000 viruses, including new polymorphic viruses.  Reports automatically document system status, and 
	journals pinpoint component failures.

Host Adapters Tested
AHA®-1510

Touchstone Software Corporation
2124 Main Street, Suite 250
Huntington Beach, CA 92648-+444
Phone	(714) 969-7746
Fax	(714) 960-1886
Toll free	(800) 531-0450

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

PERIPHERAL UTILITY	198

Winter, 1996

Touchstone Software Corporation

	WINCheckIt

	WINCheckIt™ is the diagnostic utility that provides answers, not just information. It is an ideal choice for anyone who wants an 
	easy-to-use program to assist with hardware and software purchase decisions, installing upgrades, or determining if repairs are 
	required.

Host Adapters Tested
AHA®-1510

Touchstone Software Corporation
2124 Main Street, Suite 250
Huntington Beach, CA 92648-+444
Phone	(714) 969-7746
Fax	(714) 960-1886
Toll free	(800) 531-0450

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

PERIPHERAL UTILITY	199

Winter, 1996

Watergate Software, Inc.

	PC-Doctor

	PC-Doctor® has over 200 diagnostic tests, system information functions and utilities.  It identifies IRQ conflicts, finds available IRQ
	 lines, DMA channels, and I/O addresses.  Network/SCSI/IDE support and identification is included.  A unique Maximum System Load Test 
	provides high-performance burn-in testing.  PC-Doctor is easy-to-use and it has context-sensitive help and an on-line manual.  
	PC-Doctor is very portable, fitting easily on a 3.5" or 5.25" diskette.  PC-Doctor works with PCs from PC/XT to Pentium.  It’s perfect 
	for corporate support personnel, end users and service organizations.  An OEM version is available for licensing by PC manufacturers to
	 improve their technical support.

Host Adapters Tested
AHA®-1540/2/F/P  
AHA®-1740/2/4

Watergate Software, Inc.
2000 Powell Street, Suite 1200
Emeryville, CA 94608
USA
Phone	(510) 596-1770
Fax	(510) 653-4784

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

PERIPHERAL UTILITY	200

Winter, 1996

Windsor Technologies, Inc.

	PC-Technician

	PC-Technician™ is professional-level diagnostic software for Intel-based (8088->Pentium) and compatible PCs.  Written in assembly 
	language, it has its own proprietary operating system and boot-loader program.  PC-Technician will boot the target PC and directly test
	 its hardware without interference from its native operating system (DOS, UNIX, OS/2, Windows NT, etc.).  PC-Technician contains over 
	200 comprehensive tests and functions that can be run in single or continuous mode.  PC-Technician is used by service technicians to 
	troubleshoot a malfunctioning PC, certify a repaired PC, burn in a new PC, edit CMOS, or low-level format the fixed disk drive.

Host Adapters Tested
AHA®-1540/2/F/P  
AHA®-1740/2/4  
AHA®-2840/2VL  
AHA®-2940/4/W  
AHA®-2940W MAC

Windsor Technologies, Inc.
130 Alto Street
San Rafael, CA 94901
Phone	(415) 456-2200
Fax	(415) 456-2244
E-mail	pcdiags@windsortech.com
URL	http://www.windsortech.com

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

PERIPHERALS	201

Winter, 1996

ADS International, Inc.

	DockMaster M4SKF & M5SKF

	The DockMaster® M4SKF and  M5SKF Series of “hot” removable docking kits are ideal for data security, on-line backup, data 
	transportation and disk array applications.  The DockMaster docking kit product is protected by U.S. patent #4,941,841.  ADS 
	International is the patent-authorized marketer of these products.

Host Adapters Tested
APA™-348  
APA™-358  
APA™-1460  
AHA®-1510  
AHA®-1520/2  
AHA®-1540/2/F/P  
AHA®-1640  
AHA®-1740/2/4  
AHA®-2740/2/4/T/W  
AHA®-2840/2VL

ADS International, Inc.
434 Cloverleaf Drive
Baldwin Park, CA 91706
USA
Phone	(818) 369-2332
Fax	(818) 855-5059

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

PERIPHERALS	202

Winter, 1996

ADS International, Inc.

	ADS1000 & ADS4000

	The ADS1000 & ADS4000 are two of the highest performance RAID controllers on the market.  Data transfer rates exceed 3 MB/sec and can 
	support up to 35 HDDs.  Maximum capacity is 300 GB.

Host Adapters Tested
APA™-348  
APA™-358  
APA™-1460  
AHA®-1510  
AHA®-1520/2  
AHA®-1540/2/F/P  
AHA®-1640  
AHA®-1740/2/4  
AHA®-2740/2/4/T/W  
AHA®-2840/2VL

ADS International, Inc.
434 Cloverleaf Drive
Baldwin Park, CA 91706
USA
Phone	(818) 369-2332
Fax	(818) 855-5059

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

PERIPHERALS	203

Winter, 1996

AGFA

	AGFA Scanners

	From desktop to highend scanning solutions, all scanners packed with easy to use and professional imaging tools.

Host Adapters Tested
AVA™-1505  
AHA®-1510  
AVA™-1515  
AHA®-1520/2  
AHA®-1530/2P  
AHA®-1540/2/F/P  
AHA®-1640  
AHA®-1740/2/4  
AHA®-2740/2/4/T/W  
AHA®-2840/2VL  
AHA®-2940/4/W  
AHA®-3940/W

AGFA
Septestraat  27
Mortsel,  2640
Belgium
Phone	32-3-444-3987
Fax	32-3-444-4240
E-mail	fotolook@eps.agfa.be

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

PERIPHERALS	204

Winter, 1996

Chi Corporation

	Outright

	OutRight™ SCSI Software Package for NineTrack and 3480, 3490 (IDRC), and 3490E tape drive is designed to reliably expand the data 
	storage and interchange of power PCs. Add the OutRight for DOS or Windows software package to a PC and have a universal interface for 
	data backup, archiving and transfer.  Using the package, PC users have the flexibility to access on-site or off-site IBM, Unisys®, DEC®
	 and numerous other mainframes, mini computers, and PCs.  OutRight for DOS and Windows also supports 4mm, 8mm, and DLT tape drives.

Host Adapters Tested
APA™-348  
APA™-1460  
AVA™-1505  
AHA®-1510  
AVA™-1515  
AHA®-1520/2  
AHA®-1530/2P  
AHA®-1540/2/F/P  
AHA®-1640  
AHA®-1740/2/4  
AHA®-2740/2/4/T/W  
AHA®-2840/2VL  
AHA®-2940/4/W  
AHA®-3940/W

Chi Corporation
31200 Carter Street
Solon, OH 44139
USA
Phone	(216) 349-8605
Fax	(216) 349-8609
Toll free	(800) 828-0599

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

PERIPHERALS	205

Winter, 1996

Digi-Data

	Model Z

	Digi-Data’s Model Z is an intelligent disk controller designed to manage an array of up to 35 SCSI disk drives in a RAID 0 (striping), 
	RAID 3 (parallel transfer) or RAID 5 (independent transfer) mode of operation.  The Model Z provides a high-bandwidth, Fast and Wide 
	SCSI-2 connection to the host, and a Fast SCSI-2 connection to the disk drives.

Host Adapters Tested
AHA®-1510  
AHA®-1520/2  
AHA®-1530/2P  
AHA®-1540/2/F/P  
AHA®-1640  
AHA®-1740/2/4  
AHA®-2840/2VL

Digi-Data
8580 Dorsey Run Road
Jessup, MD 20794
Phone	(301) 498-0200
Fax	(301) 498-0771
Toll free	(800) 782-6395

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

PERIPHERALS	206

Winter, 1996

ECRM Inc.

	Scriptsetter

	The ECRM Scriptsetter product line encompasses a range of Postscript imagesetters starting at the entry-level VR30 at 12 inches wide.  
	The top of the line is the Knockout which images up to 18 inches wide and includes productivity features such as built in registration 
	punches and buffering for on-line film processing.  The software Postscript RIP is available for the MAC, PoweMAC, Windows® and 
	Windows® NT.  (DEC Alpha  and Intel)

Host Adapters Tested
AHA®-1540/2/F/P

ECRM Inc.
554 Clark Road
Tewksbury, MA 01876
USA
Phone	1-800-537-3276
Fax	508-851-7016
Toll free	1-800-537-3276
E-mail	@ecrm.com

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

PERIPHERALS	207

Winter, 1996

Envisions Solutions Technology, Inc

	ENV6600S

	The ENV6600S is a 24 bit color flatbed scanner capable of 4800 DPI, 16 million colors, OCR and more.  Operating platforms include 
	PC/Windows and Macintosh.  The TWAIN based scanning software can easily be configured to use an Adaptec SCSI card.

Host Adapters Tested
AVA™-1505  
AHA®-1510  
AHA®-1520/2  
AHA®-1540/2/F/P  
AHA®-2840/2VL

Envisions Solutions Technology, Inc
822 Mahler Road
Burlingame, CA 94010
USA
Phone	(415)692-9061
Fax	(415)692-9064

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

PERIPHERALS	208

Winter, 1996

Exabyte

	EXB-1500

	Award-winner -- PC Magazine's "Editor's Choice" and PC World's "Best Buy."  A perfect match for desktop PC/ATs.  Quarter-inch tape 
	drive features 680-megabyte capacity, transfer rates up to 9.3 megabytes per minute.  High performance and low price.  Read, write in 
	choice of tape formats:  3020 or 3010.  2-year warranty, worldwide support.

Host Adapters Tested
AHA®-1510  
AHA®-1520/2  
AHA®-1540/2/F/P  
AHA®-2940/4/W

Exabyte
1685 38th Street
Boulder, CO 80301
USA
Phone	(303) 442-4333
Fax	(303) 447-7689
Toll free	800-EXA-BYTE

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

PERIPHERALS	209

Winter, 1996

Exabyte

	EXB-2501

	A gigabyte in under 25 minutes -- stores data at more than twice the speed of comparable products.  With the fastest search rate in its
	 class (34 megabytes per minute), this affordable quarter-inch drive outperforms the competition.  3.5 inch form factor, embedded 
	SCSI-1 and SCSI-2.  2-year warranty, worldwide phone and fax support.

Host Adapters Tested
AHA®-1510  
AHA®-1520/2  
AHA®-1540/2/F/P  
AHA®-2940/4/W

Exabyte
1685 38th Street
Boulder, CO 80301
USA
Phone	(303) 442-4333
Fax	(303) 447-7689
Toll free	800-EXA-BYTE

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

PERIPHERALS	210

Winter, 1996

Exabyte

	EXB-4200 and EXB-4200c

	Big performance, small package.  DAT drive with 2-gigabyte capacity, 14-megabyte-per-minute transfer rate, 20-second average access.  
	Quick, compact and reliable.  Fully compatible with all major applications for Windows and network environments.  Optional data 
	compression (EXB-4200c) doubles capacity and transfers.  SCSI-1 and SCSI-2.  2 year warranty, worldwide phone and fax support.

Host Adapters Tested
AHA®-1510  
AHA®-1520/2  
AHA®-1540/2/F/P  
AHA®-2940/4/W

Exabyte
1685 38th Street
Boulder, CO 80301
USA
Phone	(303) 442-4333
Fax	(303) 447-7689
Toll free	800-EXA-BYTE

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

PERIPHERALS	211

Winter, 1996

Exabyte

	EXB-8205XL

	The safeguard of single server networks.  Stores 7 gigabytes of compressed data on one EXATAPE™ 160mXL 8mm Data Cartridge.  Use 
	industry-standard 8200 tape formats for easy data interchange.  Compressed data transfer rates to 32 megabytes per minute, full 
	compatibility with all major software and hardware.  2-year warranty, worldwide support.

Host Adapters Tested
AHA®-1510  
AHA®-1520/2  
AHA®-1540/2/F/P  
AHA®-2940/4/W

Exabyte
1685 38th Street
Boulder, CO 80301
USA
Phone	(303) 442-4333
Fax	(303) 447-7689
Toll free	800-EXA-BYTE

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

PERIPHERALS	212

Winter, 1996

Exabyte

	EXB-8505XL

	Internationally acclaimed:  the 8mm standard of excellence.  Features 14-gigabyte compressed capacity, transfer rates up to 60 
	megabytes per minute.  5.25-inch half-high drive can interchange data with full-high models.  Advanced Compression Integrity Check™ for
	 data integrity.  Super compatibility with all major hardware and software.  SCSI-1 and SCSI-2.  2-year warranty, worldwide support.

Host Adapters Tested
AHA®-1510  
AHA®-1540/2/F/P  
AHA®-2940/4/W

Exabyte
1685 38th Street
Boulder, CO 80301
USA
Phone	(303) 442-4333
Fax	(303) 447-7689
Toll free	800-EXA-BYTE

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

PERIPHERALS	213

Winter, 1996

Exabyte

	EXB-10h

	A compact power tower of storage automation.  Affordable, plug-and-play library backup:  capacity up to 140 gigabytes, transfers to 1 
	megabyte per second.  Reliable robotics, LCD status screen, key-lock security.  Complete with EXB-8505XL tape drive, 10 EXATAPE™ 8mm 
	160mXL Data Cartridges and Data Cartridge magazine.  Interface:  SCSI-2.  Worldwide phone, fax support.

Host Adapters Tested
AHA®-1510  
AHA®-1520/2  
AHA®-1540/2/F/P  
AHA®-2940/4/W

Exabyte
1685 38th Street
Boulder, CO 80301
USA
Phone	(303) 442-4333
Fax	(303) 447-7689
Toll free	800-EXA-BYTE

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

PERIPHERALS	214

Winter, 1996

Exabyte

	EXB-210

	Collect, protect and control -- up to 154 gigabytes at transfer rates of  2 megabytes a second.  Available with 1 or 2 EXB-8505XL 
	half-high drives, the EXB-210 accommodates 11 EXATAPE™ Data Cartridges.  Average cartridge access:  <10 seconds.  Supports HSM, imaging
	 and remote storage functions.  2-year warranty.  Worldwide phone, fax support.

Host Adapters Tested
AHA®-1510  
AHA®-1520/2  
AHA®-1540/2/F/P  
AHA®-2940/4/W

Exabyte
1685 38th Street
Boulder, CO 80301
USA
Phone	(303) 442-4333
Fax	(303) 447-7689
Toll free	800-EXA-BYTE

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

PERIPHERALS	215

Winter, 1996

Exabyte

	EXB-440 and EXB-480

	Time-tested, field-proven and elegant.  Command up to 1.12 terabytes of compressed data at transfer rates of 4 megabytes per second.  
	HSM, imaging and remote storage support.  Includes Exabyte robotics, security interlock, modular design, LCD screen and bar code 
	reader.  Interface:  SCSI-2.  2-year warranty, worldwide phone and fax support.

Host Adapters Tested
AHA®-1510  
AHA®-1520/2  
AHA®-1540/2/F/P  
AHA®-2940/4/W

Exabyte
1685 38th Street
Boulder, CO 80301
USA
Phone	(303) 442-4333
Fax	(303) 447-7689
Toll free	800-EXA-BYTE

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

PERIPHERALS	216

Winter, 1996

Florida Datamation

	Data On Demand

	Data On Demand is a fault tolerance disk array with user programmable RAID 0, 3 and 5. It supports up to 24GB with desk side and 96GB 
	with rack mount. Features include hot swap data and power modules, and redundant fan and I/O control.

Host Adapters Tested
AHA®-1540/2/F/P  
AHA®-1640  
AHA®-1740/2/4  
AHA®-2740/2/4/T/W  
AHA®-2840/2VL  
AHA®-2940/4/W

Florida Datamation
AMTEC Center, 6405 Congress Ave, Suite 140
Boca Raton, FL 33487
Phone	(407) 241-2966
Fax	(407) 241-3108
Toll free	(800) 642-5938
E-mail	sales@fdma.com

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

PERIPHERALS	217

Winter, 1996

Fujitsu Computer - Intellistor Division

	M160X

	Fujitsu's M160x series of low-profile 3.5" SCSI-2 Winchester disk drives are designed to deliver cost-effective storage solutions for a
	 variety of environments and applications without sacrificing performance or reliability.  These one-inch-high drives offer formatted 
	capacities of 540 and 1080 MB.  They combine a high rotational 5,400 rpm spindle motor, 10 ms seek time and high data transfer rates up
	 to 7.8 MB/s with advanced caching and intelligent power management to provide users with the highest capacity/performance solution for
	 today's server and workstation applications.

Host Adapters Tested
AHA®-1510  
AVA™-1515  
AHA®-1520/2  
AHA®-1530/2P  
AHA®-1540/2/F/P  
AHA®-1640  
AHA®-2740/2/4/T/W  
AHA®-2840/2VL  
AHA®-2940/4/W

Fujitsu Computer - Intellistor Division
2402 Clover Basin Drive
Longmont, CO 80503
USA
Phone	303-682-6400
Fax	303-682-6401

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

PERIPHERALS	218

Winter, 1996

Fujitsu Computer - Intellistor Division

	DynaMO 230

	At one-inch-high, DynaMO 230 is the world's smallest magneto-optical disk drive.  DynaMO 230 packs 230 MB of information onto 
	industry-standard 3.5-inch cartridges.  It also read/writes to 128 MB DynaMO media.  The high 3,600 rpm rotational rate and fast 30 ms 
	average seek time combine to give data transfer rates of up to 2.1 MB per second.  Its 237KB read and write cache/buffer further 
	increases DynaMO 230's performance.

Host Adapters Tested
APA™-1460  
AHA®-1510  
AVA™-1515  
AHA®-1520/2  
AHA®-1530/2P  
AHA®-1540/2/F/P  
AHA®-1640  
AHA®-2740/2/4/T/W  
AHA®-2840/2VL  
AHA®-2940/4/W

Fujitsu Computer - Intellistor Division
2402 Clover Basin Drive
Longmont, CO 80503
USA
Phone	303-682-6400
Fax	303-682-6401

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

PERIPHERALS	219

Winter, 1996

Fujitsu Computer - Intellistor Division

	M251XA

	The M251xA is the industry's first one-inch profile, 3.5-inch magneto-optical disk drive for the 230MB media.  The 251xA maintains 
	downward compatibility with other 128MB media, and meets ISO standards.  Behind the one-inch-high design is our unique spindle loading 
	technology.  The low profile M251xA allows it to be easily installed into personal computers and workstations.

Host Adapters Tested
APA™-1460  
AHA®-1510  
AVA™-1515  
AHA®-1520/2  
AHA®-1530/2P  
AHA®-1540/2/F/P  
AHA®-1640  
AHA®-2740/2/4/T/W  
AHA®-2840/2VL  
AHA®-2940/4/W

Fujitsu Computer - Intellistor Division
2402 Clover Basin Drive
Longmont, CO 80503
USA
Phone	303-682-6400
Fax	303-682-6401

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

PERIPHERALS	220

Winter, 1996

Fujitsu Computer - Intellistor Division

	M270X

	Fujitsu's M270x drives are the first 5,400 rpm 2.5" form factor disk drive that provides true server-class performance for today's 
	notebooks and portables.  The M270x provides up to 530 MB of formatted capacity by combining Fujitsu's Magneto-resistive (MR) heads and
	 digital read channel (PR4ML) technology, advanced caching techniques, and spindle synchronization.  The 270's performance advantages 
	include a 512KB programmable cache, high internal transfer rates, tagged command queuing/reordering, 12 ms average access time, and 
	Fujitsu's Intelligent Power Management scheme to support the latest Energy Star standards.

Host Adapters Tested
AHA®-1510  
AVA™-1515  
AHA®-1520/2  
AHA®-1530/2P  
AHA®-1540/2/F/P  
AHA®-1640  
AHA®-2740/2/4/T/W  
AHA®-2840/2VL  
AHA®-2940/4/W

Fujitsu Computer - Intellistor Division
2402 Clover Basin Drive
Longmont, CO 80503
USA
Phone	303-682-6400
Fax	303-682-6401

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

PERIPHERALS	221

Winter, 1996

Fujitsu Computer - Intellistor Division

	M290X

	Fujitsu's M290X combine magneto-resistive (MR) heads with digital read channel electronics (PR4ML) and advanced caching techniques to 
	deliver ultimate performance and capacity.  Rotational speeds of 5,400 rpm, 5.6 ms rotational latency, spindle synchronization, sub 10 
	ms seek times, high internal transfer rates, and many other high performance features make the M290X a leader in the mass storage 
	industry.  Drives are also available with Fast or Wide SCSI-2 interfaces.

Host Adapters Tested
AHA®-1510  
AVA™-1515  
AHA®-1520/2  
AHA®-1530/2P  
AHA®-1540/2/F/P  
AHA®-1640  
AHA®-2740/2/4/T/W  
AHA®-2840/2VL  
AHA®-2940/4/W

Fujitsu Computer - Intellistor Division
2402 Clover Basin Drive
Longmont, CO 80503
USA
Phone	303-682-6400
Fax	303-682-6401

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

PERIPHERALS	222

Winter, 1996

Fujitsu Computer - Intellistor Division

	M291X

	Fujitsu's M291X combine magneto-resistive (MR) heads with digital read channel electronics (PR4ML) and advanced caching techniques to 
	deliver ultimate performance and capacity.  Rotational speeds of 7,200 rpm, sub-5.6 ms rotational latency, spindle synchronization, sub
	 10 ms seek times, high internal transfer rates, and many other high performance features make the M291X a leader in the mass storage 
	industry.  Drives are also available with Fast or Wide SCSI-2 interfaces.

Host Adapters Tested
AHA®-1510  
AVA™-1515  
AHA®-1520/2  
AHA®-1530/2P  
AHA®-1540/2/F/P  
AHA®-1640  
AHA®-2740/2/4/T/W  
AHA®-2840/2VL  
AHA®-2940/4/W

Fujitsu Computer - Intellistor Division
2402 Clover Basin Drive
Longmont, CO 80503
USA
Phone	303-682-6400
Fax	303-682-6401

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

PERIPHERALS	223

Winter, 1996

Fujitsu Computer - Intellistor Division

	M293X

	Fujitsu's M293X combine magneto-resistive (MR) heads with digital read channel electronics (PR4ML) and advanced caching techniques to 
	deliver ultimate performance and capacity.  Rotational speeds of 7,200 rpm, sub-5 ms rotational latency, spindle synchronization, 10 ms
	 seek times, fast internal transfer rates, and many other high performance features make the M293X a leader in the mass storage 
	industry.  Drives are also available with Fast/Wide/Single Ended/Differential/SCA interfaces.

Host Adapters Tested
AHA®-1510  
AVA™-1515  
AHA®-1520/2  
AHA®-1530/2P  
AHA®-1540/2/F/P  
AHA®-1640  
AHA®-2740/2/4/T/W  
AHA®-2840/2VL  
AHA®-2940/4/W

Fujitsu Computer - Intellistor Division
2402 Clover Basin Drive
Longmont, CO 80503
USA
Phone	303-682-6400
Fax	303-682-6401

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

PERIPHERALS	224

Winter, 1996

HCL Hewlett Packard Ltd.

	Busy Bee and Meteor

	The HCL-Hewlett Packard Busy Bee and Meteor Systems are developed in India for use in the Indian market.  They are highly scalable 
	designs starting from home PC low-end configurations to large business UNIX and NetWare servers.

Host Adapters Tested
AHA®-1520/2  
AHA®-1540/2/F/P  
AHA®-1740/2/4  
AHA®-2740/2/4/T/W  
AHA®-2940/4/W  
AHA®-2940/4/U/UW

HCL Hewlett Packard Ltd.
E4, E5, E6 Sector 11, Noida
Dist Ghaziabad,  201301
India
Phone	91-11-8531353
Fax	91-11-8521113

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

PERIPHERALS	225

Winter, 1996

Hewlett-Packard Company

	HP SureStore Tape 5000

	The HP SureStore Tape 5000 provides reliable backup for high-end PCs and UNIX workstations, as well as peer-to-peer and server-based 
	networks.  
	  
	The HP SureStore Tape 5000i is a 5.25-inch, half-height internal drive.  The HP SureStore Tape 5000e and 5000eU are external drives.  
	  
	The products come complete with everything you need for backup, including Colorado Backup for Windows, diagnostics and accessories.  
	  
	You can choose from a long list of compatible software solutions.  HP SureStore Tape Premier Solutions are industry-leading software 
	solutions which are supplied and supported by HP.  HP SureStore Tape Referenced Solutions are supplied by industry-leading vendors and 
	are fully tested for compatibility with HP SureStore Tape products.  
	  
	Key Features  
	· Typically 4 GB of unattended backup in just over three hours using hardware data compression   
	· HP’s reliable DAT technology   
	· Industry-standard DDS-DC format   
	· Includes Colorado Backup for Windows  
	· Compatible with a wide range of operating systems and software solutions  
	· HP service and support

Host Adapters Tested
APA™-348  
APA™-358  
APA™-1460  
AHA®-1510  
AHA®-1520/2  
AHA®-1540/2/F/P  
AHA®-1640  
AHA®-1740/2/4  
AHA®-2740/2/4/T/W  
AHA®-2940/4/W  
AHA®-2940/4/U/UW

Hewlett-Packard Company
Computer Peripherals Bristol, Filton Road, Stoke Gifford
Bristol, Avon BS12 6QZ
England
Phone	(44) 117-9228304
Fax	(44)117-9799910
E-mail	adrian_kerton@hp.com
URL	http://www.hp.com/go/dat

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

PERIPHERALS	226

Winter, 1996

Hewlett-Packard Company

	HP SureStore Tape 6000

	The HP SureStore Tape 6000 provides reliable backup for high-end PCs and UNIX workstations, as well as peer-to-peer and server-based 
	networks.  
	  
	The HP SureStore Tape 6000i is a 5.25-inch, half-height internal drive.  The HP SureStore Tape 6000e and 6000eU are external drives.  
	  
	The products come complete with everything you need for dependable backup, including Colorado Backup for Windows, diagnostics and 
	accessories.  
	  
	You can choose from a long list of compatible software solutions.  HP SureStore Tape Premier Solutions are industry-leading software 
	solutions which are supplied and supported by HP.  HP SureStore Tape Referenced Solutions are supplied by industry-leading vendors and 
	are fully tested for compatibility with HP SureStore Tape products.  
	  
	Key Features  
	· Typically 8 GB of unattended backup in just over two hours using hardware data compression   
	· HP’s reliable DAT technology   
	· Industry-standard DDS-2 format   
	· Includes Colorado Backup for Windows   
	· Compatible with a wide range of operating systems and software solutions   
	· HP service and support

Host Adapters Tested
APA™-348  
APA™-358  
APA™-1460  
AHA®-1510  
AHA®-1520/2  
AHA®-1540/2/F/P  
AHA®-1640  
AHA®-1740/2/4  
AHA®-2740/2/4/T/W  
AHA®-2940/4/W  
AHA®-2940/4/U/UW

Hewlett-Packard Company
Computer Peripherals Bristol, Filton Road, Stoke Gifford
Bristol, Avon BS12 6QZ
England
Phone	(44) 117-9228304
Fax	(44)117-9799910
E-mail	adrian_kerton@hp.com
URL	http://www.hp.com/go/dat

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

PERIPHERALS	227

Winter, 1996

Hewlett-Packard Company

	HP SureStore Tape 2000

	The HP SureStore Tape 2000 provides reliable backup for highend PCs and UNIX workstations, as well as small peer-to-peer and 
	server-based networks.  
	  
	The HP SureStore Tape 2000i is a 5.25 inch, half height internal drive.  The HP SureStore Tape 2000e is an external drive.  
	  
	The products come complete with everything you need for dependable backup, including Colorado Backup for Windows, diagnostics and 
	accessories.  
	  
	You can choose from a long list of compatible software solutions.  HP SureStore Tape Premier Solutions are the industry leading 
	software solutions which are supplied and supported by HP.  HP SureStore Tape Referenced Solutions are supplied by industry leading 
	vendors and are fully tested for compatibility with HP SureStore Tape products.  
	  
	Key Features  
	· 2 GB of unattended backup in just over three hours   
	· HP’s reliable DAT technology   
	· Industry-standard DDS format   
	· Includes Colorado Backup for Windows   
	· Compatible with a wide range of operating Systems and Software solutions   
	· HP service and support  
	· Compatible with a wide range of operating systems and software solutions   
	· HP service and support

Host Adapters Tested
APA™-348  
APA™-358  
APA™-1460  
AHA®-1510  
AHA®-1520/2  
AHA®-1540/2/F/P  
AHA®-1640  
AHA®-1740/2/4  
AHA®-2740/2/4/T/W  
AHA®-2940/4/W  
AHA®-2940/4/U/UW

Hewlett-Packard Company
Computer Peripherals Bristol, Filton Road, Stoke Gifford
Bristol, Avon BS12 6QZ
England
Phone	(44) 117-9228304
Fax	(44)117-9799910
E-mail	adrian_kerton@hp.com
URL	http://www.hp.com/go/dat

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

PERIPHERALS	228

Winter, 1996

Hewlett-Packard Company

	HP SureStore Tape 12000e

	The HP SureStore Tape 12000e autoloader offers 48 GB of reliable, high performance storage.  
	  
	The autoloader can be combined with your choice of software solutions to meet a wide range of requirements, such as automated backup of
	 workgroup servers centralized backup of enterprise multi-server networks as well as archive and hierarchical storage management 
	applications.  
	  
	To help ensure worry-free operation, products include lifetime telephone support and HP’s one year Express Exchange warranty.  
	  
	Key Features  
	· A typical capacity of 8 GB per cartridge using hardware data compression, for a typical capacity of 48 GB per magazine   
	· High-speed data transfer and high-speed file retrieval   
	· Compatible with a wide range of operating and software solutions   
	· HP reliable DAT technology ensures the protection of your valuable data   
	· Industry standard DDS-2 format provides interchange with other DDS tape drives   
	· HP service and support

Host Adapters Tested
AHA®-2940/4/W

Hewlett-Packard Company
Computer Peripherals Bristol, Filton Road, Stoke Gifford
Bristol, Avon BS12 6QZ
England
Phone	(44) 117-9228304
Fax	(44)117-9799910
E-mail	adrian_kerton@hp.com
URL	http://www.hp.com/go/dat

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

PERIPHERALS	229

Winter, 1996

Interface Data

	DX-SCSI

	DX-SCSI is a tape drive subsystem for backup and data exchange including interactive, menu-driven software.  It supports character set 
	conversion, fixed and variable length records, various record separators, and several standard tape formats.  It is compatible with 
	most SCSI tape drives and ideal for exchange of tapes with mainframes.

Host Adapters Tested
AHA®-1510  
AHA®-1520/2  
AHA®-1540/2/F/P  
AHA®-1640  
AHA®-1740/2/4

Interface Data
600 West Cummings Park, Suite 3100
Woburn, MA 01801
USA
Phone	(617) 938-6333
Fax	(617) 938-0626
Toll free	(800) 370-3282

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

PERIPHERALS	230

Winter, 1996

JNL Computer Products, Inc.

	DataPort

	JNL's DataPort is a US patented removable storage adapter.  It has a hot-swappable capability that allows any 3.5" hard drive to be 
	swapped while the computer continues to run.  DataPort is form-fitted to any standard 5.25" drive bay.  It is ideal for data security, 
	portability, back-up and RAID applications.  There are IDE, SCSI, aluminum and plastic options.  The US patent no. protecting this type
	 of device is #4,941,841 & des. 308,052.

Host Adapters Tested
AHA®-1540/2/F/P  
AHA®-1640  
AHA®-1740/2/4  
AHA®-2740/2/4/T/W  
AHA®-2840/2VL

JNL Computer Products, Inc.
4512 Enterprise St.
Fremont, CA 94538
Phone	(510)353-0262
Fax	(510)353-0266
Toll free	(800)283-5123

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

PERIPHERALS	231

Winter, 1996

LaserByte

	LB4230 MO Drive (3.5" 230MB)

	The LB4230 rewritable optical disk drive utilizes state-of-the-art Magnetico Optical technology.  With off-the-shelf, low cost optical 
	media it offers the following features:  
	* 25.4mm (1 inch) high 3.5" form factor, which will fit into any floppy location  
	* standard SCSI-II interface  
	* patented autowrite calibration sequence that optimizes the laser power read/write operations to ensure consistent high performance 
	across a wide range of environmental conditions and media  
	* the lowest power requirement of a 3.5" drive, requiring only +5vDC  
	* the lowest power dissipation at only 4.7 Watts average, and   
	* a Smart Power Sleep mode, which cuts power to 1 Watt when not in use.

Host Adapters Tested
AHA®-1520/2  
AHA®-1540/2/F/P

LaserByte
1330 Bordeaux Drive
Sunnyvale, CA 94089
Phone	(408) 734-9200
Fax	(408) 734-5471
Toll free	(800) 619-9200

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

PERIPHERALS	232

Winter, 1996

Legacy Storage Systems

	Legacy Tape Drives

	Legacy manufactures a complete line of Legacy Tape Drives that can incorporate 8mm Helical-Scan, DAT (Digital Audio Tape) or QIC 
	(Quarter-Inch Cartridge) tape technologies.  All of Legacy’s tape solutions are tested and developed to ensure successful integration 
	with a customer’s primary disk storage.  Some of the family’s many features include:  capacities ranging from 60 MB to over 10 GB; QFA 
	(Quick File Access) capabilities for fast file retrieval; and data transfer rates approaching over 72 MB/minute for Legacy’s higher-end
	 tape family members.  

	  
	  
	Canadian  Corporate Headquarters  
	43 Riviera Drive  
	Markham, Ontario L3R 5J6  
	Canada  
	Tel:  (905)475-1077  
	Fax:  (905)475-1088

Host Adapters Tested
AVA™-1505  
AHA®-1510  
AVA™-1515  
AHA®-1520/2  
AHA®-1530/2P  
AHA®-1540/2/F/P  
AHA®-1640  
AHA®-1740/2/4  
AHA®-2740/2/4/T/W  
AHA®-2840/2VL  
AHA®-2940/4/W

Legacy Storage Systems
138 River Road, Suite 204
Andover, MA 01810
USA
Phone	(508) 681-8400
Fax	(508) 689-9004
Toll free	(800) 966-6442

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

PERIPHERALS	233

Winter, 1996

Legacy Storage Systems

	Smart Array®, Smart Array XE

	Legacy's SmartArray® family of disk array subsystems offer the best combination of performance and fault tolerance for mission-critical
	 servers.  Available as either a storage tower or rack-mount, SmartArray subsystems accommodate every major storage technology:  hard 
	disk, CD-ROM, and tape (DAT, QIC, and 8mm).  Devices and power supplies are hot-swappable for zero-downtime applications.  The advanced
	 intelligent monitor displays device, power supply, temperature, and fan status.  It also monitors RAID rebuilds and detects duplicate 
	SCSI IDs.  Visual and audio alarms indicate error conditions, and messages can be broadcast by MHS or SNMP, or via pager.    
	  
	SmartArray supports up to 6 SCSI-3 Fast/Wide buses, and all major operating systems.  

	  
	Canadian  Corporate Headquarters  
	43 Riviera Drive  
	Markham, Ontario L3R 5J6  
	Canada  
	Tel:  (905)475-1077  
	Fax:  (905)475-1088

Host Adapters Tested
AHA®-1640  
AHA®-1740/2/4  
AHA®-2740/2/4/T/W  
AHA®-2940/4/W  
AHA®-3940/W

Legacy Storage Systems
138 River Road, Suite 204
Andover, MA 01810
USA
Phone	(508) 681-8400
Fax	(508) 689-9004
Toll free	(800) 966-6442

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

PERIPHERALS	234

Winter, 1996

Logicraft Information Systems

	The Jukebox Manager

	The Jukebox Manager™ option for Logicraft's LanCD™ network server software provides a versatile solution for networked access to 
	archived CD-ROM storage.  It is modular in design, hardware independent and non-vendor specific for jukebox support.  Features include 
	Document Image Management, static directory or platter caching and DDC (dynamic hard disk cache), asynchronous access, multiple jukebox
	 support, Intelligent Optical Reader Selection, local on-line management, and support for up to 1280 platters and 56 readers per LanCD 
	server.  With up to 10 servers per client, each user could have access to more than 12 thousand CD-ROM discs.

Host Adapters Tested
AHA®-1540/2/F/P  
AHA®-1740/2/4  
AHA®-2740/2/4/T/W  
AHA®-2940/4/W  
AHA®-3940/W

Logicraft Information Systems
22 Cotton Road
Nashua, NH 03063
Phone	603-880-0300
Fax	(603) 880-7229
Toll free	800-880-5644
E-mail	sales@logicraft.com
URL	http://www.logicraft.com

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

PERIPHERALS	235

Winter, 1996

Logicraft Information Systems

	FastCD™, LanCD

	FastCD™ is an option available with Logicraft's LanCD™ networking software for providing multiple concurrent access to CD-ROM 
	applications in a multi-platform, multi-protocol networking environment.  FastCD creates "virtual CD-ROM discs" on fast, high 
	performance SCSI hard drives by caching the entire contents of a CD-ROM in its native format onto a FastCD partition of the hard disk, 
	providing users with easy access to their CD-ROM applications at hard disk speeds up to 300 times faster than standard CD-ROM drives.  
	FastCD software includes comprehensive status reports, multimedia support, and asynchronous disk access for higher throughput during 
	multiple concurrent accessing.

Host Adapters Tested
AHA®-1540/2/F/P  
AHA®-1740/2/4  
AHA®-2740/2/4/T/W  
AHA®-2940/4/W  
AHA®-3940/W

Logicraft Information Systems
22 Cotton Road
Nashua, NH 03063
Phone	603-880-0300
Fax	(603) 880-7229
Toll free	800-880-5644
E-mail	sales@logicraft.com
URL	http://www.logicraft.com

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

PERIPHERALS	236

Winter, 1996

Logicraft Information Systems

	CDexecutive™ CD-ROM Network Server

	The CDexecutive /XF5500 CD-ROM network server provides a turnkey solution for multiple concurrent accesses to CD-ROM applications in a 
	multi-platform, multi-protocol environment.  The Pentium™ based XF hardware architecture is bundled with Logicraft's high performance 
	CDexecutive Management Center software that automatically monitors and manages CD-ROM applications as a background Windows NT™ service.
	  Client support includes Windows® 95, Windows® for Workgroups, Macintosh® and NetWare clients.  The XF server holds up to 14 SCSI 
	devices and comes equipped with IDE hard drive, network interface card, floppy drive and SCSI host adapters.  It runs at 120MHz, has 
	32MB of RAM and supports up to 56 SCSI devices.

Host Adapters Tested
AHA®-2740/2/4/T/W

Logicraft Information Systems
22 Cotton Road
Nashua, NH 03063
Phone	603-880-0300
Fax	(603) 880-7229
Toll free	800-880-5644
E-mail	sales@logicraft.com
URL	http://www.logicraft.com

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

PERIPHERALS	237

Winter, 1996

Logicraft Information Systems

	LanCD™ CD-ROM Network Servers

	The LanCD/XF family of CD-ROM network servers provides a turnkey solution for multiple concurrent accesses to CD-ROM applications in a 
	multi-platform, multi-protocol environment.  The Pentium™ based XF hardware architecture is bundled with Logicraft's high-performance 
	LanCD and FastCD™ software that supports DOS, Windows® and Windows® 95 clients.  Optional support is available for Windows NT® and 
	Macintosh clients.  Each chassis holds up to 14 SCSI devices and comes equipped with IDE hard drive, network interface card, floppy 
	drive and SCSI host adapters.  The XF5300 runs at 75MHz, has 16MB of RAM and expands to 28 drives.  The XF5500 runs at 120MHz, has 32MB
	 and supports up to 56 drives.

Host Adapters Tested
AHA®-1520/2  
AHA®-1540/2/F/P  
AHA®-1640  
AHA®-1740/2/4  
AHA®-2740/2/4/T/W  
AHA®-2940/4/W  
AHA®-3940/W

Logicraft Information Systems
22 Cotton Road
Nashua, NH 03063
Phone	603-880-0300
Fax	(603) 880-7229
Toll free	800-880-5644
E-mail	sales@logicraft.com
URL	http://www.logicraft.com

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

PERIPHERALS	238

Winter, 1996

Lumisys Inc

	Rayven

	Through XRS' patented "SC" and "NL" technologies, the Rayven series scanners and "SC" flatbed models are able to attain a wide optical 
	density range normally found in more costly, less rugged laser-based scanners.

Host Adapters Tested
AVA™-1505  
AHA®-1510  
AHA®-1540/2/F/P

Lumisys Inc
225 Humboldt Ct
Sunnyvale, CA 94089
USA
Phone	408-733-6565
Fax	408-733-6567

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

PERIPHERALS	239

Winter, 1996

Maxoptix Corporation

	T4-2600

	The T4-2600 is a new 5.25" multifunction optical disk drive with 2.6GB capacity.  It provides unlimited transportable storage at an 
	excellent value, offering unparalleled reliability, a fast seek rate up to 4.0 MB/second transfer rate and with 1 read/write cache, it 
	delivers an outstanding performance.  The T4-2600 drive conforms to ISO specifications and accepts three ISO standard media formats - 
	2.6GB, 1.3GB and 650MB.  
	This drive is reliable, affordable and high performance.  The media can be written and erased more than 10,000,000 times.

Host Adapters Tested
AHA®-1540/2/F/P  
AHA®-1640  
AHA®-1740/2/4  
AHA®-2740/2/4/T/W  
AHA®-2940/4/W  
AHA®-3940/W

Maxoptix Corporation
3342 Gateway Blvd.
Fremont, CA 94538
USA
Phone	(510) 353-9700
Fax	(510) 353-1845
Toll free	(800) 848-3092

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

PERIPHERALS	240

Winter, 1996

Maxoptix Corporation

	MaxLyb

	The Maxoptix MaxLyb family of optical auto changers utilizes the T4-2600 drives to deliver high performance and reliable 
	specifications.  The MaxLyb family covers a wide range of capacities - 26GB to over 600GB, which ensures the most useful library is 
	available for a variety of applications.  
	  
	With the MaxLyb family of optical storage libraries, Maxoptix offers the widest selection of optical library solutions and fills the 
	price-performance gaps left by other storage technologies.  With the fastest on-line access to stored data and information, they are 
	the logical choice for those who need top performance, demonstrated reliability and future expandability at competitive prices.

Host Adapters Tested
AHA®-1540/2/F/P  
AHA®-1640  
AHA®-1740/2/4  
AHA®-2740/2/4/T/W  
AHA®-2940/4/W  
AHA®-3940/W

Maxoptix Corporation
3342 Gateway Blvd.
Fremont, CA 94538
USA
Phone	(510) 353-9700
Fax	(510) 353-1845
Toll free	(800) 848-3092

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

PERIPHERALS	241

Winter, 1996

Maxtor Southern Europe

	7000 Series

	7000 Series SCSI disk drives are 1' x 3.5" high random access storage devices using an on-board SCSI controller. Reduced size, 
	increased durability and low power consumption make them especially well suited to notebook, laptop and desktop applications.

Host Adapters Tested
AHA®-1520/2  
AHA®-1540/2/F/P  
AHA®-1640  
AHA®-1740/2/4  
AHA®-2740/2/4/T/W  
AHA®-2940/4/W  
AHA®-2940/4/U/UW  
AHA®-3940/W

Maxtor Southern Europe
18 rue Saarinen
Rungis,  94568
France
Phone	(33) 1-46-86-20-98
Fax	(33) 1-46-87-35-19
E-mail	BrunoCourtois@maxtor.com

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

PERIPHERALS	242

Winter, 1996

Media Integration, Inc.

	Intelligent Storage

	Intelligent Storage™ is a fault-tolerant SCSI storage subsystem for hard disks, optical disks and tape drives.  Features include 
	distributed power with redundant, hot removable and replaceable power supplies and removable storage devices, including those with 
	removable media.  It provides the highest level of fault tolerant, redundant power and removability while continuing full operation.  
	It will accept any standard 5.25" or 3.5" storage device.

Host Adapters Tested
AHA®-1510  
AHA®-1520/2  
AHA®-1540/2/F/P  
AHA®-1640  
AHA®-1740/2/4  
AHA®-2740/2/4/T/W

Media Integration, Inc.
3949 Research Park Court, Suite 190
Soquel, CA 95073
USA
Phone	(408) 475-9400
Fax	(408) 475-0110
Toll free	(800) 824-7385

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

PERIPHERALS	243

Winter, 1996

Media Integration, Inc.

	Media SmartStor

	Media SmartStor™ provides RAID levels 0, 1, and 5, with full data and power supply fault tolerant support.  Removable data and power 
	supply with continuous operation and user-defined priority for data recovery is provided.    NetWare, UNIX and OS/2 are supported on 
	ISA, EISA and Micro Channel buses.  A scalable number of drives and adapters are used.  The system can support up to 41 drives per SCSI
	 connection.

Host Adapters Tested
AHA®-1540/2/F/P  
AHA®-1640  
AHA®-1740/2/4  
AHA®-2740/2/4/T/W

Media Integration, Inc.
3949 Research Park Court, Suite 190
Soquel, CA 95073
USA
Phone	(408) 475-9400
Fax	(408) 475-0110
Toll free	(800) 824-7385

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

PERIPHERALS	244

Winter, 1996

Media Integration, Inc.

	DAT-Manager

	The DAT-Manager™ provides from 48 GB to 1 Terrabyte of near-line storage of data, thus providing the ability to restore, backup and 
	archive large quantities of data at the lowest cost per MB. Data Librarian software manages all cassettes, even those off-line in cold 
	storage, for quick and automatic recovery.

Host Adapters Tested
AHA®-1510  
AHA®-1520/2  
AHA®-1540/2/F/P  
AHA®-1640  
AHA®-1740/2/4

Media Integration, Inc.
3949 Research Park Court, Suite 190
Soquel, CA 95073
USA
Phone	(408) 475-9400
Fax	(408) 475-0110
Toll free	(800) 824-7385

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

PERIPHERALS	245

Winter, 1996

Media Integration, Inc.

	Opti-Manager

	Opti-Manager™ provides very large near-line or on-line data storage, from 20 GB to 1 Terrabyte and the ability to define the partition 
	or volume to cover an entire data set or any combination subset of cartridge side, whole cartridge or group of cartridges.  Multiple 
	drive access is also available.  Data Librarian software manages all optical cartridges, even those in cold storage, for quick 
	recovery.

Host Adapters Tested
AHA®-1510  
AHA®-1520/2  
AHA®-1540/2/F/P  
AHA®-1640  
AHA®-1740/2/4  
AHA®-2740/2/4/T/W

Media Integration, Inc.
3949 Research Park Court, Suite 190
Soquel, CA 95073
USA
Phone	(408) 475-9400
Fax	(408) 475-0110
Toll free	(800) 824-7385

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

PERIPHERALS	246

Winter, 1996

NSM Jukebox GmbH

	CDR 100 XA Quad Speed

	Single drive (Toshiba XM3501B) quad speed, 100 disk CD-ROM changer, SCSI-2 data interface, RS-232 robotics interface.

Host Adapters Tested
APA™-348  
APA™-1460  
AHA®-1540/2/F/P  
AHA®-2740/2/4/T/W  
AHA®-2940/4/W  
AHA®-3940/W

NSM Jukebox GmbH
IM Tiergarten 20-30
D-55411Bingen,  55411
Germany
Phone	49-6721-964-394
Fax	49-6721-964-414
E-mail	CompuServe 73503,3467

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

PERIPHERALS	247

Winter, 1996

NSM Jukebox GmbH

	CDR 100 Recordable Quad Speed

	Single drive (Yamaha CDR100, 4x) 100 disk CD-R changer, SCSI-2 data interface, RS-232 robotics interface.

Host Adapters Tested
APA™-348  
APA™-1460  
AHA®-1540/2/F/P  
AHA®-2740/2/4/T/W  
AHA®-2940/4/W  
AHA®-3940/W

NSM Jukebox GmbH
IM Tiergarten 20-30
D-55411Bingen,  55411
Germany
Phone	49-6721-964-394
Fax	49-6721-964-414
E-mail	CompuServe 73503,3467

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

PERIPHERALS	248

Winter, 1996

NSM Jukebox GmbH

	CDR 100 XA

	Single drive 100 disk CD-ROM changer, SCSI-2 data interface, RS-232 robotics control, 2x speed, Toshiba XM3401B.

Host Adapters Tested
APA™-358  
APA™-1460  
AHA®-1540/2/F/P  
AHA®-2740/2/4/T/W  
AHA®-2940/4/W  
AHA®-3940/W

NSM Jukebox GmbH
IM Tiergarten 20-30
D-55411Bingen,  55411
Germany
Phone	49-6721-964-394
Fax	49-6721-964-414
E-mail	CompuServe 73503,3467

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

PERIPHERALS	249

Winter, 1996

NSM Jukebox GmbH

	Mercury 20

	150 disk, 2 drive CD-ROM changer, 4x drives (Toshiba XM3501B) SCSI data interface, RS-232 robotics interface.

Host Adapters Tested
APA™-348  
APA™-1460  
AHA®-1540/2/F/P  
AHA®-2740/2/4/T/W  
AHA®-2940/4/W  
AHA®-3940/W

NSM Jukebox GmbH
IM Tiergarten 20-30
D-55411Bingen,  55411
Germany
Phone	49-6721-964-394
Fax	49-6721-964-414
E-mail	CompuServe 73503,3467

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

PERIPHERALS	250

Winter, 1996

NSM Jukebox GmbH

	Mercury 40

	CD-ROM changer with 4 4x drives (Toshiba XM3501B) and 150 CD capacity.  SCSI-2 data interface, RS-232 robotics interface.

Host Adapters Tested
APA™-348  
APA™-1460  
AHA®-1540/2/F/P  
AHA®-1640  
AHA®-2740/2/4/T/W  
AHA®-2940/4/W  
AHA®-3940/W

NSM Jukebox GmbH
IM Tiergarten 20-30
D-55411Bingen,  55411
Germany
Phone	49-6721-964-394
Fax	49-6721-964-414
E-mail	CompuServe 73503,3467

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

PERIPHERALS	251

Winter, 1996

NSM Jukebox GmbH

	Mercury 20 S

	CD-ROM changer with 2 4x CD-ROM drives (Toshiba XM3501B) and 150 CDs capacity. SCSI-2 data and robotics interface.

Host Adapters Tested
APA™-348  
APA™-1460  
AHA®-1540/2/F/P  
AHA®-1640  
AHA®-2740/2/4/T/W  
AHA®-2940/4/W  
AHA®-3940/W

NSM Jukebox GmbH
IM Tiergarten 20-30
D-55411Bingen,  55411
Germany
Phone	49-6721-964-394
Fax	49-6721-964-414
E-mail	CompuServe 73503,3467

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

PERIPHERALS	252

Winter, 1996

NSM Jukebox GmbH

	Mercury 40 S

	CD-ROM changer with 4 4x CD-ROM drives (Toshiba XM3501B) and 150 CDs capacity.  SCSI-2 data and robotics interface.

Host Adapters Tested
APA™-348  
APA™-1460  
AHA®-1540/2/F/P  
AHA®-1640  
AHA®-2740/2/4/T/W  
AHA®-2940/4/W  
AHA®-3940/W

NSM Jukebox GmbH
IM Tiergarten 20-30
D-55411Bingen,  55411
Germany
Phone	49-6721-964-394
Fax	49-6721-964-414
E-mail	CompuServe 73503,3467

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

PERIPHERALS	253

Winter, 1996

NSM Jukebox GmbH

	Mercury 31

	CD-ROM/CD-R changer with 3 4x CD-ROM drives (Toshiba XM3501B), 1 4x CD recorder drive (Yamaha CDR 100), 150 CDs capacity, 2 SCSI-2 data
	 interfaces (1 for CD-ROMs, 1 for recorder).  RS-232 robotics interface.

Host Adapters Tested
APA™-348  
APA™-1460  
AHA®-1540/2/F/P  
AHA®-1640  
AHA®-2740/2/4/T/W  
AHA®-2940/4/W  
AHA®-3940/W

NSM Jukebox GmbH
IM Tiergarten 20-30
D-55411Bingen,  55411
Germany
Phone	49-6721-964-394
Fax	49-6721-964-414
E-mail	CompuServe 73503,3467

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

PERIPHERALS	254

Winter, 1996

NSM Jukebox GmbH

	Mercury 31 S

	CD-ROM/CD-R changer with 3 4x CD-ROM drives (Toshiba XM3501B) and 1 4x recorder drive (Yamaha COR100), 150 CDs capacity.  SCSI-2 data 
	and robotics interface.  Separate SCSI-2 interface for recorder.

Host Adapters Tested
APA™-348  
APA™-1460  
AHA®-1540/2/F/P  
AHA®-1640  
AHA®-2740/2/4/T/W  
AHA®-2940/4/W  
AHA®-3940/W

NSM Jukebox GmbH
IM Tiergarten 20-30
D-55411Bingen,  55411
Germany
Phone	49-6721-964-394
Fax	49-6721-964-414
E-mail	CompuServe 73503,3467

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

PERIPHERALS	255

Winter, 1996

Optisys

	GlobalNet

	GlobalNet™ storage servers provide Novell Network access to optical jukeboxes, including CD-ROM, Erasable and WORM (Write Once Read 
	Many) technologies.  Notable for its ease of installation, use and its speed.

Host Adapters Tested
AHA®-1540/2/F/P  
AHA®-2840/2VL  
AHA®-3940/W

Optisys
9250 North 43rd Avenue, Suite 12
Glendale, AZ 85302
Phone	(602) 997-9699
Fax	(602) 944-4051
Toll free	(800) 327-1271

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

PERIPHERALS	256

Winter, 1996

Pacific Micro Data, Inc.

	MAST VII

	MAST VII™ is an open architecture subsystem which supports non-proprietary SCSI-2 drives, host adapters, 4mm DAT drives, and RAID 
	technologies (software and hardware based).  The SCSI control panel provides complete system monitoring for easy system diagnostics.  
	“Hot Fix” drives, fans, and air filters provide easy maintenance.  
	  
	Features include:  
	– RAID 5 technology (hardware and software) which cost-effectively increases performance and fault tolerance  
	  
	–Hot Fix drive shuttles permit power-on placement  
	  
	–Intelligent SCSI backplane  
	  
	–Multiple SCSI bus channels for performance and configuration tuning

Host Adapters Tested
AHA®-1520/2  
AHA®-1540/2/F/P  
AHA®-1640  
AHA®-1740/2/4

Pacific Micro Data, Inc.
3002 Dow Avenue, #140
Tustin, CA 92680
US
Phone	(714) 838-8900
Fax	(714) 838-9787
Toll free	(800) 933-7575

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

PERIPHERALS	257

Winter, 1996

Ricoh Company, Ltd.

	IS50

	IS50® provides high-quality scanning at 256 levels of gray-scale and 400 dpi.  Its crisp, clear scanning capabilities to the very end 
	of the page make the Ricoh IS50 well-suited for desktop publishing and OCR applications.  And this advanced machine offers these 
	features as well:  full legal-size reading; enhanced image processing functions; a variety of brightness, contrast and gamma curves; 
	SCSI-2 interface; and an optional 30-sheet document feeder.

Host Adapters Tested
AHA®-1520/2  
AHA®-1540/2/F/P  
AHA®-1740/2/4  
AHA®-2740/2/4/T/W  
AHA®-2840/2VL  
AHA®-2940/4/W

Ricoh Company, Ltd.
1-3-6 Naka-Magome, Ohta-Ku
Tokyo,  143
Japan
Phone	(81) 3-3777-3479
Fax	(81) 3-3777-2878

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

PERIPHERALS	258

Winter, 1996

Ricoh Company, Ltd.

	IS60

	The IS60 provides high-quality scanning at 256 levels of gray-scale and 600dpi to accommodate the needs of the most demanding DTP users
	 including high-quality photograph scanning.  This advanced machine offers these features as well:  enhanced image processing 
	functions, a variety of brightness, contrast and gamma curves, SCSI-2 interface and an optional 30-sheet document feeder.

Host Adapters Tested
AHA®-1520/2  
AHA®-1540/2/F/P  
AHA®-1740/2/4  
AHA®-2740/2/4/T/W  
AHA®-2840/2VL  
AHA®-2940/4/W

Ricoh Company, Ltd.
1-3-6 Naka-Magome, Ohta-Ku
Tokyo,  143
Japan
Phone	(81) 3-3777-3479
Fax	(81) 3-3777-2878

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

PERIPHERALS	259

Winter, 1996

Ricoh Company, Ltd.

	IS410

	The IS410 is a powerful, versatile machine that can handle all office filing needs.  This advanced machine offers these features:  fast
	 processing of long documents, 400 dpi fine resolution scanning, designed for durability, document feeder automatically feeds up to 50 
	sheets and SCSI-2 interface and an optional endorser which is an accessory of the ADF, prints up to 16 alphanumeric characters on 
	scanned documents for improved record management and DCU board enables data compression in three CCITT format.

Host Adapters Tested
AHA®-1520/2  
AHA®-1540/2/F/P  
AHA®-1740/2/4  
AHA®-2740/2/4/T/W  
AHA®-2840/2VL  
AHA®-2940/4/W

Ricoh Company, Ltd.
1-3-6 Naka-Magome, Ohta-Ku
Tokyo,  143
Japan
Phone	(81) 3-3777-3479
Fax	(81) 3-3777-2878

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

PERIPHERALS	260

Winter, 1996

Ricoh Company, Ltd.

	IS420

	The IS420 provides high-resolution optics and image processing with 256 levels of gray-scale and 400 dpi.  Its various functions have 
	been incorporated to enhance versatility.  These include area extraction (permitting selection of a rectangular area on a page for 
	scanning), section area (allowing assignment of appropriate scanning processes to as many as six areas), and built-in image-processing 
	functions (eliminating noise and smoothing text to achieve a crisp, clear image).  
	  
	The Ricoh IS420 is well-suited for document imaging processing and OCR applications.  This advanced machine offers these features as 
	well:  flexible contrast, brightness and gamma curve adjustment, document feeder automatically feeds up to 100 sheets, SCSI-2 interface
	 and expansion slot for optional Image Processing Unit, Data Compression Unit and Video Interface Unit.

Host Adapters Tested
AHA®-1520/2  
AHA®-1540/2/F/P  
AHA®-1740/2/4  
AHA®-2740/2/4/T/W  
AHA®-2840/2VL  
AHA®-2940/4/W

Ricoh Company, Ltd.
1-3-6 Naka-Magome, Ohta-Ku
Tokyo,  143
Japan
Phone	(81) 3-3777-3479
Fax	(81) 3-3777-2878

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

PERIPHERALS	261

Winter, 1996

Ricoh Company, Ltd.

	FS2

	The FS2 provides clarity of 1200 dpi, enabling the FS2 to scan even small details without losing information. With a depth of 30 bits 
	per pixel, even the dark area can be scanned.  The FS2 was designed to meet the various demands from general scanning across 
	mass-scanning to professional color scanning.  
	  
	This advanced machine offers these features as well:  enhanced image processing functions, a variety of brightness, contrast and gamma 
	curves, SCSI-2 interface and an optional 30-sheet document feeder.

Host Adapters Tested
AHA®-1520/2  
AHA®-1540/2/F/P  
AHA®-1740/2/4  
AHA®-2740/2/4/T/W  
AHA®-2840/2VL  
AHA®-2940/4/W

Ricoh Company, Ltd.
1-3-6 Naka-Magome, Ohta-Ku
Tokyo,  143
Japan
Phone	(81) 3-3777-3479
Fax	(81) 3-3777-2878

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

PERIPHERALS	262

Winter, 1996

Ricoh Corporation

	Hyperspace

	Hyperspace® is one of the few 5.25" magneto-optical drives which has 3600 rpm.  In addition, this drive employs a dust-free design.  
	This means end-users do not need to periodically clean the optical heads.  A PC kit is also available. The product is ISO standard.  
	  
	Hyperspace® 1.3 GB is the next generation 5.25" magneto-optical disk drive offering 1.3 GB capacity. The Hyperspace 1.3 GB is fully 
	compatible with older 594/650 MB optical cartridges, and incorporates Ricoh’s advanced dust-free design. The Hyperspace 1.3 GB is 
	offered in both internal and external configurations, and is fully ISO standard.

Host Adapters Tested
AHA®-1510  
AHA®-1520/2  
AHA®-1540/2/F/P  
AHA®-1740/2/4

Ricoh Corporation
3001 Orchard Parkway
San Jose, CA 95134
USA
Phone	(408) 432-8800
Fax	(408) 943-9364
Toll free	(800) 955-3453

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

PERIPHERALS	263

Winter, 1996

Ricoh Corporation

	Transporter

	Transporter® is a 3.5" magneto-optical drive that supports the O-ROM function which utilizes CD-ROM technology, allowing mass data 
	distribution.  DOS and Novell kits are also available.  This product is ISO compatible.  
	  
	Transporter 2 is a 3.5" magneto-optical drive that offers 3000 rpm spindle speed coupled with Ricoh’s exclusive dust-proof design. The 
	Transporter 2 is available in internal and external configurations, and is fully ISO standard.

Host Adapters Tested
AHA®-1510  
AHA®-1520/2  
AHA®-1540/2/F/P  
AHA®-1740/2/4

Ricoh Corporation
3001 Orchard Parkway
San Jose, CA 95134
USA
Phone	(408) 432-8800
Fax	(408) 943-9364
Toll free	(800) 955-3453

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

PERIPHERALS	264

Winter, 1996

Ricoh Corporation

	HyperSpace Shuttle

	HyperSpace Shuttle® is a five-platter jukebox which comes with the HyperSpace drive inside. This product provides over 2 MB/second 
	sustained transfer rate.  It is ideal for large file archival and retrieval purposes.  The recording capacity is 3.25 GB.  DOS/Windows,
	 Sun Microsystems®, Novell and Macintosh kits are available.

Host Adapters Tested
AHA®-1510  
AHA®-1520/2  
AHA®-1540/2/F/P  
AHA®-1740/2/4

Ricoh Corporation
3001 Orchard Parkway
San Jose, CA 95134
USA
Phone	(408) 432-8800
Fax	(408) 943-9364
Toll free	(800) 955-3453

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

PERIPHERALS	265

Winter, 1996

SHAFFSTALL Corporation

	QT3490E

	The QT3490E provides high speed data interchange between PCs/Networks and Mainframes via 3490E 1/2" tape cartridges.  
	IBM/ANSI/EBCDIC/ASCII tapes can be accomodated on PCs, Windows NT, and Netware Servers.

Host Adapters Tested
AHA®-1510  
AHA®-1520/2  
AHA®-1540/2/F/P  
AHA®-1640  
AHA®-1740/2/4  
AHA®-2740/2/4/T/W  
AHA®-2940/4/W  
AHA®-3940/W

SHAFFSTALL Corporation
7901 East 88th Street
Indianapolis, IN 46256
Phone	(317) 842-2077
Fax	(317) 842-8294
Toll free	(800) 248-3475
E-mail	sales@shaffstall.com
URL	http://www.shaffstall.com

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

PERIPHERALS	266

Winter, 1996

SHAFFSTALL Corporation

	QuickTape MediaServer

	'Data Interchange and Duplication'  
	  
	MediaServer converts and copies magnetic tapes including labeled and unlabeled ASCII/EBCDIC/BINARY datasets.  System software includes 
	a number of translator programs or "filters" to assist the user in converting from many of the popular industry standard tape formats. 
	 These include UNIX "tar" and "cpio" archives from virtually any UNIX workstation or server; DEC VMS and PDP-11 backup tapes from VAX 
	systems; IBM System 36, and AS/400.  Tape drives included are SCSI 3490E, 9-track reel, DLT 2000/4000, 4MM DAT, 8MM, and QIC.

Host Adapters Tested
AHA®-1510  
AHA®-1520/2  
AHA®-1540/2/F/P  
AHA®-1640  
AHA®-1740/2/4  
AHA®-2740/2/4/T/W  
AHA®-2940/4/W  
AHA®-3940/W  
AHA®-3940U/UW

SHAFFSTALL Corporation
7901 East 88th Street
Indianapolis, IN 46256
Phone	(317) 842-2077
Fax	(317) 842-8294
Toll free	(800) 248-3475
E-mail	sales@shaffstall.com
URL	http://www.shaffstall.com

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

PERIPHERALS	267

Winter, 1996

Sony Electronics, Inc.

	CDU-55S

	Sony’s latest CDU-55S SCSI CD-ROM drive provides the best solution for computer applications requiring high performance at a low cost 
	of ownership.  The CDU-55S features a 256KB read ahead cache buffer, low average access time of 22ms and fast 2.4 times spin speed.  
	The CDU-55S is supported by the industry’s highest MTBF of 100,000 power on hours and is backed by Sony’s expertise of over fifteen 
	years in CD-ROM technology.  With its 4.0 MB per second burst transfer rate and SCSI-2 interface, the CDU-55S is ideal for today’s SCSI
	 applications.

Host Adapters Tested
AVA™-1515

Sony Electronics, Inc.
3300 Zanker Road
San Jose, CA 95134
USA
Phone	(408) 955-4173
Fax	(408) 955-5169
Toll free	(800) 352-7669

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

PERIPHERALS	268

Winter, 1996

Symbios Logic

	MetaStor

	MetaStor disk array products provide high performance RAID in addition to other features that contribute to continuous data 
	availability.

Host Adapters Tested
AHA®-2940/4/W

Symbios Logic
3718 N Rock Road
Wichita, KS 67226
USA
Phone	(316) 636-8000
Fax	(316) 636-8889
Toll free	(800) 440-5606

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

PERIPHERALS	269

Winter, 1996

Tandberg Data S.A.

	Tape Storage Solutions: Panther

	The Panther Family of tape backup systems offers a full range of backup solutions from 250 MB up to 13/26 GB.  The Panther Family 
	provides turnkey solutions for all major OS and network environments with industry leaders such as Adaptec®, Arcada, Cheyenne, JMR,  
	3M, and Sony.

Host Adapters Tested
APA™-348  
APA™-358  
APA™-1460  
AVA™-1505  
AHA®-1510  
AVA™-1515  
AHA®-1520/2  
AHA®-1530/2P  
AHA®-1540/2/F/P  
AHA®-1640  
AHA®-1740/2/4  
AHA®-2740/2/4/T/W  
AHA®-2840/2VL  
AHA®-2940/4/W

Tandberg Data S.A.
16-18 Avenue Morane Saulnier, Bat A
F-78941 Velizy,
France
Phone	33-1-39260101
Fax	33-1-34650289
URL	www.tandberg.com

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

PERIPHERALS	270

Winter, 1996

Tandberg Data S.A.

	Streaming Tape Drives

	Tandberg Data DC600 and mini cartridges QIC tape drives are the ultimate choice for hard disk backup, archival storage and data 
	interchange for PC, workstation and mid-range computer.

Host Adapters Tested
APA™-348  
APA™-358  
APA™-1460  
AVA™-1505  
AHA®-1510  
AVA™-1515  
AHA®-1520/2  
AHA®-1530/2P  
AHA®-1540/2/F/P  
AHA®-1640  
AHA®-1740/2/4  
AHA®-2740/2/4/T/W  
AHA®-2825VL  
AHA®-2840/2VL  
AHA®-2940/4/U/UW  
AHA®-3940/W  
AHA®-3980/5/W

Tandberg Data S.A.
16-18 Avenue Morane Saulnier, Bat A
F-78941 Velizy,
France
Phone	33-1-39260101
Fax	33-1-34650289
URL	www.tandberg.com

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

PERIPHERALS	271

Winter, 1996

Tandberg Data S.A.

	Panther 250 (TDC 3660)

	Tandberg data tape drives series offers one of the most affordable backup choices for Power PC and LAN users.  Low cost per megabyte 
	coupled with significant growth potential provide outstanding backup value.

Host Adapters Tested
APA™-348  
APA™-358  
APA™-1460  
AVA™-1505  
AHA®-1510  
AVA™-1515  
AHA®-1520/2  
AHA®-1530/2P  
AHA®-1540/2/F/P  
AHA®-1640  
AHA®-1740/2/4  
AHA®-2740/2/4/T/W  
AHA®-2825VL  
AHA®-2840/2VL  
AHA®-2940/4/W  
AHA®-2940W MAC  
AHA®-3940/W  
AHA®-3980/5/W

Tandberg Data S.A.
16-18 Avenue Morane Saulnier, Bat A
F-78941 Velizy,
France
Phone	33-1-39260101
Fax	33-1-34650289
URL	www.tandberg.com

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

PERIPHERALS	272

Winter, 1996

Tandberg Data S.A.

	Panther 525 (TDC 3820)

	Tandberg data tape drives series offers one of the most affordable backup choices for Power PC and LAN users.  Low cost per megabyte 
	coupled with significant growth potential provide outstanding backup value.

Host Adapters Tested
APA™-348  
APA™-358  
APA™-1460  
AVA™-1505  
AHA®-1510  
AVA™-1515  
AHA®-1520/2  
AHA®-1530/2P  
AHA®-1540/2/F/P  
AHA®-1640  
AHA®-1740/2/4  
AHA®-2740/2/4/T/W  
AHA®-2825VL  
AHA®-2840/2VL  
AHA®-2940/4/W  
AHA®-2940W MAC  
AHA®-3940/W  
AHA®-3980/5/W

Tandberg Data S.A.
16-18 Avenue Morane Saulnier, Bat A
F-78941 Velizy,
France
Phone	33-1-39260101
Fax	33-1-34650289
URL	www.tandberg.com

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

PERIPHERALS	273

Winter, 1996

Tandberg Data S.A.

	Panther 1200 (TDC 4120)

	Tandberg data tape drives series offers one of the most affordable backup choices for Power PC and LAN users.  Low cost per megabyte 
	coupled with significant growth potential provide outstanding backup value.

Host Adapters Tested
APA™-348  
APA™-358  
APA™-1460  
AVA™-1505  
AHA®-1510  
AVA™-1515  
AHA®-1520/2  
AHA®-1530/2P  
AHA®-1540/2/F/P  
AHA®-1640  
AHA®-1740/2/4  
AHA®-2740/2/4/T/W  
AHA®-2825VL  
AHA®-2840/2VL  
AHA®-2940/4/W  
AHA®-2940W MAC  
AHA®-3940/W  
AHA®-3980/5/W

Tandberg Data S.A.
16-18 Avenue Morane Saulnier, Bat A
F-78941 Velizy,
France
Phone	33-1-39260101
Fax	33-1-34650289
URL	www.tandberg.com

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

PERIPHERALS	274

Winter, 1996

Tandberg Data S.A.

	Panther 2500 (TDC 4220)

	Tandberg data tape drives series offers one of the most affordable backup choices for Power PC and LAN users.  Low cost per megabyte 
	coupled with significant growth potential provide outstanding backup value.

Host Adapters Tested
APA™-348  
APA™-358  
APA™-1460  
AVA™-1505  
AHA®-1510  
AVA™-1515  
AHA®-1520/2  
AHA®-1530/2P  
AHA®-1540/2/F/P  
AHA®-1640  
AHA®-1740/2/4  
AHA®-2740/2/4/T/W  
AHA®-2825VL  
AHA®-2840/2VL  
AHA®-2940/4/W  
AHA®-2940W MAC  
AHA®-3940/W  
AHA®-3980/5/W

Tandberg Data S.A.
16-18 Avenue Morane Saulnier, Bat A
F-78941 Velizy,
France
Phone	33-1-39260101
Fax	33-1-34650289
URL	www.tandberg.com

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

PERIPHERALS	275

Winter, 1996

Tandberg Data S.A.

	Panther 5000 (TDC 4222)

	Tandberg data tape drives series offers one of the most affordable backup choices for Power PC and LAN users.  Low cost per megabyte 
	coupled with significant growth potential provide outstanding backup value.

Host Adapters Tested
APA™-348  
APA™-358  
APA™-1460  
AVA™-1505  
AHA®-1510  
AVA™-1515  
AHA®-1520/2  
AHA®-1530/2P  
AHA®-1540/2/F/P  
AHA®-1640  
AHA®-1740/2/4  
AHA®-2740/2/4/T/W  
AHA®-2825VL  
AHA®-2840/2VL  
AHA®-2940/4/W  
AHA®-2940W MAC  
AHA®-3940/W  
AHA®-3980/5/W

Tandberg Data S.A.
16-18 Avenue Morane Saulnier, Bat A
F-78941 Velizy,
France
Phone	33-1-39260101
Fax	33-1-34650289
URL	www.tandberg.com

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

PERIPHERALS	276

Winter, 1996

Tandberg Data S.A.

	Panther Mini 2000 (TDC 3520)

	Tandberg data tape drives series offers one of the most affordable backup choices for Power PC and LAN users.  Low cost per megabyte 
	coupled with significant growth potential provide outstanding backup value.

Host Adapters Tested
APA™-348  
APA™-358  
APA™-1460  
AVA™-1505  
AHA®-1510  
AVA™-1515  
AHA®-1520/2  
AHA®-1530/2P  
AHA®-1540/2/F/P  
AHA®-1640  
AHA®-1740/2/4  
AHA®-2740/2/4/T/W  
AHA®-2825VL  
AHA®-2840/2VL  
AHA®-2940/4/W  
AHA®-2940W MAC  
AHA®-3940/W  
AHA®-3980/5/W

Tandberg Data S.A.
16-18 Avenue Morane Saulnier, Bat A
F-78941 Velizy,
France
Phone	33-1-39260101
Fax	33-1-34650289
URL	www.tandberg.com

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

PERIPHERALS	277

Winter, 1996

Tandberg Data S.A.

	Panther Mini 4600 (TDC 3720)

	Tandberg data tape drives series offers one of the most affordable backup choices for Power PC and LAN users.  Low cost per megabyte 
	coupled with significant growth potential provide outstanding backup value.

Host Adapters Tested
APA™-348  
APA™-358  
APA™-1460  
AVA™-1505  
AHA®-1510  
AVA™-1515  
AHA®-1520/2  
AHA®-1530/2P  
AHA®-1540/2/F/P  
AHA®-1640  
AHA®-1740/2/4  
AHA®-2740/2/4/T/W  
AHA®-2825VL  
AHA®-2840/2VL  
AHA®-2940/4/W  
AHA®-2940W MAC  
AHA®-3940/W  
AHA®-3980/5/W

Tandberg Data S.A.
16-18 Avenue Morane Saulnier, Bat A
F-78941 Velizy,
France
Phone	33-1-39260101
Fax	33-1-34650289
URL	www.tandberg.com

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

PERIPHERALS	278

Winter, 1996

Tandberg Data S.A.

	Tandberg MLR 1

	The Tandberg MLR series tape drive is the ultimate choice today and in the future for data storage, backup, archival storage and data 
	interchange on your workstation, network server or mid-range computer.

Host Adapters Tested
AVA™-1505  
AHA®-1510  
AVA™-1515  
AHA®-1520/2  
AHA®-1530/2P  
AHA®-1540/2/F/P  
AHA®-1640  
AHA®-1740/2/4  
AHA®-2740/2/4/T/W  
AHA®-2840/2VL  
AHA®-2910A/Ai  
AHA®-2940/4/W  
AHA®-2940/4/U/UW  
AHA®-3940/W  
AHA®-3940U/UW

Tandberg Data S.A.
16-18 Avenue Morane Saulnier, B at A
F-78941 Velizy,
France
Phone	33-1-34650289
Toll free	33-1-34650289
URL	www.tandberg.com

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

PERIPHERALS	279

Winter, 1996

UMAX Technologies, Inc.

	UC 1260

	The UC1260, with its 600 x 1200 hardware resolution, captures the sharpness and fine detail you need for image enlargement and lineart 
	work.  With the MagicScan driver, you'll get advanced features like color balancing, descreening, and batch scanning.

Host Adapters Tested
APA™-1460  
AVA™-1505  
AHA®-1510  
AVA™-1515  
AHA®-1520/2  
AHA®-1530/2P  
AHA®-1540/2/F/P  
AHA®-1640  
AHA®-1740/2/4  
AHA®-2740/2/4/T/W  
AHA®-2840/2VL  
AHA®-2940/4/W  
AHA®-3940/W

UMAX Technologies, Inc.
3353 Gateway Blvd.
Fremont, CA 94538
Phone	(510) 651-9488
Fax	(510) 651-8834
Toll free	(800) 562-0311

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

PERIPHERALS	280

Winter, 1996

UMAX Technologies, Inc.

	Gemini-D16

	The Gemini-D-16 is the world's first dual lens scanner.  The Gemini D-16 is capable of hardware resolution of 800 x 1600 dpi.  It comes
	 complete with MagicScan, the intelligent user-interface for scanning control.  Magic Scan features batch scanning, unsharp masking, 
	color balancing and descreening of printed material.

Host Adapters Tested
APA™-1460  
AVA™-1505  
AHA®-1510  
AVA™-1515  
AHA®-1520/2  
AHA®-1530/2P  
AHA®-1540/2/F/P  
AHA®-1640  
AHA®-1740/2/4  
AHA®-2740/2/4/T/W  
AHA®-2840/2VL  
AHA®-2940/4/W  
AHA®-3940/W

UMAX Technologies, Inc.
3353 Gateway Blvd.
Fremont, CA 94538
Phone	(510) 651-9488
Fax	(510) 651-8834
Toll free	(800) 562-0311

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

PERIPHERALS	281

Winter, 1996

UMAX Technologies, Inc.

	PowerLook

	The award-winning PowerLook combines blazing speed and superior image quality.  The PowerLook comes with UMAX's own MagicScan, 
	intuitive software that gives you scanning domination.  MagicScan features batch scanning unsharp masking, color balancing, and 
	descreening of printed material.  With a dynamic range of > 3.1, the UMAX PowerLook will serve all of your prepress needs.

Host Adapters Tested
APA™-1460  
AVA™-1505  
AHA®-1510  
AVA™-1515  
AHA®-1520/2  
AHA®-1530/2P  
AHA®-1540/2/F/P  
AHA®-1640  
AHA®-1740/2/4  
AHA®-2740/2/4/T/W  
AHA®-2840/2VL  
AHA®-2940/4/W  
AHA®-3940/W

UMAX Technologies, Inc.
3353 Gateway Blvd.
Fremont, CA 94538
Phone	(510) 651-9488
Fax	(510) 651-8834
Toll free	(800) 562-0311

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

PERIPHERALS	282

Winter, 1996

UMAX Technologies, Inc.

	Vista Series

	UMAX's new Vista-T630 is the "next generation" of the award winning UC630.  Micro-stepping motors and I/O buffers in the Vista-T630 
	provide scanning speeds that surpass all other three-pass scanners.    
	  
	UMAX designed the new Vista-S6 to give you the speed you need.    
	  
	With a hardware resolution of 400 x 800 dpi and a maximum resolution of 6400 dpi through interpolation, the Vista S-8 captures images 
	with more clarity and detail.    
	  
	The Vista-T630 and -S6 use a full spectrum cold-cathode lamp for long life and low maintenance.  
	  
	All of these scanners come complete with VistaScan.  With features like autodensity, descreen, and quality scan, it's no wonder 
	VistaScan is one of the most intuitive scanner interfaces available.

Host Adapters Tested
APA™-1460  
AVA™-1505  
AHA®-1510  
AVA™-1515  
AHA®-1520/2  
AHA®-1530/2P  
AHA®-1540/2/F/P  
AHA®-1640  
AHA®-1740/2/4  
AHA®-2740/2/4/T/W  
AHA®-2840/2VL  
AHA®-2940/4/W  
AHA®-3940/W

UMAX Technologies, Inc.
3353 Gateway Blvd.
Fremont, CA 94538
Phone	(510) 651-9488
Fax	(510) 651-8834
Toll free	(800) 562-0311

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

PERIPHERALS	283

Winter, 1996

Valitek, Inc.

	PST 2 Series Tape Backup

	Valitek manufactures portable tape backups that work through the parallel, serial or SCSI port and are designed to be shared among 
	multiple PCs, laptops, and file servers.  Valitek ships its tape backups with the Valitek Tape Backup Software—a DOS application that 
	drives the unit—either parallel or serial.  The drives can be used on the SCSI port via a third party tape backup software package 
	(Cheyenne, ARCSERVE, Central Point backup, Norton Backup for Windows, etc.)  The PST2 Series of tape drives is available in eight 
	models: the PST2 500, 1000, 2400, 5000, M2000, DAT2, DAT2+ and the DAT4+ with capacities ranging from 250MB to 4GB (uncompressed).

Host Adapters Tested
AHA®-1510  
AHA®-1540/2/F/P  
AHA®-1640  
AHA®-2840/2VL  
AHA®-2940/4/W  
AHA®-2940/4/U/UW

Valitek, Inc.
100 University Drive
Amherst, MA 01002
USA
Phone	(413) 549-2700
Fax	(413) 549-2900
E-mail	acer18@aol.com
URL	http://www.contagious.com/valitek/va

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

PERIPHERALS	284

Winter, 1996

XYXIS Corporation

	Erasable Optical Subsystems

	XYXIS™ provides erasable optical subsystems and associated drivers which support all Adaptec® SCSI host adapters with the ASPI software
	 managers.

Host Adapters Tested
APA™-348  
AVA™-1505  
AHA®-1510  
AVA™-1515  
AHA®-1520/2  
AHA®-1540/2/F/P  
AHA®-1640  
AHA®-1740/2/4  
AHA®-2740/2/4/T/W  
AHA®-2840/2VL  
AHA®-3940/W

XYXIS Corporation
2010 East Hennepin Avenue
Minneapolis, MN 55413
US
Phone	(612) 378-2577
Fax	(612) 378-2464

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

PERIPHERALS	285

Winter, 1996

Young Minds, Inc.

	SimpliCD

	SimpliCD, awarded PC Magazines Editors' Choice, May 17, 1994, is CD-Recordable software for the Windows user.  SimpliCD lets you record
	 data files and/or digital audio tracks.  SimpliCD works with a Windows-based file manager to "drag and drop" files from your hard disk
	 to a CD-Recordable disc.  Users can create ISO 9660-compliant, CD-ROM/XA, CD-DA, multisession, and mixed mode discs.  SimpliCD is 
	packed with new features, such as faster recording times and an integrated Backup & Restore utility, support for the Kodak Disc 
	Transporter and the PCD 600 (6x recorder).

Host Adapters Tested
AHA®-1540/2/F/P

Young Minds, Inc.
1906 Orange Tree Lane, Suite 240
Redlands, CA 92374
Phone	909-335-1350
Fax	909-798-0488
Toll free	800-964-4964
E-mail	marketing@ymi.com
URL	http://www.ymi.com

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

PERIPHERALS	286

Winter, 1996

Young Minds, Inc.

	MakeDisc - Unix CD-R

	MakeDisc premastering software for UNIX enables users to format data sets for ISO 9660/Rock Ridge compliant CD-ROM production.  
	MakeDisc provides transparent recovery of original UNIX file names, directories, and symbolic links.  The graphical user interface 
	makes it simple to professionally produce, format and test CD-ROM disc images before sending them to a writer or to a manufacturing 
	facility.  Because the software was written in C++, it can be ported in a matter of hours, and is now available on over 26 UNIX 
	platforms.

Host Adapters Tested
AHA®-1540/2/F/P

Young Minds, Inc.
1906 Orange Tree Lane, Suite 240
Redlands, CA 92374
Phone	909-335-1350
Fax	909-798-0488
Toll free	800-964-4964
E-mail	marketing@ymi.com
URL	http://www.ymi.com

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

PERIPHERALS	287

Winter, 1996

Young Minds, Inc.

	CD Studio - UNIX CD-R

	CD Studio is a complete UNIX-based solution for recording CD-ROM discs either at your desktop or across a network.  Integrating 
	MakeDisc premastering software, the CD Studio controller and a CD-Writer, CD Studio provides users with a valuable resource for 
	cost-effective data storage and distribution.  This completely reliable and networkable system supports the extended UNIX file 
	structure by creating ISO 9660/Rock Ridge discs.  CD Studio sets the standard for cross-platform portability, reliability, scalability,
	 and security.  Records multiple binaries, such as UNIX, Windows, and Macintosh, on a single disc.  Available on more than 26 different
	 UNIX platforms, OS/2 and DOS.  Creates CDs quickly, easily and efficiently.  CD studio was recently named 1995 Product of the Year by 
	Imaging Magazine.  In addition, the Digital Science Division of Eastman Kodak awarded CD Studio with an "Integration Excellence Award."

Host Adapters Tested
AHA®-1540/2/F/P

Young Minds, Inc.
1906 Orange Tree Lane, Suite 240
Redlands, CA 92374
Phone	909-335-1350
Fax	909-798-0488
Toll free	800-964-4964
E-mail	marketing@ymi.com
URL	http://www.ymi.com

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

OPERATING SYSTEMS	288

Winter, 1996

IBM Personal Software Products

	OS/2 Warp

	With OS/2 Warp you can dictate a memo and navigate the Internet by simply talking.  Use your voice to launch popular DOS, OS/2, Windows
	 3.1 and Java applications.  OS/2 Warp 4 provides a clear path to a connected world.  You can link to colleagues, customers and the 
	Internet.  Set up peer-to-peer networks and tap into a variety of servers from work, home or on the road.  This battle-tested operating
	 system provides improved security and tools to manage your network easily.  OS/2 Warps's wealth of connectivity function helps you 
	save time and money in setting up your network.

Host Adapters Tested
APA™-348  
APA™-358  
APA™-1460  
AVA™-1505  
AHA®-1510  
AVA™-1515  
AHA®-1520/2  
AHA®-1530/2P  
AHA®-1540/2/F/P  
AHA®-1640  
AHA®-1740/2/4  
AHA®-2740/2/4/T/W  
AHA®-2840/2VL  
AHA®-2910A/Ai  
AHA®-2940/4/W  
AHA®-2940/4/U/UW  
AHA®-3940/W  
AHA®-3940U/UW

IBM Personal Software Products
1140 Burnet Road
Austin, TX 78758
Phone	(512) 838-9926
Toll free	800-3IBM-OS2
URL	http://www.austin.ibm.com/pspinfo

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

OPERATING SYSTEMS	289

Winter, 1996

Lynx Real-Time Systems

	LynxOS

	The LynxOS is highly modular and scalable. At its fullest, it is a self-hosted development environment consisting of software 
	development tools, UNIX compatible utilities, industry standard networking, a graphical user interface, and a UNIX-like file system. At
	 its smallest, LynxOS can be configured with only the kernel, which can be linked with an application to form a ROMable image for 
	specialized embedded control applications.

Host Adapters Tested
APA™-1460  
AHA®-1520/2  
AHA®-1540/2/F/P  
AHA®-1740/2/4

Lynx Real-Time Systems
2239 Samaritan Drive
San Jose, CA 95124
Phone	(408) 879-3900
Fax	(408) 879-3945
E-mail	sales@lynx.com

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

OPERATING SYSTEMS	290

Winter, 1996

Microsoft Corporation

	DOS®, Windows®

	MS-DOS® is a single-user, single-tasking PC operating system.    
	  
	Windows® operating system is a robust desktop environment for business applications.  The ability to run more than one application at 
	one time with Windows® and transfer information between applications, the way Windows® uses the full power of a computer, and the rich 
	Windows® graphical interface provide a more intuitive, more efficient work environment for personal computers.

Host Adapters Tested
AHA®-1510  
AHA®-1520/2  
AHA®-1540/2/F/P  
AHA®-1640  
AHA®-1740/2/4  
AHA®-2740/2/4/T/W  
AHA®-2840/2VL

Microsoft Corporation
One Microsoft Way
Redmond, WA 98052-6399
Phone	(206) 882-8080
Fax	(206) 93MSFAX

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

OPERATING SYSTEMS	291

Winter, 1996

Microsoft Corporation

	Windows NT”

	Windows NT operating system is Microsoft’s platform for high-end computing needs for the 1990s.  It combines the ease-of-use and broad 
	application support of the Microsoft® Windows® operating system, and the advanced capabilities of a new, high-end operating system, 
	with support for MS-DOS, Windows®, and 32-bit Windows-based applications, as well as OS/2 character-based and POSIX-compliant 
	applications.

Host Adapters Tested
AHA®-1510  
AHA®-1520/2  
AHA®-1540/2/F/P  
AHA®-1640  
AHA®-1740/2/4  
AHA®-2740/2/4/T/W  
AHA®-2840/2VL  
AHA®-2940/4/W

Microsoft Corporation
One Microsoft Way
Redmond, WA 98052-6399
Phone	(206) 882-8080
Fax	(206) 93MSFAX

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

OPERATING SYSTEMS	292

Winter, 1996

Microsoft Corporation

	Windows® 95

	Windows 95 makes PCs even easier to use.    
	Windows 3.1 put a friendly interface on top of MS-DOS to make common PC tasks easier.  In Windows 95, the goal is to make those tasks 
	more intuitive, or where possible, automatic.  The addition and configuration of new hardware devices on the PC is one example.  
	Windows 95 plug and play automatically loads the appropriate drivers, sets IRQs, and notifies applications of the new capabilities of 
	the hardware device without any action by the user.  A redesigned user interface, highlighted by the Windows Taskbar, makes computing 
	more automatic for novices --usability tests show a ten-fold improvement over Windows 3.1 in time to complete certain common tasks such
	 as starting an application -- and makes the power of the PC more discoverable for intermediate and advanced users.  
	  
	Windows 95 is a faster and more powerful operating system.    
	Ease on the surface requires power and speed at the core, and the modern, 32-bit architecture of Windows 95 meets these requirements.  
	Freed from the limitations of MS-DOS, Windows 95 preemptively multitasks for better PC responsiveness -- so users will no longer have 
	to wait while the system copies files, for example -- and also delivers increased robustness and protection for applications.  Windows 
	95 also provides the foundation for a new generation of easier, more powerful multi-threaded 32-bit applications.  And most 
	importantly, Windows 95 delivers this power and robustness on today's average PC platform while scaling well to take advantage of 
	additional memory and CPU cycles.

Host Adapters Tested
APA™-1460  
AHA®-1510  
AHA®-1520/2  
AHA®-1530/2P  
AHA®-1540/2/F/P  
AHA®-1640  
AHA®-1740/2/4  
AHA®-2740/2/4/T/W  
AHA®-2840/2VL  
AHA®-2940/4/W  
AHA®-3940/W

Microsoft Corporation
One Microsoft Way
Redmond, WA 98052-6399
Phone	(206) 882-8080
Fax	(206) 93MSFAX

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

OPERATING SYSTEMS	293

Winter, 1996

NeXT Software, Inc.

	NEXTSTEP™

	NeXT is the only company to provide a completely integrated object-oriented client/server computing environment for enterprise-wide 
	software development and deployment.  Its environment, NEXTSTEP™, is the premier system for developing and deploying custom 
	client/server business applications and integrateing them with advanced productivity software throughout a heterogeneous network.  
	NEXTSTEP provides cross-platform integration, superior ease of use, and the robustness needed for handling mission-critical 
	applications globally.  
	  
	NEXTSTEP is based on the industry-standard Berkeley UNIX operating system and the Mach system kernel.  NEXTSTEP integrates seamlessly 
	with the most popular local and wide area networks including NFS and Novell and also accesses Macintosh and MS-DOS filesystems.  
	  
	NEXTSTEP also bundles powerful user and system management applications.  These include NeXTmail, a multimedia electronic mail system; 
	FaxReader for viewing faxes; Digital Librarian a powerful full-text searching tool; Edit, a multifont text editor; and NetInfo, a tool 
	for administering network resources.

Host Adapters Tested
APA™-1460  
AVA™-1505  
AHA®-1510  
AHA®-1520/2  
AHA®-1530/2P  
AHA®-1540/2/F/P  
AHA®-1740/2/4  
AHA®-2740/2/4/T/W  
AHA®-2840/2VL  
AHA®-2940/4/W  
AHA®-2940/4/U/UW

NeXT Software, Inc.
900 Chesapeake Drive
Redwood City, CA 94063
Phone	415-366-0900
Fax	800-228-NEXT
Toll free	800-TRY-NEXT
E-mail	trynext@next.com
URL	http://www.next.com

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

OPERATING SYSTEMS	294

Winter, 1996

Novell Unix Systems Group

	UnixWare

	UnixWare™ is an advanced general purpose UNIX operating system. It offers a multitasking, multiuser environment that is portable, 
	scalable, fully graphical and seamlessly integrated with Novell®s NetWare®.  
	  
	It is based on the mature, robust, and reliable UNIX SVR4.2 32-bit operating system and provides transparent access to NetWare’s 
	network services as well as support for TCP/IP protocols. Thousands of business-critical UNIX applications and many DOS and Windows 
	applications are supported in UnixWare.  
	  
	It operates on Intel 386, 486, and Pentium-based systems.

Host Adapters Tested
AHA®-1510  
AHA®-1520/2  
AHA®-1540/2/F/P  
AHA®-1640  
AHA®-1740/2/4  
AHA®-2740/2/4/T/W  
AHA®-2840/2VL  
AHA®-2940/4/W  
AHA®-3940/W

Novell Unix Systems Group
2180 Fortune Drive
San Jose, CA 95131
Phone	(408) 729-2300
Fax	(408) 729-2310

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

OPERATING SYSTEMS	295

Winter, 1996

Novell, Inc.

	NetWare

	Novell’s® NetWare® network computing products manage and control the sharing of services, data and applications among computer 
	workgroups, departmental networks and business-wide information systems. NetWare v4.1x provides interoperability, network services, 
	high performance, reliability and security in a network operating system. It utilizes a 32-bit, multitasking architecture and supports 
	DOS, Windows, Macintosh, OS/2 and UNIX workstations. In addition, NetWare v4.1x offers reliability features such as disk duplexing, 
	read-after-write verfication and disk mirroring.

Host Adapters Tested
AHA®-1540/2/F/P  
AHA®-1740/2/4  
AHA®-2840/2VL  
AHA®-2910A/Ai  
AHA®-2940/4/W  
AHA®-3940/W  
AHA®-3980/5/W

Novell, Inc.
122 East 1700 South
Provo, UT 84606
Phone	800-NETWARE
Fax	(801)861-2665
Toll free	800-NETWARE
E-mail	hbasup@novell.com
URL	www.novell.com

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

OPERATING SYSTEMS	296

Winter, 1996

Pebble Ridge Systems

	TXServer

	TxServer™ is a fully integrated client/server system specifically designed for high performance, high integrity transaction processing 
	applications on LAN connected PC's.  It is built around a multi-tasking server (mono or multiprocessor), providing database, 
	communications and transaction management, to tightly integrated Windows or DOS clients.  
	  
	The tight integration between the client-based development tools and the server's development and run time environment provides 
	end-to-end integrity and extremely high performance unmatched on comparable hardware.  
	  
	TxServer is a generic toolset sold to applications developers across many industry sectors.  It's ideal for supporting distributed 
	computing where businesses operate through multiple outlets that reconcile with a regional/central site.

Host Adapters Tested
AHA®-2940/4/W

Pebble Ridge Systems
19600 Fairchild #330
Irvine, CA 92715-2511
USA
Phone	(714) 752-7375
Fax	(714) 752-7377
E-mail	info@txs.com

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

OPERATING SYSTEMS	297

Winter, 1996

QNX Software Systems Ltd.

	QNX Realtime Operating System

	The QNX RTOS (version 4.23) is the leading realtime OS fro PCs.  A POSIX, microkernel-based, network-distributed OS, QNX can be easily 
	scaled from a deeply embedded system all the way up to a vast network running hundreds of CPUs.  QNX delivers realtime performance 
	through priority-driven pre-emptive scheduling, and responsive context-switch speeds (2.6 u sec microseconds per context switch on a 
	120 MHz Pentium).    
	  
	QNX's built-in networking provides transparent fault-tolerance, load-balancing, and handles multiple networks (e.g. Arcnet, Ethernet, 
	FDDI) simultaneously.  The development environment features Watcom's award-winning C/C++ compiler.  GUI options include the X Window 
	System and the award-winning Photon microGUI™, an embeddable window system that requires as little as 400K of ROM.  Photon applications
	 can be used in other GUI environments, including Windows 95, NT, OS/2, and X.  As a result, users can take advantage of the realtime 
	performance of QNX without having to leave their preferred desktop OS.

Host Adapters Tested
AVA™-1505  
AHA®-1510  
AVA™-1515  
AHA®-1520/2  
AHA®-1530/2P  
AHA®-1540/2/F/P  
AHA®-1640  
AHA®-1740/2/4  
AHA®-2740/2/4/T/W  
AHA®-2825VL  
AHA®-2840/2VL  
AHA®-2940/4/W  
AHA®-2940/4/U/UW  
AHA®-3940/W  
AHA®-3940U/UW  
AHA®-3980/5/W

QNX Software Systems Ltd.
175 Terence Matthews Crescent
Kanata, Ontario K2M 1W8
Canada
Phone	(613) 591-0931
Fax	(613) 591-3579
Toll free	(800) 676-0566
E-mail	info@qnx.com
URL	http://www.qnx.com

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

OPERATING SYSTEMS	298

Winter, 1996

S&H Computer Systems, Inc.

	TSX-32

	TSX-32™ offers the power of real-time, multi-user UNIX operating system with the ease-of-use of DOS. It excels as an application server
	 for DOS (16-bit & DPMI) and 32-bit applications, an NFS file server, a communication server and a printer server. TSX-32 supports up 
	to 256 users and 400 concurrent tasks on a single PC. Or, up to 40 times that number on a TCP/IP LAN or WAN. Add the BBS engine for 
	advanced remote access functionality. Add full Internet connectivity. See the TSX-BBS also listed in this guide.

Host Adapters Tested
AHA®-1540/2/F/P  
AHA®-1740/2/4  
AHA®-2740/2/4/T/W  
AHA®-2840/2VL  
AHA®-2940/4/W

S&H Computer Systems, Inc.
1027 17th Avenue South
Nashville, TN 37212
USA
Phone	(615) 327-3670
Fax	(615) 321-5929

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

OPERATING SYSTEMS	299

Winter, 1996

SunSoft, Inc.

	Solaris 2.5 for x86

	Solaris leads the UNIX operating system market, running on an installed base of more than 2 million systems.  It is the fastest, most 
	secure and reliable 32-bit operating system for SPARC, Intel, and Power PC server and desktop systems.  
	  
	Solaris provides a foundation for highly - integrated enterprise network environments, supporting multi-vendor interoperability and 
	resource sharing.  The operating system fits seamlessly into existing computing environments, providing the network management and 
	configuration tools for customers' growing computing needs.  
	  
	Solaris includes advanced technologies for multithreading, symmetric multiprocessing, integrated TCP/IP-based networking, and 
	centralized network administration tools.  And, recognizing the diversity of customer needs, Solaris comes in a series of 
	configurations.

Host Adapters Tested
AHA®-1510  
AHA®-1520/2  
AHA®-1530/2P  
AHA®-1540/2/F/P  
AHA®-1640  
AHA®-1740/2/4  
AHA®-2740/2/4/T/W  
AHA®-2840/2VL  
AHA®-2940/4/W  
AHA®-2940/4/U/UW

SunSoft, Inc.
2550 Garcia Avenue
Mountain View, CA 94043
USA
Phone	(415) 960-3200
Fax	(415) 336-0555
URL	http://www.sun.com

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

OPERATING SYSTEMS	300

Winter, 1996

SunSoft, Inc.

	Interactive UNIX 4.1

	The INTERACTIVE UNIX System V/386 Release 3.2, from SunSoft is a powreful and versatile 32-bit, multitasking, multiuser, operating 
	environment for Intel 80386, 80486 and Pentium-based platforms.  It delivers significant enhancements over the UNIX System V Release 
	3.2 operating system that enables you to exploit the full power of your 32-bit x86 platform.  And it complies with the major open 
	systems standards.  The INTERACTIVE UNIX System is the industry leader for reliability, robustness, and ease of use, and it is 
	available at an economical price.  Best of all, it is backed by SunSoft, the world's leading supplier of UNIX operating environments.

Host Adapters Tested
AHA®-1510  
AHA®-1520/2  
AHA®-1540/2/F/P  
AHA®-1740/2/4  
AHA®-2740/2/4/T/W  
AHA®-2840/2VL  
AHA®-2940/4/W

SunSoft, Inc.
2550 Garcia Avenue
Mountain View, CA 94043
USA
Phone	(415) 960-3200
Fax	(415) 336-0555
URL	http://www.sun.com

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

OPERATING SYSTEMS	301

Winter, 1996

The Santa Cruz Operation, Inc.

	SCO UNIX

	SCO® UNIX System V/386 Release 3.2 Operating System is the business choice for organizations requiring a proven open systems software 
	platform that runs on all standard 386/486 computers. The SCO UNIX System supports thousands of off-the-shelf applications, and is easy
	 to install, configure, use and administer. With its extensive communications capabilities and compliance with international and 
	government standards, the SCO UNIX System also supports interoperability with other systems. Its 32-bit, multithreaded, multitasking, 
	multiuser kernal with virtual memory delivers unprecedented performance on today’s advanced 386/486 systems.

Host Adapters Tested
AHA®-1510  
AHA®-1520/2  
AHA®-1540/2/F/P  
AHA®-1640  
AHA®-1740/2/4  
AHA®-2740/2/4/T/W

The Santa Cruz Operation, Inc.
400 Encinal Street, P.O. Box 1900
Santa Cruz, CA 95061
Phone	(408) 425-7222
Fax	(408) 427-5432
Toll free	(800) SCO-UNIX

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

OPERATING SYSTEMS	302

Winter, 1996

THEOS Software Corporation

	THEOS NetServer

	THEOS NetServer® is a network operating system that integrates THEOS-based applications seamlessly with Novell and Microsoft platforms,
	 including Windows for Workgroups 3.11, Windows 95 and Windows NT.  As a dedicated application server, NetServer can support a mixed 
	Client/Server environment of terminals and graphics workstations, offering centralized data security and fast file access.  
	  
	The THEOS operating system is primarily used in vertical markets such as Dental, Veterinarian, Alarm Systems and Point-of-Sale.

Host Adapters Tested
AHA®-1540/2/F/P

THEOS Software Corporation
1777 Botelho Drive, Suite 110
Walnut Creek, CA 94596
Phone	(510) 935-1118
Fax	(510) 935-1177
Toll free	800-600-5660
E-mail	info@theos-software.com
URL	http://www.theos-software.com

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

OPERATING SYSTEMS	303

Winter, 1996

THEOS Software Corporation

	THEOS 32

	THEOS 32® is a 32-bit multiuser, multi-threaded, preemptive multitasking operating system.  Optimized to run on 486 and Pentium based 
	systems, THEOS can support over 200 users.  Built-in features include:  Windowing capabilities, RS-232 Communications tools, Tape 
	Backup Utilities, SCSI support.  Additional products include 32-bit C and BASIC development languages.  
	  
	The THEOS operating system is primarily used in vertical markets such as Dental, Veterinarian,  Alarm Systems and Point-of-Sale.

Host Adapters Tested
AHA®-1540/2/F/P

THEOS Software Corporation
1777 Botelho Drive, Suite 110
Walnut Creek, CA 94596
Phone	(510) 935-1118
Fax	(510) 935-1177
Toll free	800-600-5660
E-mail	info@theos-software.com
URL	http://www.theos-software.com

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

SERVICES	304

Winter, 1996

Berg Software Design

	Device Driver & Software Design Services

	Berg Software Design is a consulting organization offering software design and implementation services.  Brian Berg, its principal, has
	 been a consultant since 1979.  He is familiar with SCSI and optical storage devices and standards.  Specialties include SCSI device 
	drivers for Windows/DOS, UNIX (particularly Silicon Graphics) and embedded operating systems.  Mr. Berg has been a project leader, 
	writer, industry analyst, conference speaker and session chair, patent reviewer, and expert witness.  He has worked with many SCSI 
	device types, both in initiator and target mode, and has extensive ASPI experience.

Host Adapters Tested
AHA®-1520/2  
AHA®-1540/2/F/P  
AHA®-2940/4/W  
AHA®-2940W MAC  
AHA®-2940/4/U/UW  
AHA®-3940/W  
AHA®-3940U/UW

Berg Software Design
14363 Saratoga Ave. Suite 200-B, P O Box 3488
Saratoga, CA 95070
USA
Phone	(408) 741-5010
Fax	(408) 741-5234
E-mail	BBERG@BSWD.COM

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

SERVICES	305

Winter, 1996

IPT Corporation

	Contract Product Development

	IPT Corporation is a Contract Product Development company specializing in the design, engineering, and manufacturing of electronic 
	products on a turnkey basis.  Since 1974, over 300 leading technology companies have turned to IPT to design and develop innovative new
	 technology products, such as embedded controllers and system software.    
	  
	Today, IPT’s product development services provide manufacturers the most viable alternative to building in-house engineering groups to 
	develop new high-tech products.  IPT’s staff of 45 full-time professionals is organized into fast-moving product development teams 
	specializing in interface electronics, SCSI device drivers and ASPI managers.  Other IPT teams provide comprehensive product 
	development services including the following:    
	–Electronic design  
	–Software engineering  
	–Mechanical engineering  
	–Industrial design  
	–Turnkey manufacturing  
	–Specification & documentation

Host Adapters Tested
AHA®-1540/2/F/P

IPT Corporation
1096 East Meadow Circle
Palo Alto, CA 94303
USA
Phone	(415) 494-7500
Fax	(415) 494-2758

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

SERVICES	306

Winter, 1996

Lookout Geophysical Company

	SeiScope/SeaScope

	Subsurface geo-technical images (Seismic, sonar, ground penetrating radar, etc.) are processed and displayed in real time and written 
	to SCSI tape drives (4mm, 8mm, DLT, 3480) and processed from tape after acquisition.

Host Adapters Tested
AHA®-1520/2  
AHA®-1540/2/F/P  
AHA®-2940/4/W  
AHA®-2940/4/U/UW

Lookout Geophysical Company
433 Park Point Drive, Suite 250
Golden, CO 80401
USA
Phone	303-526-5108
Fax	303-526-5150
E-mail	vgoebel@aol.com

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

SERVICES	307

Winter, 1996

Media Integration, Inc.

	Storage Integration Services

	Media Integration is a mass storage integrator specializing in digital video and fault tolerant subsystems for Novell, UNIX and OS/2 
	using ISA, EISA and Micro Channel Architecture buses.  Any combination of hard disk, tape drives, autochangers, optical disks and 
	jukeboxes are combined in external subsystems configured with all cabling and software.

Host Adapters Tested
AHA®-1510  
AHA®-1520/2  
AHA®-1540/2/F/P  
AHA®-1640  
AHA®-1740/2/4

Media Integration, Inc.
3949 Research Park Court, Suite 190
Soquel, CA 95073
USA
Phone	(408) 475-9400
Fax	(408) 475-0110
Toll free	(800) 824-7385

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

SERVICES	308

Winter, 1996

NovaStor Corporation

	Data Conversion Utilities

	DCU for DOS and OS/2 is NovaStor's Data Conversion Utility that offers users a SQL (Structured Query Language) conversion application. 
	 DCU is media independent allowing for transfers between tape, disk, and optical drives.  It allows users to query the data and extract
	 only the information that is vital to their application.  DCU provides powerful field-level conversions for numeric formats including 
	COM3, BCD, Zoned Decimal, 2 and 4 byte integer and many more.  Users can perform IF-THEN conditional tests bfore reading or processing 
	data.  DCU offers support for fixed and variable length records, IBM and ANSI labeled tapes and field-level manipulations.

Host Adapters Tested
APA™-348  
AVA™-1505  
AHA®-1510  
AVA™-1515  
AHA®-1520/2  
AHA®-1530/2P  
AHA®-1540/2/F/P  
AHA®-1640  
AHA®-1740/2/4  
AHA®-2740/2/4/T/W  
AHA®-2840/2VL  
AHA®-2940/4/W

NovaStor Corporation
80-B West Cochran Street
Simi Valley, CA 93065
Phone	(805) 579-6700
Fax	(805) 579-6710

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

SERVICES	309

Winter, 1996

NovaStor Corporation

	Tape Processing Utilities

	TPU for DOS and OS/2 offers users the ability to read and write any data stored on tape or disk.  TPU writes IBM, ANSI or ISO labeled 
	tape formats.  It is a flexible utility that allows you to convert between ASCII (American Standard Code for Information Interchange) 
	and EBCDIC (Extended Binary Coded Decimal Interchange Code) character sets, insert delimiters between records, examine tape formats, 
	and convert between media formats (1/4", 4mm, 8mm, 9-track, and 3480/90).

Host Adapters Tested
APA™-348  
AVA™-1505  
AHA®-1510  
AVA™-1515  
AHA®-1520/2  
AHA®-1530/2P  
AHA®-1540/2/F/P  
AHA®-1640  
AHA®-1740/2/4  
AHA®-2740/2/4/T/W  
AHA®-2840/2VL  
AHA®-2940/4/W

NovaStor Corporation
80-B West Cochran Street
Simi Valley, CA 93065
Phone	(805) 579-6700
Fax	(805) 579-6710

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

SERVICES	310

Winter, 1996

NovaStor Corporation

	NovaTar

	NovaTar offers users the ability to read UNIX standard TAR format tapes.  NovaTar easily converts UNIX name spaces to DOS-OS/2 and 
	translates CRLF to FL and FL to CRLF on the fly.  NovaTar allows for multiple volumes on a single tape.  NovaTar also allows users to 
	easily convert path names when reading/writing TAR tapes.

Host Adapters Tested
APA™-348  
AVA™-1505  
AHA®-1510  
AVA™-1515  
AHA®-1520/2  
AHA®-1530/2P  
AHA®-1540/2/F/P  
AHA®-1640  
AHA®-1740/2/4  
AHA®-2740/2/4/T/W  
AHA®-2840/2VL  
AHA®-2940/4/W

NovaStor Corporation
80-B West Cochran Street
Simi Valley, CA 93065
Phone	(805) 579-6700
Fax	(805) 579-6710

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

SERVICES	311

Winter, 1996

NovaStor Corporation

	NovaCPIO for DOS

	NovaCPIO offers users the ability to read UNIX standard CPIO format tapes.  NovaCPIO easily converts UNIX name spaces to DOS and 
	translates CRLF to LF and LF to CRLF on the fly.  NovaCPIO allows for multiple volumes on a single tape.  NovaCPIO also allows users to
	 easily convert path names when reading/writing CPIO tapes.

Host Adapters Tested
APA™-348  
AVA™-1505  
AHA®-1510  
AVA™-1515  
AHA®-1520/2  
AHA®-1530/2P  
AHA®-1540/2/F/P  
AHA®-1640  
AHA®-1740/2/4  
AHA®-2740/2/4/T/W  
AHA®-2840/2VL  
AHA®-2940/4/W

NovaStor Corporation
80-B West Cochran Street
Simi Valley, CA 93065
Phone	(805) 579-6700
Fax	(805) 579-6710

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

SERVICES	312

Winter, 1996

NovaStor Corporation

	QuTape

	QuTape is a utility program for use with a streaming tape drive incorporating a SCSI Controller,  It implements standard features for 
	tape positioning, and reading or writing any number of blocks at a time to or from the tape.  File formatting on input and output to 
	the tape is provided as well.  Raw tape data may be displayed on the screen ("dumped") without reading it into a disk file.

Host Adapters Tested
APA™-348  
AVA™-1505  
AHA®-1510  
AVA™-1515  
AHA®-1520/2  
AHA®-1530/2P  
AHA®-1540/2/F/P  
AHA®-1640  
AHA®-1740/2/4  
AHA®-2740/2/4/T/W  
AHA®-2840/2VL  
AHA®-2940/4/W

NovaStor Corporation
80-B West Cochran Street
Simi Valley, CA 93065
Phone	(805) 579-6700
Fax	(805) 579-6710

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

SERVICES	313

Winter, 1996

NovaStor Corporation

	QuTar

	QuTar allows users to read/write UNIX standard TAR format tapes.  It allows for easy data interchange between any Macintosh and any 
	Unix based system.  QuTar easily converts UNIX name spaces to Macintosh name spaces and translates CRLF to LF and LF to CRLF on the 
	fly.  QuTar allows for multiple volumes on a single tape.  QuTar also allows users to easily convert path names when reading/writing 
	TAR tapes.

Host Adapters Tested
APA™-348  
AVA™-1505  
AHA®-1510  
AVA™-1515  
AHA®-1520/2  
AHA®-1530/2P  
AHA®-1540/2/F/P  
AHA®-1640  
AHA®-1740/2/4  
AHA®-2740/2/4/T/W  
AHA®-2840/2VL  
AHA®-2940/4/W

NovaStor Corporation
80-B West Cochran Street
Simi Valley, CA 93065
Phone	(805) 579-6700
Fax	(805) 579-6710

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

SERVICES	314

Winter, 1996

SHAFFSTALL Corporation

	Conversion Services

	SHAFFSTALL Conversion Services offer tape-to-tape, disk-to-tape, tape-to-diskette and diskette conversion and transfer services.  We 
	also provide tape duplication services for software developers and other businesses needing multiple copies of their tape(s).

Host Adapters Tested
AHA®-1540/2/F/P  
AHA®-1740/2/4  
AHA®-2940/4/W  
AHA®-3940/W

SHAFFSTALL Corporation
7901 East 88th Street
Indianapolis, IN 46256
Phone	(317) 842-2077
Fax	(317) 842-8294
Toll free	(800) 248-3475
E-mail	sales@shaffstall.com
URL	http://www.shaffstall.com

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

SERVICES	315

Winter, 1996

Technical Integration Services

	Systems Engineering Consulting

	Technical Integration Services specializes in Systems Engineering Consulting for PC and LAN systems using Novell and Windows NT servers
	 with Windows, Windows for Workgroups and Windows NT clients.

Host Adapters Tested
APA™-1460  
AHA®-1540/2/F/P  
AHA®-1740/2/4  
AHA®-2740/2/4/T/W  
AHA®-2840/2VL  
AHA®-2940/4/W

Technical Integration Services
PO Box 370
Twinsburg, OH 44807
Phone	(216) 364-3655
Fax	(216) 364-3655

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

MISCELLANEOUS	316

Winter, 1996

Adaptec, Inc.

	Easy-CD Toolkit

	Easy CD Toolkit™ enables C or Visual Basic Programmers to integrate CD-R recording capability into their own applicaions.

Host Adapters Tested
AHA®-1510  
AHA®-1520/2  
AHA®-1530/2P  
AHA®-1540/2/F/P  
AHA®-2740/2/4/T/W  
AHA®-2840/2VL  
AHA®-2940/4/W  
AHA®-2940AU

Adaptec, Inc.
691 S Milpitas Blvd
Milpitas, CA
USA
Phone	1-800-934-2766
Fax	408-262-2533
Toll free	1-800-934-2766
E-mail	sales@adaptec.com
URL	http://www.adaptec.com

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

MISCELLANEOUS	317

Winter, 1996

Cactus International, Inc.

	LONE-OPTIMIZER

	LONE-OPTIMIZER is a UNIX and Xenix disk optimizer that increases the speed of your system by 20% to 75%. It is fully menu driven for 
	the UNIX impaired making it extremely easy-to-use. The LONE-OPTIMIZER offers a practice mode to let you see exactly what happens before
	 an actual optimization begins. With LONE-OPTIMIZER you can change the high-level interleave on the fly. This feature alone can double 
	system performance. It consolidates all directory information and keeps it next to the inode table for maximum file lookup performance.

Host Adapters Tested
AHA®-1510  
AHA®-1520/2  
AHA®-1540/2/F/P  
AHA®-1640  
AHA®-1740/2/4  
AHA®-2740/2/4/T/W

Cactus International, Inc.
13987 West Annapolis Court
Mt. Airy, MD 21771
USA
Phone	(301) 829-1622
Fax	(301) 829-1623
Toll free	(800) 525-UNIX
E-mail	cowboy@cactus.com

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

MISCELLANEOUS	318

Winter, 1996

Cirrus Technology, Inc.

	Unite CD-Maker

	Unite® CD-Maker is a 32-bit software package for creating custom CDs.  Unite CD-Maker allows users to quickly and easily make audio CDs
	 as well as create CD-ROMs for backup, archiving and distribution of data.  Included with Unite CD-Maker is a 32-Bit API set for 
	automating the recording process.  Advanced features include multisession support, enhanced CD and mixed mode support and a visual 
	buffer meter to monitor the burn. Many recorders are supported and Windows 95, Windows NT and OS/2 are supported.

Host Adapters Tested
AVA™-1505  
AHA®-1510  
AVA™-1515  
AHA®-1520/2  
AHA®-1530/2P  
AHA®-1540/2/F/P  
AHA®-1640  
AHA®-1740/2/4  
AHA®-2740/2/4/T/W  
AHA®-2825VL  
AHA®-2840/2VL  
AHA®-2910A/Ai  
AHA®-2940/4/W  
AHA®-3940/W  
AHA®-3980/5/W

Cirrus Technology, Inc.
5301 Buckeystown Pike, 4th floor
Frederick, MD 21704
US
Phone	(301)698-1900
Fax	(301)698-1909
E-mail	sales@cirunite.com
URL	http://www.cirunite.com

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

MISCELLANEOUS	319

Winter, 1996

Cornerstone Imaging, Inc.   Storage Division

	Storage Accel

	The Optical File System software (OFS) provides transparent access for users and developer level access to the optical drives and 
	jukeboxes. With the OFS, users manage optical media contained in the jukebox.  The software is compatible with Microsoft NT v3.51 or 
	4.0, IBM OS/2 WARP, Windows, DOS, Novell, Lantastic, Banyan Vines and LANserver.  It can be used in workstation or server environments.
	 When using the OFS for NT, users also have access to information stored in the jkukebox via Novell, Unix, or Apple systems.  
	  
	Key Features include:  
	* Full 32-bit multi-tasking and queue management.  
	* NT's built-in security features.  
	* Management of on-line and off-line volumes.  
	* Easy to use 5-minute installation.  
	  
	The OFS makes it easy to access the optical library  because the system administrator assigns a single drive letter to the optical 
	hardware.

Host Adapters Tested
AHA®-1540/2/F/P  
AHA®-1640  
AHA®-2740/2/4/T/W  
AHA®-2840/2VL  
AHA®-2940/4/W  
AHA®-2940AU

Cornerstone Imaging, Inc.   Storage Division
1600 South Main Street
Walnut Creek, CA 94596
Phone	(510) 938-5340
Fax	(510) 938-5341

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

MISCELLANEOUS	320

Winter, 1996

Dassault Electronique

	Ruggedized Computer Systems

	Dassault Electronique’s Ruggedized Computer Systems are a powerful combination of civil standards and military specifications.  The 
	Ruggedized Computer Systems satisfy today’s computer systems users and offer easy upgrade and low life cycle cost.  
	  
	The Dassault Electronique ruggedized computers are used in military programs and also in industrial applications where environmental 
	conditions demand it.  
	  
	Military applications include:  
	–Nuclear-missile and attack submarines, patrol boats, and surface ships  
	–On-board electronic-mail systems  
	–Test systems in helicopters  
	–Message or radio terminals in vehicles  
	–On-board acquisition systems in military vehicles  
	  
	Industrial applications include:  
	–On-board acquisition systems in test vehicles or prototypes  
	–Power stations, control or machine tools  
	–Measurements and calibration systems in nuclear power stations  
	–Acquisition control station for on-board measurement on planes  
	–Data transmission systems on networks or over radio links

Host Adapters Tested
APA™-348  
APA™-358  
APA™-1460  
AHA®-1540/2/F/P  
AHA®-1640  
AHA®-1740/2/4  
AHA®-2940/4/W

Dassault Electronique
55 Quai Marcel Dassault
Saint Cloud 92214,
France
Phone	331-34-81-47-39
Fax	331-49-11-83-90

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

MISCELLANEOUS	321

Winter, 1996

Delphi Data

	TestBox

	The TestBox™ series of testers provides a simple, low cost solution for most test environments. Adaptec controllers are combined with 
	hardware and software to provide a flexible tool for in-coming inspection, reliability, error injectors, fault-analysis, SCSI protocol 
	conformance and benchmark testing of high performance devices.

Host Adapters Tested
AHA®-1510  
AHA®-1520/2  
AHA®-1740/2/4

Delphi Data
9069 Cajalco Road
Corona, CA 91719
Phone	(909) 279-7955
Fax	(909) 279-7957
Toll free	(800) -DELPHI5
E-mail	76470.1544@compuserve.com

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

MISCELLANEOUS	322

Winter, 1996

DiagSoft, Inc.

	QAPlus/FE, QAPlus/Factory

	The QAPlus family of products provide direct SCSI and ASPI compliant disk, tape and CD-ROM diagnostics and product identification 
	reports for manufacturing, compatibility and support interests.

Host Adapters Tested
AHA®-1510  
AHA®-1520/2  
AHA®-1540/2/F/P  
AHA®-1640  
AHA®-1740/2/4  
AHA®-2740/2/4/T/W  
AHA®-2840/2VL  
AHA®-2940/4/W

DiagSoft, Inc.
5615 Scotts Valley Drive, Suite 140
Scotts Valley, CA 95066
Phone	(408) 438-8247
Fax	(408) 438-7113
Toll free	1-800-342-4763
E-mail	sales@diagsoft.com

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

MISCELLANEOUS	323

Winter, 1996

Digital Instrumentation Technology

	TransferPro

	TransferPro™ allows you to read and write Macintosh files directly from your PC.  TransferPro is a fast and easy file transfer 
	solution.  TransferPro reads, writes and formats Macintosh media including SyQuest™ , Bernoulli ™, Iomega™  Zip, data shuttle drives, 
	Pinnacle Micro™, Sony™,  MOST™, Ricoh™  and other magneto-optical drives, SCSI hard drives and CD-ROM drives.  TransferPro features 
	graphics viewers and converters and a high quality, easy to use Windows-based installer with an automatic configuration feature.  
	TransferPro is available for Windows, Windows 95 and Windows NT.

Host Adapters Tested
APA™-1460  
AVA™-1505  
AHA®-1510  
AVA™-1515  
AHA®-1520/2  
AHA®-1530/2P  
AHA®-1540/2/F/P  
AHA®-1640  
AHA®-1740/2/4  
AHA®-2740/2/4/T/W  
AHA®-2840/2VL  
AHA®-2940/4/W  
AHA®-3940/W

Digital Instrumentation Technology
127 Eastgate Dr. #20500
Los Alamos, NM 87544
Phone	(505) 662-1459
Fax	(505) 662-0897
Toll free	(800) 467-1459
E-mail	tpro-request@dit.com
URL	hhttp://www.dit.com

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

MISCELLANEOUS	324

Winter, 1996

Everex Systems, Inc.

	Explora

	The Everex Explora Integrated all-in-one computer makes compromise a thing of the past in a one piece unit.  The Explora supports 
	Pentium® processors and features a built-in, 15", 0.28 dot pitch non-interlaced monitor.  With up to 128 MB RAM and five expansion 
	slots (up to two PCI), the Explora provides true upgradability while offering the space and installation advantages of a one-piece 
	system.  With built-in stereo sound and speakers the Explora comes multimedia ready.  An optional base pedestal provides more powerful 
	speakers and 3D surround sound.

Host Adapters Tested
AHA®-1530/2P  
AHA®-1540/2/F/P  
AHA®-2940/4/W

Everex Systems, Inc.
5020 Brandin Court
Fremont, CA 94538
USA
Phone	1-800-EVEREX1
Fax	510-683-2186
Toll free	1-800-EVEREX1
E-mail	sales@everex.com
URL	http://www.everex.com

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

MISCELLANEOUS	325

Winter, 1996

Everex Systems, Inc.

	Tempo PCI 486

	Advanced PCI Local Bus graphics and disk control, plus 100 or 120 MHz  Am486DX4 or 133 MHz  AmX5 processors, make the Tempo PCI 486 
	systems the fastest 486s on the market.  Available as a desktop or midtower.  Designed for Windows 95 certification ensures flawless 
	performance in the 32-bit environment.  The Tempo PCI 486 offers the most performance for the dollar in the business market today.

Host Adapters Tested
AHA®-1540/2/F/P  
AHA®-2940/4/W

Everex Systems, Inc.
5020 Brandin Court
Fremont, CA 94538
USA
Phone	1-800-EVEREX1
Fax	510-683-2186
Toll free	1-800-EVEREX1
E-mail	sales@everex.com
URL	http://www.everex.com

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

MISCELLANEOUS	326

Winter, 1996

Everex Systems, Inc.

	TempoStation

	The TempoStation is ideal for users looking for powerful, reliable and economical solutions, offering high power and extreme 
	reliability in a slim desktop case.  This Windows 95 compatible system is the ideal personal workstation or LAN station.  It supports 
	486DX2 processors, and features integrated video, disk control and I/O functions.  This no-nonsense business computer is the perfect 
	workstation for any office.

Host Adapters Tested
AHA®-1530/2P  
AHA®-1540/2/F/P  
AHA®-2840/2VL

Everex Systems, Inc.
5020 Brandin Court
Fremont, CA 94538
USA
Phone	1-800-EVEREX1
Fax	510-683-2186
Toll free	1-800-EVEREX1
E-mail	sales@everex.com
URL	http://www.everex.com

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

MISCELLANEOUS	327

Winter, 1996

Everex Systems, Inc.

	Tempo VLG Desktop

	The Tempo VLG Desktop is a high performance VESA Local Bus system for graphics, multimedia, CAD, DTP and other demanding, high-end 
	applications.  Also available as a mid tower, the system supports all 486-class processors up to the 5x86-133, up to 128MB RAM and up 
	to 1MB cache, providing more than enough horsepower for business multimedia.

Host Adapters Tested
AHA®-1520/2  
AHA®-1540/2/F/P

Everex Systems, Inc.
5020 Brandin Court
Fremont, CA 94538
USA
Phone	1-800-EVEREX1
Fax	510-683-2186
Toll free	1-800-EVEREX1
E-mail	sales@everex.com
URL	http://www.everex.com

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

MISCELLANEOUS	328

Winter, 1996

Everex Systems, Inc.

	Step DP

	The Everex STEP DP is an EISA/PCI dual-Pentium® Symmetrical Multi Processing (SMP) solution, built with the quality and reliability 
	only Everex can provide.  The STEP DP adds PCI to EISA, supports Windows-NT, Solaris, OS/2 SMP or SCO MPX solution and is an ideal 
	graphical workstation, CAD drafting station or as a departmental server.  The system is also available as a single processor system, 
	letting you upgrade to SMP when ready.

Host Adapters Tested
AHA®-1540/2/F/P  
AHA®-1740/2/4  
AHA®-2740/2/4/T/W  
AHA®-2940/4/W

Everex Systems, Inc.
5020 Brandin Court
Fremont, CA 94538
USA
Phone	1-800-EVEREX1
Fax	510-683-2186
Toll free	1-800-EVEREX1
E-mail	sales@everex.com
URL	http://www.everex.com

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

MISCELLANEOUS	329

Winter, 1996

Everex Systems, Inc.

	STEP SP

	The Everex STEP SP provides entry-level and mid-range Pentium® processor solutions, built with the quality and reliability only Everex 
	can provide.  The "Designed for Windows 95" STEP SP offers exceptional price-performance at the entry-level.  Supporting up to 133 Mhz 
	processors, the STEP SP comes with up to 128MB RAM and 1MB cache for exceptional performance.  The system comes with a three year 
	limited warranty.

Host Adapters Tested
AHA®-2940/4/W

Everex Systems, Inc.
5020 Brandin Court
Fremont, CA 94538
USA
Phone	1-800-EVEREX1
Fax	510-683-2186
Toll free	1-800-EVEREX1
E-mail	sales@everex.com
URL	http://www.everex.com

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

MISCELLANEOUS	330

Winter, 1996

Everex Systems, Inc.

	STEP Pro

	The STEP Pro is a high-end Pentium® processor solution.  The "Designed for Windows 95" system features the high-performance Triton chip
	 set and delivers support for 133 MHz processors and beyond, plus EDO DRAM and pipeline burst SRAM for exceptional performance.  With 
	up to 128MB RAM and up to seven drive bays in a full tower configuration, the STEP Pro is ideal for use as a high-end system or server.
	  The system comes with a three year limited warranty.

Host Adapters Tested
AHA®-1530/2P  
AHA®-1540/2/F/P  
AHA®-2940/4/W

Everex Systems, Inc.
5020 Brandin Court
Fremont, CA 94538
USA
Phone	1-800-EVEREX1
Fax	510-683-2186
Toll free	1-800-EVEREX1
E-mail	sales@everex.com
URL	http://www.everex.com

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

MISCELLANEOUS	331

Winter, 1996

Fischer International Systems Corporation

	SafeBoot

	SafeBoot™ provides two factor access control, complete disk encryption and virus protection.  SafeBoot consists of SmartDisk, which 
	resembles a 3.5" floppy disk, but it’s actually a hardware device with its own microprocessor, firmware, memory and operating system 
	that fits into a normal floppy disk drive.  SafeBoot is initialized after entering a password at which time an encryption key is then 
	generated.  The key is used with the encryption algorithm to encrypt the hard drive. The password, key and encryption algorithm remain 
	resident on the SmartDisk.  The user will not be allowed access to the PC until the SmartDisk is inserted and correct password entered.

Host Adapters Tested
AHA®-1510  
AHA®-1520/2  
AHA®-1540/2/F/P  
AHA®-1740/2/4  
AHA®-2940/4/U/UW  
AHA®-3940/W  
AHA®-3940U/UW

Fischer International Systems Corporation
4073 Mercantile Avenue
Naples, FL 33942
Phone	800-237-4510
Fax	941-643-6357
Toll free	800-237-4510
URL	http:www.fisc.com

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

MISCELLANEOUS	332

Winter, 1996

GEVA Datentechnik GmbH

	X/EASY

	GEVA designs and develops innovative solutions for electronic data exchange and produces highgrade computer systems according to 
	individual requirements.    
	Keypoints of GEVA products include:  
	*Applications for electronic funds transfer for credit institutions of all sizes,  
	*Data carrier exchange for all lines of business, e.g. public administration, industry and the graphics trade,  
	*The configuration of bespoke, modular computer systems.

Host Adapters Tested
AHA®-1540/2/F/P  
AHA®-1640  
AHA®-1740/2/4  
AHA®-2740/2/4/T/W  
AHA®-2840/2VL  
AHA®-2940/4/W

GEVA Datentechnik GmbH
6 Joseph-von-Fraunhofer-Str. 3a
52477 Alsdorf,
Germany
Phone	49-2404 5500-0
Fax	49-2404 5500-99

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

MISCELLANEOUS	333

Winter, 1996

Matrox Electronic Systems Ltd.

	Matrox DigiSuite

	The Matrox DigiSuite™ are hardware and software tools that let developers design professional applications that require the storage and
	 retrieval of digital video and audio.  All hardware is PCI/ISA and supports plug and play.  Boards are available for Video I/O, 
	Graphic overlay, keying, mixing, 2D DVE and 3D DVE.  All software tools are 32-bit and object oriented.  Matrox supplies all the tools 
	required to build professional audio/video production equipment.

Host Adapters Tested
AHA®-2740/2/4/T/W  
AHA®-2940/4/W  
AHA®-2940/4/U/UW  
AHA®-3940/W  
AHA®-3940U/UW

Matrox Electronic Systems Ltd.
1055 St. Regis Boulevard, Dorval
Quebec, Quebec H9P 2T4
Canada
Phone	800-361-4903
Fax	(514) 685-2853
Toll free	800-361-4903
E-mail	video.info@matrox.com
URL	http://www.matrox.com/video

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

MISCELLANEOUS	334

Winter, 1996

Rancho Technology, Inc.

	RTSDA-USW Wide Fast20 (Ultra SCSI) Converter

	The RTSDA-USW 16-Bit Wide Fast20  (UltraSCSI) Converter connects a single-ended SCSI device to a differential-ended SCSI device.  Two 
	RTSDA-USW converters can be used to extend the SCSI cable length up to 200 feet.  Convert to differential-ended SCSI for better noise 
	immunity.  The RTSDA-USW converters are plug-and-play, support hot swapping and require no software.

Host Adapters Tested
AVA™-1505  
AHA®-1510  
AVA™-1515  
AHA®-1520/2  
AHA®-1530/2P  
AHA®-1540/2/F/P  
AHA®-2940/4/W  
AHA®-2940/4/U/UW

Rancho Technology, Inc.
10783 Bell Court
Cucamonga, CA 91730
Phone	(909) 987-3966
Fax	(909) 989-2365
E-mail	scsi@rancho.com
URL	http://www.rancho.com

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

MISCELLANEOUS	335

Winter, 1996

Rancho Technology, Inc.

	RTSDA-W16 Wide Converter Family

	RTSDA-W16 Converters connect single-ended SCSI devices to differential-ended SCSI devices.  Two SCSI converters can be used to extend 
	the SCSI cable length up to 200 feet.  Convert to differential-ended SCSI for better noise immunity.  These converters are 
	plug-and-play, support hot swapping and require no software.

Host Adapters Tested
AVA™-1505  
AHA®-1510  
AVA™-1515  
AHA®-1520/2  
AHA®-1530/2P  
AHA®-1540/2/F/P  
AHA®-2940/4/W  
AHA®-2940/4/U/UW

Rancho Technology, Inc.
10783 Bell Court
Cucamonga, CA 91730
Phone	(909) 987-3966
Fax	(909) 989-2365
E-mail	scsi@rancho.com
URL	http://www.rancho.com

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

MISCELLANEOUS	336

Winter, 1996

Rancho Technology, Inc.

	RTSDA-PW CD-ROM Peripheral Converter

	The RTSDA-PW Converter converts 8-bit single-ended CD-ROM and other peripherals, not available with a differential-ended interface, to 
	a wide differential-ended interface.  The RTSDA-PW is the same form-factor of the CD-ROM drive and mounts directly on the drive.  RTI 
	converters are plug-and-play, require no softwae and support hot swapping.

Host Adapters Tested
AVA™-1505  
AHA®-1510  
AVA™-1515  
AHA®-1520/2  
AHA®-1530/2P  
AHA®-1540/2/F/P

Rancho Technology, Inc.
10783 Bell Court
Cucamonga, CA 91730
Phone	(909) 987-3966
Fax	(909) 989-2365
E-mail	scsi@rancho.com
URL	http://www.rancho.com

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

MISCELLANEOUS	337

Winter, 1996

Rancho Technology, Inc.

	RTSDA-HP DAT Peripheral Converter

	The RTSDA-HP 8-Bit Converter connects SCSI DAT tape and other peripherals, not available with a differential-ended interface, to a 
	differential-ended interface.  The RTSDA-HP is the same form-factor as the 3 1/2 inch DAT drive and mounts directly on the drive.  RTI 
	converters are plug-and-play, support hot swapping and require no software.

Host Adapters Tested
AVA™-1505  
AHA®-1510  
AVA™-1515  
AHA®-1520/2  
AHA®-1530/2P  
AHA®-1540/2/F/P

Rancho Technology, Inc.
10783 Bell Court
Cucamonga, CA 91730
Phone	(909) 987-3966
Fax	(909) 989-2365
E-mail	scsi@rancho.com
URL	http://www.rancho.com

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

MISCELLANEOUS	338

Winter, 1996

Rancho Technology, Inc.

	RTREP-2 8 Bit Fast Repeater

	The RTREP-2 8-Bit Fast SCSI Repeater connects a single-ended device to a single-ended device.  The RTREP-2 extends the single-ended 
	SCSI bus by a factor of two.  The RTREP-2 is plug-and-play, supports hot swapping and requires no software.

Host Adapters Tested
AVA™-1505  
AHA®-1510  
AVA™-1515  
AHA®-1520/2  
AHA®-1530/2P  
AHA®-1540/2/F/P

Rancho Technology, Inc.
10783 Bell Court
Cucamonga, CA 91730
Phone	(909) 987-3966
Fax	(909) 989-2365
E-mail	scsi@rancho.com
URL	http://www.rancho.com

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

MISCELLANEOUS	339

Winter, 1996

Rancho Technology, Inc.

	RTSDA-S2 Fast 8-Bit Converter Family

	SCSI Converters connect a single-ended SCSI device to a differential-ended SCSI device.  Two SCSI converters can be used to extend the 
	SCSI cable length up to 200 feet.  Convert to differential-ended SCSI for better noise immunity.  These converters are plug-and-play, 
	support hot swapping and require no software.

Host Adapters Tested
AVA™-1505  
AHA®-1510  
AVA™-1515  
AHA®-1520/2  
AHA®-1530/2P  
AHA®-1540/2/F/P

Rancho Technology, Inc.
10783 Bell Court
Cucamonga, CA 91730
Phone	(909) 987-3966
Fax	(909) 989-2365
E-mail	scsi@rancho.com
URL	http://www.rancho.com

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

MISCELLANEOUS	340

Winter, 1996

Rancho Technology, Inc.

	RTSCSI-3

	The RTSCSI-3 Controller chip can be used in SCSI single to differential-ended converter and SCSI repeater designs.  The RTSCSI-3 
	operates with SASI, SCSI-1 through SCSI-3 and Fast20 (Ultra SCSI) designs.  These include 8- and 16-bit designs.  The RTSCSI-3 allows 
	the OEM to add a SCSI converter or repeater to their own form-factor.  The RTSCSI-3 is available in 84-pin PLCC and 100-pin QFP.

Host Adapters Tested
AVA™-1505  
AHA®-1510  
AVA™-1515  
AHA®-1520/2  
AHA®-1530/2P  
AHA®-1540/2/F/P

Rancho Technology, Inc.
10783 Bell Court
Cucamonga, CA 91730
Phone	(909) 987-3966
Fax	(909) 989-2365
E-mail	scsi@rancho.com
URL	http://www.rancho.com

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

MISCELLANEOUS	341

Winter, 1996

Rancho Technology, Inc.

	RTSDA-PM

	SCSI-2 Single to differential converter designed to be mounted on a panel via the 50-pin connector.

Host Adapters Tested
AVA™-1505  
AHA®-1510  
AHA®-1520/2  
AHA®-1530/2P  
AHA®-1540/2/F/P

Rancho Technology, Inc.
10783 Bell Court
Cucamonga, CA 91730
Phone	(909) 987-3966
E-mail	scsi@rancho.com
URL	http://www.rancho.com

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

MISCELLANEOUS	342

Winter, 1996

Suria Computer Corporation

	Suria Motherboard Family

	The Suria Mainboard family includes some of the most technologically advanced mainboards available today.  This family includes a 
	series of 486 mainboards as well as the Pentium mainboards that span the MHz spectrum from 25 DX4 100 and the 60 - 180 MHz 
	respectively.  They are available in the combination of VLB, PCI, EISA, and ISA bus connectors.  Certain mainboards also feature 
	on-board io's .  Our latest edition of Pentium mainboards are available with Plug & Play BIOS that include 'Bridge'  Technology used in
	 the latest Adaptec AHA-3940 Controllers.

Host Adapters Tested
AHA®-1540/2/F/P  
AHA®-2840/2VL  
AHA®-2940/4/W  
AHA®-3940/W

Suria Computer Corporation
2691 Richter Avenue, Suite 123
Irvine, CA 92714
Phone	714-851-0596
Fax	714-851-0598

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

MISCELLANEOUS	343

Winter, 1996

TAPEDISK Corporation

	TD RAW

	TD RAW is a DOS/Windows device driver with utilities designed for cross platform data exchange and data recovery applications.  It 
	enables a PC to read a tape, containing RAW data, created on a HP 3000, or other workstation, mini or mainframe computer.  The raw data
	 on the tape appears as files on a logical drive.  These files can be directly opened with any DOS/Windows/Windows 95 application that 
	can read the data format in the file.  An ASCII file, it can be opened by any PC database application.  Other advantages of using RAW 
	on a tape drive just like a disk include:  large file exchange, compressed file libraries (.zip files), and MultiMedia applications.  
	TD RAW can also read data from corrupted tapes.

Host Adapters Tested
APA™-358  
AHA®-1510  
AHA®-1520/2  
AHA®-1540/2/F/P  
AHA®-2740/2/4/T/W  
AHA®-2840/2VL  
AHA®-2940/4/W

TAPEDISK Corporation
P.O. Box 379, 85 Cove Lane
Oshkosh, WI 54902-0379
Phone	(800) 827-3372
Fax	(414) 233-8699
Toll free	(800) 827-3372

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters

MISCELLANEOUS	344

Winter, 1996

Windsor Technologies, Inc.

	PC-Technician

	PC-Technician™ is professional-level diagnostic software for Intel-based (8088->Pentium) and compatible PCs.  Written in assembly 
	language, it has its own proprietary operating system and boot-loader program.  PC-Technician will boot the target PC and directly test
	 its hardware without interference from its native operating system (DOS, UNIX, OS/2, Windows NT, etc.).  PC-Technician contains over 
	200 comprehensive tests and functions that can be run in single or continuous mode.  PC-Technician is used by service technicians to 
	troubleshoot a malfunctioning PC, certify a repaired PC, burn in a new PC, edit CMOS, or low-level format the fixed disk drive.

Host Adapters Tested
AHA®-1540/2/F/P  
AHA®-1740/2/4  
AHA®-2840/2VL  
AHA®-2940/4/W  
AHA®-2940W MAC

Windsor Technologies, Inc.
130 Alto Street
San Rafael, CA 94901
Phone	(415) 456-2200
Fax	(415) 456-2244
E-mail	pcdiags@windsortech.com
URL	http://www.windsortech.com

Adaptec Compatibility Directory: A Guide to Products Compatible with Adaptec Host Adapters