//--------------------------------------------------------------------
//
// INSTALL on-line Help Text File 
//
// Help Customization Guidelines:
//
// 0) Comment lines start with leading '//'.
// 1) Help Message Text starts with #MESSAGE statement
// 2) Never change the number after the #MESSAGE statement. That is
//    the search Message ID for the INSTALL program.
// 3) LINES statement defines how many (lines) x (characters) allowed.
//    Never exceed this limits when you type the text for the message.
// 4) TITLE statement defines the sub-Title of this message.
//    (allow to modify for your customization)
// 5) Text area starts and ends with a '$'.
//    (allow to modify for your customization)  
// 6) the INSTALL program is not going to format your 
//    text. It just show whatever text you typed here 
//    line by line. So you have to do the formatting for
//    better effect and please use SPACEs but not TABs.   
//    (you don't need to enter trailing SPACE lines. If there is space
//     left at the bottom of a HELP message, white space is the default.)
// 7) Anyway, give a try and see how it goes.
//
// 9) Format Overview (example)
//
//    #MESSAGE = 1                         // starts Help message 1
//    TITLE="Selcet CD-ROM Type"        // sub-title of this message
//    LINES=9x50                        // allowed text area: 
//                                      // 9 lines x 50 characters
//    $	                                // starts text area
//    TEXT LINEs
//    TEXT """"	                        // help text
//    " " "
//    $                                 // end of text area
//-----------------------------------------------------------------    

//
// INSTALL Help Text: Message by Message
//


#MESSAGE = 20
TITLE="Exit Program" 
LINES=1x60
$
  Are you sure you want to exit Program?
$

#MESSAGE = 21
TITLE="Sound Playing" 
LINES=3x60
$
   If you can not hear anything, please check
   I/O Port, IRQ, Play DMA and the volume of
   MASTER and WAVE settings.
$

#MESSAGE = 24
TITLE="REBOOT SYSTEM" 
LINES=5x49
$
Your CONFIG.SYS has been updated according to 
the new settings for your CD-ROM. You must REBOOT
your computer in order for the new settings to 
take effect. Select [OK] to REBOOT your computer.
Select [EXIT] to continue without reboot.
$

#MESSAGE = 25
TITLE="REBOOT SYSTEM"
LINES=4x46
$
Your BLASTER Environment Variable is updated
in your AUTOEXEC.BAT file. Some DOS games may
reference this variable for initialization
purposes. Do you wish to REBOOT your computer?
$

#MESSAGE = 26
TITLE="Error!"
LINES=2x48
$
Hardware Error Detected! Please reconfigure your
Sound Card's I/O Port, IRQ, or DMA settings.
$

#MESSAGE = 27
TITLE="Error!"
LINES=4x45
$
You have selected the same I/O Port setting
between your Audio, CD-ROM, or MPU-401
device. This will cause conflict on your
system. Please reselect a different I/O Port.
$

#MESSAGE = 28
TITLE="Error!"
LINES=4x47
$
You have selected the same IRQ settings between
your Audio, CD-ROM, Modem, or MPU-401 device.
This will cause conflict on your system. Please
reselect a different IRQ setting.
$

#MESSAGE = 29
TITLE="Error!"
LINES=3x47
$
You have selected the DMA settings, which
caused conflicts on your system. Please 
reselect a different DMA setting.
$

#MESSAGE = 30
TITLE="Warning!"
LINES=3x48
$
You have selected Windows Sound System using IRQ
5.  Some DOS games that support Windows Sound
System may not work with this option.  
$

#MESSAGE = 35
TITLE="AUDIO DEVICE NOT ENABLED"
LINES=6x48
$
There is no proper audio resources assigned for
your sound card. To play DOS games or to run 
Audio applications, resources must be assigned 
to the audio device. Please check the audio 
configuration to see if there is any conflict 
with other devices on your system.
$

#MESSAGE = 36
TITLE=""
LINES=5x20
$
Disabled
I/O:3f8 IRQ:4
I/O:2f8 IRQ:3
I/O:3e8 IRQ:4
I/O:2e8 IRQ:3
$

#MESSAGE = 37
TITLE=""
LINES=4x20
$
Disabled
I/O:168 IRQ:10
I/O:170 IRQ:15
I/O:1e8 IRQ:11
$

#MESSAGE = 38
TITLE="16-BIT DMA"
LINES=2x48
$
Some games use Sound Blaster commands may
not work for the current DMA settings. 
$

#MESSAGE = 41
TITLE="~C~ontinue"
LINES=1x5
$
41
$

#MESSAGE = 47
TITLE="~E~xit"
LINES=1x5
$
47
$
     
#MESSAGE = 49
TITLE="~O~K"
LINES=1x5
$
49
$

#MESSAGE = 55
TITLE="~C~ANCEL"
LINES=1x5
$
55
$

#MESSAGE = 56
TITLE="~N~ONE"
LINES=1x5
$
56
$

#MESSAGE = 59
TITLE="N/A"
LINES=1x5
$
59
$

#MESSAGE = 60
TITLE="~C~HANGE"
LINES=1x5
$
60
$

#MESSAGE = 73
TITLE="Disabled"
LINES=1x5
$
73
$

#MESSAGE = 74
TITLE="Enabled"
LINES=1x5
$
74
$

#MESSAGE = 76
TITLE="Please wait..."
LINES=1x5
$
76
$

#MESSAGE = 77
TITLE="CONFIGURATION"
LINES=5x25
$
~S~OUND TEST
~H~ELP
~D~EFAULT
~A~CCEPT
MI~X~ER
$

#MESSAGE = 78
TITLE=""
LINES=7x35
$
Sound Device Settings Selection
 Current Mode:
Sound Blaster Pro      IO Port:
Windows Sound System   IO Port:
     IRQ:
Play DMA:
$

#MESSAGE = 79
TITLE=""
LINES=6x25
$
Additional Options
Joystick:
MPU401 Interface
Interface:
  IO Port:
      IRQ:
$

#MESSAGE = 80
TITLE=""
LINES=5x25
$
Sound Card CD-ROM Interface
  Modem:
Record DMA:
$

#MESSAGE = 81
TITLE=""
LINES=5x25
$
Sound Blaster Pro
Windows Sound System
ON
OFF
$

#MESSAGE = 82
TITLE="EEPROM data corrupted...."
LINES=1x5
$
82
$

#MESSAGE = 83
TITLE="Error! Could not find sound card..."
LINES=1x5
$
83
$

#MESSAGE = 84
TITLE="Error! It is an invalid option."
LINES=3x60
$
The usage of SNDINIT:
SNDINIT [option]
[option] is /b to run SNDINIT in batch mode
$

#MESSAGE = 85
TITLE=""
LINES=3x50
$
Error! MIXER.CFG not found...
Error! VOLUME.CFG not found...
Error! SOUND16.CFG not found...
$


#MESSAGE = 92
TITLE="Sound Test Failed. Please reconfigure your"
LINES=1x5
$
92
$

#MESSAGE = 93
TITLE="Sound Blaster options and select "
LINES=1x5
$
93
$

#MESSAGE = 94
TITLE="Windows Sound System options and select "
LINES=1x5
$
94
$

#MESSAGE = 95
TITLE="Error! Not enough memory to play wave file."
LINES=2x50
$
Error! Sound Test has detected a wave file 
format which it cannot play.
$

#MESSAGE = 96
TITLE=""
LINES=2x50
$
Error! The wave file for Sound Test could not
be found. Please verify its location.
$

#MESSAGE = 102
TITLE="Error! Not enough memory to run program."
LINES=7x65
$
Warning! This program has detected that you do not
have the recommended 490 KBytes of conventional
memory available to run this program. Please remove
any memory resident programs that reside in your
system and run this program again. Consult your
operating system manual for details on increasing
the conventional memory in your system.
$

#MESSAGE = 103
TITLE=""
LINES=4x65
$
Warning! This program cannot be executed under a
Windows MS-DOS Prompt Session. Please type EXIT
to return to Windows and quit your Windows session
before running this program again.
$

#MESSAGE = 104
TITLE="Online Help and Information"
LINES=4x45
$
   [TAB]     to move to option
   [Enter]   to execute to option
   [F3]      to exit the program
   [ALT+Key] to activate a button
$
   
#MESSAGE = 107
TITLE=""
LINES=11x35
$
Master
Mute:
On
Off
Recording:
 Source:
   Gain:
Additional Control:
Mono Gain
~D~ONE
~S~OUND TEST
$

#MESSAGE = 108
TITLE=""
LINES=3x45
$
Could not find list file for DISK 1.
Installer Could not find DISK 1.
Installer error: Out of memory.
$

#MESSAGE = 109
TITLE=""
LINES=4x60
$
Sound Card Initialization Error!
Your SET %s environment variable is not defined.
Please verify that the above variable is defined
in your AUTOEXEC.BAT file.
$

#MESSAGE = 111
TITLE=""
LINES=1x50
$
Error! Not enough memory to run program.
$

#MESSAGE = 112
TITLE="     Initializing sound card in "
LINES=2x50
$
Sound Blaster Pro Mode...
Windows Sound System Mode...
$

#MESSAGE = 113
TITLE=""
LINES=5x50
$
                Port Address:
                 IRQ Channel:
                 DMA Channel:
        DMA Playback Channel:
         DMA Capture Channel:
$

#MESSAGE = 114
TITLE=""
LINES=3x50
$
           MPU-401 Interface:
        MPU-401 Port Address:
         MPU-401 IRQ channel:
$

#MESSAGE = 115
TITLE=""
LINES=6x50
$
            CD-ROM Interface:
         CD-ROM Port Address:
          CD-ROM IRQ Channel:
             MODEM Interface:
          MODEM Port Address:
           MODEM IRQ Channel:
$

#MESSAGE = 116
TITLE=""
LINES=2x50
$
            Game Port Access:
         Input Source Select:
$

#MESSAGE = 129
TITLE=""
LINES=5x15
$
CD
MIDI
WAVE
LINE
MIC
$
