README - FM Synthesis OPL3 Midi Device Driver Installation
-----------------------------------------------------------
This readme file contains information on how to install the FM Synthesis
OPL3 Midi Device driver.

System Requirement
------------------
Before you install FM Synthesis OPL3 Midi, make sure that
you have installed OS/2 WARP Version 3.00 Revision 8.162. Enter "VER /R" from
an OS/2 command prompt to verify.


FM Synthesis OPL3 Midi for OS/2 Installation Procedure
-------------------------------------------------------------
To install device support, insert the FM Synthesis OPL3 Midi
for OS/2 diskette in drive A:. Start the multimedia installation program "A:MINSTALL",
located on the diskette. Select the FM Synthesis OPL3 Midi" icon.

The Multimedia installation program adds the following statements
to your CONFIG.SYS file.  These statements are
displayed as follows:

   DEVICE=c:\mmos2\TIMER0.SYS
   DEVICE=c:\mmos2\opl3.sys /P:388 /N:OPL31$


