-----------------------------------------------------------------------------
  Information for installing the DS-XG WDM Audio Miniport Driver on 
                Windows98SE/WindowsME/Windows2000
                      (Version5.12.01.22xx) 
        Copyright (c) 1999-2000 YAMAHA Corporation. All Rights Reserved.
-----------------------------------------------------------------------------

Before you install the DS-XG WDM driver, please read the descriptions
hereafter to select the necessary inf file for your system.    

To better support different devices and CODECs, the DS-XG WDM driver is released 
with different customized inf files. You will need to locate the proper inf 
file for your system depending on the device and CODEC you are using.

The information below helps you to determine the inf file for your system.
Place or copy the needed inf file to the same directory of the driver files 
before you start installation. 

[1] Filename:
    The INF files are created based on the following naming convention.
    2 identifiers of Device and CODEC are included in the filename to 
    categorize functionalities for different device and CODECs. 
 	
		NLDS1#$ .INF
			#  ... Device Identifier
				E : YMF754(DS-1E)
				S : YMF744B(DS-1S)
			$  ... CODEC Identifier
				0 : AKM4543
				1 : STAC9708
				2 : STAC9721
				3 : STAC9744
				4 : AKM4544
				5 : AKM4543 for 4-ch Audio
				6 : WM9704Q
		[Example]
			NLDS1S0  .INF .... The DS-1S inf file customized for AKM4543
			
[2] File Description

    		NLDS1S0 .INF ... YMF744B(DS-1S) for Audio Docking
					CODEC AKM4543 Setting
					
		NLDS1E0 .INF ... YMF754(DS-1E) for Audio Docking 
					CODEC AKM4543 Setting
					
		NLDS1S1 .INF ... YMF744B(DS-1S) for 4-ch Audio 
					CODEC STAC9708 Setting
					
		NLDS1E1 .INF ... YMF754(DS-1E) for 4-ch Audio
					CODEC STAC9708 Setting
					
		NLDS1S4 .INF ... YMF744B(DS-1S) for Audio Docking
					CODEC AKM4544 Setting
					
		NLDS1E4 .INF ... YMF754(DS-1E) for Audio Docking 
					CODEC AKM4544 Setting
					
		NLDS1S5 .INF ... YMF744B(DS-1S) for 4-ch Audio
					CODEC AKM4543 Setting
					
		NLDS1E5 .INF ... YMF754(DS-1E) for 4-ch Audio 
					CODEC AKM4543 Setting
					
		NLDS1S6 .INF ... YMF744B(DS-1S) for 4-ch Audio
					CODEC WM9704Q Setting
					
		NLDS1E6 .INF ... YMF754(DS-1E) for 4-ch Audio 
					CODEC WM9704Q Setting
					
		