## The ADSL LED is not lit.

### Solution 1:

Verify that the ADSL2+ Ethernet/USB Router is powered on.

Be sure the cable is plugged in to the ADSL2+ Ethernet/USB Router and the wall phone jack.

### Solution 2:

Verify that the proper cable type is used and that its length does not exceed the specified limits.

### Solution 3:

Be sure that the network interface on the attached device is configured for the proper communication speed and duplex mode.

### Solution 4:

Check the adapter on the attached device and cable connections for possible defects. Replace any defective adapter or cable if necessary.