Digi Connectware Manager Installation

Enter Digi Connectware Manager port numbers and IP address to bind to.

Bind to IP Address - Enter the IP Address to bind to on a multi-homed host or select 'all' to bind to all IP addresses available on this server.

MDH Port Number - This is the port number used for Message-over-Device-Initiated HTTP connection used for device communication when there are firewalls involved. This port number is set to 80 by default since most firewalls allow port 80 traffic to go through. Warnning: Setting this port to anything other than 80 may cause devices behind some firewalls not be able to communicate with the server unless another web server is configured to redirect the port 80 requests to this server.

Remote Application Access Port Number - This is the port number the server listens to for remote application requests. The default port number is 9443.

Management Console Access Port Number - This is the port number specified in the URL entered from a browser to access the Management Console. The default port number is 8443.

Use SSL - Whether to use Secure Socket Layer for access. The default is to use SSL for both remote application and Management Console access.

Click Next.