<< Previous | Next >>

> AND HL,DE Bitwise AND Rabbit 2000/3000/4000 Instruction

> Opcode | Instruction | Clocks | Operation
> DC | AND HL,DE | 2 | HL = HL & DE

> Flags | ALTD | IOI/IOE
> S | Z | L/V | C | F | R | SP | S | D
> · | · | L | 0 | · | · |  |  |

> #### Description

> Performs a bitwise AND operation between the word in HL and the word in DE. The result is stored in HL.

<< Previous | Next >>