<< Previous | Next >>

> PUSH IP
> PUSH IX
> PUSH IY Stack Operation Rabbit 2000/3000/4000 Instruction

> Opcode | Instruction | Clocks | Operation
> ED 76 | PUSH IP | 9 (2,2,2,3) | (SP - 1) = IP SP = SP - 1
> DD E5 | PUSH IX | 12 (2,2,2,3,3) | (SP - 1) = IXhigh (SP - 2) = IXlow SP = SP - 2
> FD E5 | PUSH IY | 12 (2,2,2,3,3) | (SP - 1) = IYhigh (SP - 2) = IYlow SP = SP - 2

> Flags | ALTD | IOI/IOE
> S | Z | L/V | C | F | R | SP | S | D
> - | - | - | - |  |  |  |  |

> #### Description

> Pushes IP IX, or IY on the stack.

<< Previous | Next >>