RabbitLink User's Manual

> ## Appendix F. Serial Console Commands

> Appendix F lists all the serial console commands used to control the RabbitLink.

> Table F-1. Configuration Commands
> Task | Command | Parameters
> set gateway | set gateway x.x.x.x | x.x.x.x is the gateway IP address
> set name | set hostname <name> | <name> is a unique name (up to 40 characters) that you assign to the RabbitLink
> set IP address | set ip x.x.x.x | x.x.x.x is the IP address
> set sender's E-mail address | set mail from <username@domain.ca> | <username@domain.ca> is the RabbitLink's E-mail address
> set mail server IP address | set mail server x.x.x.x | x.x.x.x is the IP address of the mail server
> set netmask | set netmask x.x.x.x | x.x.x.x is the netmask
> set password | set passphrase | should be as long as possible (up to 255 characters)
> set port | set port x | x is the TCP port number, the default TCP port number is 4244
> NOTE | Ask your network administrator for assistance with these values.

> Table F-2. Other Commands
> Command | Description
> createv | <varname> <vartype> <format> <value> [strlen] | variable name type of the variable (int8, int16, int32, float32, or string) <format> is the printf-style format specifier (such as %d) for outputting the variable <value> is the value to assign to the variable. only used if the variable is of type string to give the maximum length of the string
> delete | <filename> | deletes <filename>
> echo | <on> | turn character echoing on
> <off> | turn character echoing off
> get | <filename> | use to view <filename>
> getv | <varname> | gets the value of the variable called <varname>
> help |  | online help
> <filename> | online help for <filename> specified
> list | files | show all files stored in flash
> variables | show all variables
> put | <filename> | use to put <filename> on RabbitLink
> putv | <varname> <value> | assigns the given <value> to the given variable <varname>
> reset |  | reset values (except password) to factory defaults
> <filename> | reset <filename>to factory defaults
> variables | deletes all variables
> show |  | get a list of all assignable variables (except the password) and their settings
> <filename>

Z-World http://www.zworld.com Voice: (530) 757-3737 FAX: (530) 753-5141 sales@zworld.com | Rabbit Semiconductor http://www.rabbitsemiconductor.com Voice: (530) 757-8400 FAX: (530) 757-8402 sales@rabbitsemiconductor.com