# Digi.Drivers.I2CiMX51 Member List

This is the complete list of members for Digi.Drivers.I2CiMX51, including all inherited members.

Addr | Digi.Drivers.I2CiMX51 |
ClockRate | Digi.Drivers.I2CiMX51 |
DisableSlave() | Digi.Drivers.I2CiMX51 |
EnableSlave() | Digi.Drivers.I2CiMX51 |
Frequency | Digi.Drivers.I2CiMX51 |
GetSlaveText(ref byte[] text) | Digi.Drivers.I2CiMX51 |
I2C() | Digi.Drivers.I2C |
I2CiMX51(I2CPort I2Cnumber) | Digi.Drivers.I2CiMX51 |
I2CPort enum name | Digi.Drivers.I2CiMX51 |
I2CResult enum name | Digi.Drivers.I2CiMX51 |
IsMaster(ref bool ismaster) | Digi.Drivers.I2CiMX51 |
IsSlave(ref bool isslave) | Digi.Drivers.I2CiMX51 |
Length | Digi.Drivers.I2CiMX51 |
Read(ref byte[] Buffer, int count) | Digi.Drivers.I2CiMX51 | `[virtual]`
Reset() | Digi.Drivers.I2CiMX51 |
Result | Digi.Drivers.I2CiMX51 |
RW | Digi.Drivers.I2CiMX51 |
RWOperation enum name | Digi.Drivers.I2CiMX51 |
SelfAddress | Digi.Drivers.I2CiMX51 |
SetMasterMode() | Digi.Drivers.I2CiMX51 |
SetSlaveMode() | Digi.Drivers.I2CiMX51 |
SetSlaveText(byte[] text) | Digi.Drivers.I2CiMX51 |
SlaveSize | Digi.Drivers.I2CiMX51 |
Write(ref byte[] Buffer, int count) | Digi.Drivers.I2CiMX51 | `[virtual]`