Show Contents

# Step 1: Requirements

To start working with the ConnectCore 6UL and Yocto, you need the following items:

- A ConnectCore 6UL Development Kit

> Verify that your kit contains the following components:

> Qty. | Part
> --- | ---
> 1 | ConnectCore 6UL SBC Pro
> 1 | 5V/3A power supply with EU, UK, AUST adapters
> 1 | USB to TTL 3.3 V cable
> 1 | U.FL female to RPSMA female cable adapter
> 1 | MMCX to RPSMA female cable adapter
> 1 | Desktop antenna, Wi-Fi 2.4/5GHz
> 1 | PCIe mounting kit

- A 64-bit Linux machine for application development and system customization, with at least:
  - 4 GB of RAM
  - 4 CPU cores
  - 100 GB of free disk space

Note For successful Digi Embedded Yocto projects, we recommend you use a Yocto Project-supported Ubuntu distribution. You can find Yocto Project-supported distributions in the Yocto Project system requirements at http://www.yoctoproject.org/docs/2.2/ref-manual/ref-manual.html#intro-requirements.

- Additional components not included in the kit:
  - FAT-formatted microSD card
  - Ethernet cable (optional)

© 2018 Digi International Inc. All rights reserved.
Step 1: Requirements updated on 22 January 2018 02:43:37 PM