Show Contents

# 6. Program the encrypted artifacts

The signed and encrypted artifacts can be flashed using standard procedures for programming a boot partition. However, in order to use any encrypted artifact, the following additional requirements must be met:

- You must use a closed device.
- The device must contain a U-Boot image encrypted with the same key in the uboot partition.

To program the linux partition containing all the encrypted artifacts:

    => update linux tftp core-image-base.boot.ubifs

To program the recovery partition containing all the encrypted artifacts:

    => update recovery tftp core-image-base.recovery.ubifs

The device now boots into a trusted Linux kernel.

© 2018 Digi International Inc. All rights reserved.
6. Program the encrypted artifacts updated on 22 January 2018 02:43:38 PM