Show Contents

# Create a makefile project

1. Select File > New > Project to open the New Project wizard.
2. Select the type of project to create under the C/C++ category. For example, choose C Project.
3. Click Next. The C Project wizard opens.

1. Type a name for your project in the Project name text box.
2. You can change the location of the project by deselecting the Use default location option.
3. From the Project type list, expand the Makefile project and select Empty Project.
4. Select DEY Cross GCC from the Toolchains list.
5. Click Next. The Select Configurations page is displayed, where you can choose the configurations to create or perform advanced configuration.
6. Click Next to display the Configure Digi Embedded Yocto platform and toolchain page. This page shows the available platforms and toolchains for the selected platform depending on the directory configured in the DEY Toolchains preference page. See Configure installed DEY toolchains for more information.

> By default, the preference values are selected.

1. Select the platform for your project in the Platform list.
2. Select the toolchain to use from the Available toolchains list.
3. Click Finish. A new project is created with the configured settings. It is listed in the Project Explorer view.

> Note If the C++ perspective is not the current one, a message appears asking if you would like to open the C/C++ perspective.

> You must provide the source code and the makefile(s) to build the project.

Note For more information, see the "C/C++ Development User Guide" at http://help.eclipse.org/index.jsp.

© 2018 Digi International Inc. All rights reserved.
Create a makefile project updated on 22 January 2018 02:43:38 PM