Show Contents

# Digi embedded APIX

Digi APIX is a C library that enables you to easily access and manage Digi ConnectCore platform interfaces. You can use Digi APIX to define aliases for your hardware interfaces. These aliases map a human-readable name with the hardware identifier of your system. For example, you can map GPIO 505 with the alias "USER_BUTTON". Because the alias is defined in a configuration file, you don't need to change your application code if you modify the hardware definition. So your application code is still valid even if the hardware changes. Once you change the value of the alias in the configuration file, the alias "USER_BUTTON" points to the new kernel number value. For information on how to work with this library, see Set up your project for Digi APIX.

Each API includes a section explaining how to establish aliases at runtime. See Hardware interface aliasing for information on adding the configuration file to your image.

Digi Embedded Yocto provides examples of using this API to connect and work with your device interfaces. Use the Digi Embedded Yocto plugin to import the examples to Eclipse. For details, see Create a new DEY sample project.

The Digi APIX includes the following features:

© 2018 Digi International Inc. All rights reserved.
Digi embedded APIX updated on 14 February 2018 12:01:53 AM