ID: 17
Name: del-4_2-hf2
Version: 1.0
Dependences: 10
Description: The present HotFix Pack contains important fixes and updates to Digi Embedded Linux 4.2 distribution.@@@@@@Contents-@@@- Added platform device for I2C interface on cme9210js-@@@  I2C platform device information was missing from machine@@@  code of cme9210 platform, preventing the interface from@@@  being probed.@@@- Reduce netdev_max_backlog on cme9210js -@@@  Due to the small quantity of memory in the cme9210js, a bigger@@@  netdev_max_backlog can trigger the out of memory killer under @@@  some circumstances (like being ping flooded)@@@- Fix double to stream conversion in libstdc++ library@@@- Fix Ethernet driver (cme9210js presented OOM killer when @@@  ping flooded)
Minidescription: HotFix Pack 2 for Digi Embedded Linux 4.2.
platformversion: 4.2
Revision: -1
platform: el
Relevance: RECOMMENDED
Filename: del-4_2-hf2_17.dipk
Date: 23/02/2009
Type: fix
Target: embedded
Size: 13875kb
Installedsize: 11609kb
